{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["ESSAI"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ESSAI","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
["N° Fiche FVC","Site","Code1","Code2","Code3","…","….","….","Date début de la session","Date fin de la session"]
["FVC12O18744"]
["FVC12O18744"]
["FVC12O18744"]
["FVC12O18744"]
["FVC12O18744"]
["FVC12O18744"]
["FVC12O18744"]
["FVC12O18745"]
["FVC12O18745"]
["FVC12O18745"]
["FVC12O18745"]
["FVC12O18745"]
["FVC12O18745"]
["FVC12O18745"]
["FVC12O18746"]
["FVC12O18746"]
["FVC12O18746"]
["FVC12O18746"]
["FVC12O18746"]
["FVC12O18746"]
["FVC12O18746"]
["FVC12O18747"]
["FVC12O18747"]
["FVC12O18747"]
["FVC12O18747"]
["FVC12O18747"]
["FVC12O18747"]
["FVC12O18747"]
["FVC12O18748"]
["FVC12O18748"]
["FVC12O18748"]
["FVC12O18748"]
["FVC12O18748"]
["FVC12O18748"]
["FVC12O18748"]
["FVC12O18749"]
["FVC12O18749"]
["FVC12O18749"]
["FVC12O18749"]
["FVC12O18749"]
["FVC12O18749"]
["FVC12O18749"]
["FVC12O18750"]
["FVC12O18750"]
["FVC12O18750"]
["FVC12O18750"]
["FVC12O18750"]
["FVC12O18750"]
["FVC12O18750"]
["FVC12O18751"]
["FVC12O18751","Saint Ouen","US/SOUD","VSR27000","Perf. cyclique - Rem","NVS0000058","Perf. cyclique - Remise en état des rails / soudage à l'arc","Ouverte","2012-10-15","2012-10-19","Ouverte","La formation respecte les prescriptions du CCFO"]
["FVC12O18751","Saint Ouen","US/SOUD","VSR27000","Perf. cyclique - Rem","NVS0000058","Perf. cyclique - Remise en état des rails / soudage à l'arc","Ouverte","2012-10-15","2012-10-19","Ouverte","Non annulée ou décalée après J-15"]
["FVC12O18751","Saint Ouen","US/SOUD","VSR27000","Perf. cyclique - Rem","NVS0000058","Perf. cyclique - Remise en état des rails / soudage à l'arc","Ouverte","2012-10-15","2012-10-19","Ouverte","Planning fiabilisé proposé aux Ets à M-2"]
["FVC12O18751","Saint Ouen","US/SOUD","VSR27000","Perf. cyclique - Rem","NVS0000058","Perf. cyclique - Remise en état des rails / soudage à l'arc","Ouverte","2012-10-15","2012-10-19","Ouverte","Résultats des éval. envoyées aux Ets sous 15 jours"]
["FVC12O18751","Saint Ouen","US/SOUD","VSR27000","Perf. cyclique - Rem","NVS0000058","Perf. cyclique - Remise en état des rails / soudage à l'arc","Ouverte","2012-10-15","2012-10-19","Ouverte","Taux de réussite éval. 2 ≥ 80%"]
["FVC12O18751","Saint Ouen","US/SOUD","VSR27000","Perf. cyclique - Rem","NVS0000058","Perf. cyclique - Remise en état des rails / soudage à l'arc","Ouverte","2012-10-15","2012-10-19","Ouverte","Taux de satisfaction éval. 1 ≥ 90%"]