{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["Design","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":64,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Design","index":0,"n_rows":21,"n_cols":17,"rows_kept":21,"cut":false,"hidden":false,"merged":[[14,1,14,3],[0,0,3,1],[6,1,6,9],[7,1,7,3],[8,1,8,3],[4,0,4,9],[19,1,19,3],[20,1,20,3],[16,1,16,9],[17,1,17,3],[9,1,9,3],[10,1,10,3],[18,1,18,3],[12,1,12,9],[13,1,13,3]],"flags":["formulas_cached_only"]}
[{"$nulls":15},-0.18,0.18]
[{"$nulls":15},0,0]
[{"$nulls":16},0]
[{"$nulls":16},0]
[]
[]
[null,"FLUID CHARACTERISTICS"]
[null,"Liquid mass flow",null,null,"WL",null,110000]
[null,"Gas mass flow",null,null,"WG",null,3500]
[null,"Liquid density",null,null,"rL",null,845]
[null,"gas density",null,null,"rG",null,4.5]
[]
[]
[null,"coefficient K",null,null,"K",null,2.2]
[null,"Diameter ",null,null,"D",null,2.5]
[]
[]
[null,"Critical velocity",null,null,"vc",null,null,0,0,0]
[null,"superficial gas velocity",null,null,"vs",null,null,0,0,0]
[null,"Vapor area",null,null,"Av",null,null,0,0,0]
[null,"Height of vapor",null,null,"hv",null,null,0,0,0]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}