{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["sheet1","Liste"],"not_rendered":{"macros":1,"external_links":7,"defined_names":133},"read":"whole","date_system":"1900"}

{"sheet":"sheet1","index":0,"n_rows":500,"n_cols":24,"rows_kept":500}
["Material#","Material Description","Maxime","Remplacement","UoM","Lab office","Mfr Code","Manufac. Name","Manufac. P/N","Basic Data Text","PO Text","QC Inspection Text","Internal Comment","Cross Plant Material Status","01","Follow-Up Material#","Old Material#","Material Class","Material Class Description","MRP Type","Safety Stock","Reorder Point / Minimum Stock","Maximum Stock Level","MovAvgPrice"]
[1000010,"(BLCK)KIT:CBL CLMP FTG,F/6MM HX HD",null,null,"EA","COM","4001096","PolyOil Ltd","M8-CFK_31974","KIT:\nTYPE: CABLE CLAMP FITTING\nAPPLICATION: FOR 6MM HEX HEAD","Cable Clamp Fitting Kit\n\n","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","06","","","FOLLOW UP 1032846","KIT:\nTYPE: CABLE CLAMP FITTING\nAPPLICATION: FOR 6MM HEX HEAD","ZGMD_KIT_NM","ND",0,0,0,{"v":3374.27,"d":"3,374.27"}]
[1000012,"COND:20\",166.56 PPF,XLC-SE,MU/L:6.19\",B>","COND","CONDUCTOR","EA","DRL","4000006","NOV PRIDECO SINGAPORE","","CONDUCTOR:\nOUTSIDE DIAMETER: 20\"\nWEIGHT: 166.56 PPF\nEND CONNECTIONS: XLC-SE, MU/L:6.19\"\nEND CONNECTION TYPE: BOX X PIN\nGRADE: X65\nLENGTH: R3\nSPECIFICATION: API 5L, PSL2","FITTED WITH PDL SUBS (METAL THREAD PROTECTORS)\nSTORAGE COMPOUND JET LUBE KORR GUARD OR SIMILAR AS PER API 5L\n","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","CONDUCTOR:\nOUTSIDE DIAMETER: 20\"\nWEIGHT: 166.56 PPF\nEND CONNECTIONS: XLC-SE, MU/L:6.19\"\nEND CONNECTION TYPE: BOX X PIN\nGRADE: X65\nLENGTH: R3\nSPECIFICATION: API 5L, PSL2","ZGMD_CONDUC_NM","PD",0,0,0,{"v":7033.33,"d":"7,033.33"}]
[1000013,"COND:20\",CTD,166.56 PPF,XLC-SE,MU/L:6.1>","COND","CONDUCTOR","EA","DRL","4000006","NOV PRIDECO SINGAPORE","","CONDUCTOR:\nOUTSIDE DIAMETER: 20\", COATED\nWEIGHT: 166.56 PPF\nEND CONNECTIONS: XLC-SE, MU/L:6.19\"\nGRADE: X-65\nLENGTH: R3\nWALL THICKNESS: 0.812\"","FITTED WITH PDL SUBS (METAL THREAD PROTECTORS)\nSTORAGE COMPOUND JET LUBE KORR GUARD OR SIMILAR AS PER API 5","","","","","","","CONDUCTOR:\nOUTSIDE DIAMETER: 20\", COATED\nWEIGHT: 166.56 PPF\nEND CONNECTIONS: XLC-SE, MU/L:6.19\"\nGRADE: X-65\nLENGTH: R3\nWALL THICKNESS: 0.812\"","ZGMD_CONDUC_NM","PD",0,0,0,{"v":9907.62,"d":"9,907.62"}]
[1000014,"(BLCK)UACU ACQ UNIT W/ 10 PDGIC TESTED",null,null,"EA","COM","4000007","HALLIBURTON USA SINGAPORE","602523","","ELECTRICAL BOX\nUACA\nRACK MOUNT,10CHANNELS\nMANUFACTURER#602523","","","06","","100084144","","-","-","PD",0,0,0,{"v":32225,"d":"32,225.00"}]
[1000015,"SSD,4.5\" DURASLEEVE,13CR L80,SLAPX","SSD","SLIDING SLEEVE","EA","COM","4000007","HALLIBURTON USA SINGAPORE","102686287","SSD: SLIDING SLEEVE\nTYPE: DURASLEEVE\nSIZE: 4.5\"\nGRADE: L80 13CR\nCONNECTION: SL APEX","","","12 June 2017 PO Long Text as per below:\nSSD: SLIDING SLEEVE\nTYPE: DURASLEEVE\nSIZE: 4.5\"\nGRADE: L80 13CR\nCONNECTION: SL APEX","","","","","-","-","PD",0,0,0,{"v":9464,"d":"9,464.00"}]
[1000016,"SSD,3.5\" DURASLEEVE,13CR L80,SLAPX","SSD","SLIDING SLEEVE","EA","COM","4000007","HALLIBURTON USA SINGAPORE","102689203","SSD: SLIDING SLEEVE\nTYPE: DURASLEEVE\nSIZE: 3.5'\nGRADE: L80 13CR\nCONNECTION: SL APEX\n","","","12 June 2017 PO Long Text as per below:\nSSD: SLIDING SLEEVE\nTYPE: DURASLEEVE\nSIZE: 3.5'\nGRADE: L80 13CR\nCONNECTION: SL APEX\n","","","","","-","-","PD",0,0,0,{"v":7986,"d":"7,986.00"}]
[1000017,"PKR:5.5\",15.5#,SLAPX,L80 13CR,CHEM INJ >",null,null,"EA","COM","4000007","HALLIBURTON USA SINGAPORE","102687589","PACKER:\nCASING/TUBING SIZE: 5.5\"\nTHREAD SIZE/WEIGHT/CONNECTION: 15.5#, SL APEX\nGRADE: L80 13CR\nTYPE: CHEMICAL INJECTION FEATURE","AC1 ANVIL","","","","","","","PACKER:\nCASING/TUBING SIZE: 5.5\"\nTHREAD SIZE/WEIGHT/CONNECTION: 15.5#, SL APEX\nGRADE: L80 13CR\nTYPE: CHEMICAL INJECTION FEATURE","ZGMD_PCKR_NM","PD",0,0,0,{"v":45741,"d":"45,741.00"}]
[1000021,"BALL:DROPPING,PDC DRILLABLE,1.5\",AL",null,null,"EA","DRL","4000008","WEATHERFORD USA","280738","BALL:\nTYPE: DROPPING, PDC DRILLABLE\nDIAMETER: 1.5\"\nMATERIAL: ALUMINIUM","DROPPING BALL for Off Bottom Cemented 7\" X 9-5/8\" Liner Hanger\n\n","","","","","",null,"BALL:\nTYPE: DROPPING, PDC DRILLABLE\nDIAMETER: 1.5\"\nMATERIAL: ALUMINIUM","ZGMD_BALL_NM","PD",0,0,0,64.05]
[1000022,"LNR:PDC DRILLABLE,1.75\",AL","LNR","LINER","EA","DRL","4001273","Al-Shaheen Weatherford","141815","LINER:\nTYPE: PDC DRILLABLE\nSIZE: 1.75\"\nMATERIAL: ALUMINIUM","DROPPING BALL for Off Bottom Cemented\n7\"X9 5/8\" Liner Hanger","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","LINER:\nTYPE: PDC DRILLABLE\nSIZE: 1.75\"\nMATERIAL: ALUMINIUM","ZGMD_LNR_NM","PD",0,0,0,97.67]
[1000023,"X-OVER,7\",23#,HYDRIL 521 BOX,SLHT PIN",null,null,"EA","DRL","4000008","WEATHERFORD USA","284156-NPN","","X-OVER: Cross Over Sub\nLenght: 7\"\nWeight: 23#\nConnection : HYDRIL 521 BOX,SLHT PIN\nPart#284156-NPN\n","","","","","","","-","-","PD",0,0,0,{"v":2194.5,"d":"2,194.50"}]
[1000031,"GAUGE:MNDRL;4-1/2\",12.6#,4-1/2\" 12.6 LB>",null,null,"EA","COM","4000009","SCHLUMBERGER USA","100940583","GAUGE:MANDREL;\nSIZE: 4-1/2\"\nWEIGHT: 12.6#\nTHREAD UP: 4-1/2\" 12.6 LB/FT SL-APEX BOX\nTHREAD DOWN: 4-1/2\" 12.6 LB/FT SL-APEX PIN\nPRESSURE RATING: 10600PSI MIN WORKING\nTEMPERATURE RATING: 300 DEGF\nINSIDE DIAMETER: 3.864\" MIN\nDRIFT: 3.833\"\nMATERIAL: 13% CR 80 ICS118 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\n","Permanent Gauge Mandrel - Internal Reading\nMax OD (In.), combined with 5 x Encapsulated control lines.: 6.515\nMandrel: Long tapers longitudinal slot for 5 chemical Injection/control\nlines (11mm x 11mm)\nMetallurgy: 13% Cr 80 ics118 - 22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb): 13,200\nTensile Strength thru Body (Ibs): 295,500","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","GAUGE:MANDREL;\nSIZE: 4-1/2\"\nWEIGHT: 12.6#\nTHREAD UP: 4-1/2\" 12.6 LB/FT SL-APEX BOX\nTHREAD DOWN: 4-1/2\" 12.6 LB/FT SL-APEX PIN\nPRESSURE RATING: 10600PSI MIN WORKING\nTEMPERATURE RATING: 300 DEGF\nINSIDE DIAMETER: 3.864\" MIN\nDRIFT: 3.833\"\nMATERIAL: 13% CR 80 ICS118 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\n","ZGMD_GGE_MANDREL","PD",0,0,0,{"v":14446.7,"d":"14,446.70"}]
[1000032,"GAUGE,DHPTG, XDPG-CA DIGITAL,13CR",null,null,"EA","COM","4000009","SCHLUMBERGER USA","101472072","","PERMANENT PT GAUGE:\nXDPG-CA (X-SERIES DIGITAL PERMANENT GAUGE WITH SEALTITE)\nTYPE: XDPG-CA ( X Series, Digital Permanent Gauge\nGrade: 13%Cr","","18 May 2017: Comment NLH\nWhen PO#4500000186 received PO long text to be updated as per below to\nmatch with contract:\nPermanent Gauge - XPDG-CA (X-Series Digital Permanent Gauge with\nSealtite\nReading 1 dataset / sec.\nCable Encapsulated\nSensor\npressure stability (drift) for the\nXDPG series gauge is <(><<)> 3\nPsi/Year over full scale\nMinimum accuracy pressure accuracy for the\nXDPG series gauge is <(><<)> 3 psi\nPressure resolution\npressure resolution for the\nXDPG series gauge Is 0.02 psi\n@ 5 seconds sampling\nTemperature Accuracy\ntemperature accuracy for the\nXDPG series gauge Is 0.5 (+/-)\nden C\nTemperature Resolution\ntemperature resolution for the\nNDPG series gauge is 0.004\ndeg C @ 5 second sampling","","","","","-","-","PD",0,0,0,{"v":13843.85,"d":"13,843.85"}]
[1000033,"GAUGE:MNDRL;5-1/2\",15.5#,5-1/2\" 15.5 LB>",null,null,"EA","COM","4000009","SCHLUMBERGER USA","102819034","GAUGE:MANDREL;\nSIZE: 5-1/2\"\nWEIGHT: 15.5#\nTHREAD UP: 5-1/2\" 15.5 LB/FT SL-APEX BOX\nTHREAD DOWN: 5-1/2\" 15.5 LB/FT SL-APEX PIN\nPRESSURE RATING: 6900PSI MIN\nTEMPERATURE RATING: 300 DEGF\nINSIDE DIAMETER: 4.856\"\nDRIFT: 4.825\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\n\n","Permanent Gauge Mandrel – Internal Reading\nMax OD (in.), combined with 5 x Encapsulated control lines.: 7.360\nMandrel: Long tapers, longitudinal slot for 5 chemical injection/control\nlines (11mm x 11mm)\nMetallurgy: 13% Cr 80 ksi 18 - 22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb): 8,800\nTensile Strength thru Body (Ibs): 428,800","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","GAUGE:MANDREL;\nSIZE: 5-1/2\"\nWEIGHT: 15.5#\nTHREAD UP: 5-1/2\" 15.5 LB/FT SL-APEX BOX\nTHREAD DOWN: 5-1/2\" 15.5 LB/FT SL-APEX PIN\nPRESSURE RATING: 6900PSI MIN\nTEMPERATURE RATING: 300 DEGF\nINSIDE DIAMETER: 4.856\"\nDRIFT: 4.825\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\n\n","ZGMD_GGE_MANDREL","PD",0,0,0,{"v":21402.5,"d":"21,402.50"}]
[1000041,"X-OVER,7\",23#,HYDRIL 521 PIN,SLHT PIN",null,null,"EA","DRL","4000008","WEATHERFORD USA","284156-NPN","","X-OVER: Cross Over Sub\nLenght: 7\"\nWeight: 23#\nConnection : HYDRIL 521 PIN,SLHT PIN\nPart#284156-NPN\n","","","","","","","-","-","PD",0,0,0,{"v":2201.23,"d":"2,201.23"}]
[1000050,"CTRL:TEC","CTR","CENTRALISER","FT","COM","4000468","HALLIBURTON","665775 / 95BA1100012251","CONTROL:\nTYPE: TEC\n","CABLE:ENCAPSULATED DOWNHOLE GAUGE CABLE\nTYPE 16 AWG SOLID COPPER\nENCASED IN 1/4\" OD INCOLOY 825 TUBING WITH FEP Insulation\nENCAPSULATION 11MM X 11MM TPR/TPV/TPE\nLENGTH TO BE SPECIFIED UPON ORDER\nWALL THICKNESS(IN.): 0.035\n","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","13June 2017 PO Long Text as per below:\nCABLE:ENCAPSULATED DOWNHOLE GAUGE CABLE\nTYPE 100% SOLID COPPER CONDUCTOR\nENCASED IN 1/4\" OD INCOLOY 825 TUBING WITH EPOXY FILL\nENCAPSULATION 11MM X 11MM POLYAMIDE TI200\nLENGTH TO BE SPECIFIED UPON ORDER\nWALL THICKNESS(IN.): 0.035\nWORKING PRESSURE (PSI): 10,000","","","","100121840","CONTROL:\nTYPE: TEC\n","ZGMD_CTRL_NM","PD",0,0,0,2.14]
[1000051,"C/L:0.25\" X 3,TRPL FLATPACK,INCLY 825,L>",null,null,"FT","COM","4000007","HALLIBURTON USA SINGAPORE","102436321","CONTROL LINE:\nSIZE: 0.25\" X 3\nTYPE: TRIPLE FLATPACK\nMATERIAL: INCOLOY 825\nSPECIFICATION: LASER WELDED, DRAWN ANNEALED TUBING\nENCAPSULATION SECTION SIZE: 33MM X 12MM\nENCAPSULATION MATERIAL: NYLON GR. 12, POLYAMIDE TT200\nFLUSHING/FILLING STANDARD: NAS 1638 CLASS 6\nFILLING TYPE: TEXACO RANDO HDZ15 OIL\nPACKING: STEEL DRUM\n","ADDITIONAL INFORMATION: WITH CONTINUOUS ENCAPSULATION STRIPPING AIDS","","12 June 2017 PO Long as per below:\nCONTROL LINE:\nSIZE: 0.25\" X 3\nMATERIAL: INCOLOY 825\nSPECIFICATION: LASER WELDED, DRAWN ANNEALED TUBING\nENCAPSULATION SECTION SIZE: 33MM X 12MM\nENCAPSULATION MATERIAL: NYLON GRADE 12, POLYAMIDE TT200\nFLUSHING/FILLING STANDARD: NAS 1638 CLASS 6\nFILLING TYPE: TEXACO RANDO HDZ15 OIL\nPACKING: STEEL DRUM\nADDITIONAL INFORMATION: WITH CONTINUOUS ENCAPSULATION STRIPPING AIDS","","","","","CONTROL LINE:\nSIZE: 0.25\" X 3\nTYPE: TRIPLE FLATPACK\nMATERIAL: INCOLOY 825\nSPECIFICATION: LASER WELDED, DRAWN ANNEALED TUBING\nENCAPSULATION SECTION SIZE: 33MM X 12MM\nENCAPSULATION MATERIAL: NYLON GR. 12, POLYAMIDE TT200\nFLUSHING/FILLING STANDARD: NAS 1638 CLASS 6\nFILLING TYPE: TEXACO RANDO HDZ15 OIL\nPACKING: STEEL DRUM\n","ZGMD_C_L_NM","PD",0,0,0,10.48]
[1000242,"CTR:13-3/8\"CASING X 16\"OH,HNG,BOW SPR,N>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-B-01-13381600","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 13-3/8\"CASING  X 16\"OH\nTYPE: HINGED\nCONFIGURATION: BOW SPRING\nSTYLE: NON WELD\n\n","Centraliser for 13-3/8\" Casing in 16\" OH\n(Hinged Non Weld Bow Spring Centralizer)\nQA/QC: API 10D, API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 13-3/8\"CASING  X 16\"OH\nTYPE: HINGED\nCONFIGURATION: BOW SPRING\nSTYLE: NON WELD\n\n","ZGMD_CTRLSER_NM","PD",0,0,0,28.42]
[1000243,"CTR:20\" X 23\"OH,HNG,BOW SPR,NON WELD,AP>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-B-01-20002300","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 20\" X 23\"OH\nTYPE: HINGED\nCONFIGURATION: BOW SPRING\nSTYLE: NON WELD\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","Centraliser for 20\" Conductor in 23\" OH\n(Hinged Non Weld Bow Spring Centralizer)\nQA/QC: API 10D, API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 20\" X 23\"OH\nTYPE: HINGED\nCONFIGURATION: BOW SPRING\nSTYLE: NON WELD\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",30,0,0,{"v":52.8,"d":"52.80"}]
[1000244,"CTR:7\" X 8-1/2\" OH,BOW SPR,NO HNG,API 1>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-B-19-07000812","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 7\" X 8-1/2\" OH\nTYPE: BOW SPRING\nCONFIGURATION: NO HINGED\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","Centraliser for 7\" Liner in 8-1/2\" Open Hole\n(Bow - Single piece - No Hinged - Stello-N-Centralizer - No buttons)\nQA/QC: API 10D, API Q1, ISO 9001","","","03","","","199140893","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 7\" X 8-1/2\" OH\nTYPE: BOW SPRING\nCONFIGURATION: NO HINGED\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",0,0,0,34.59]
[1000245,"CTR:9-5/8\" X 12-1/4\"OH,BOW SPR,NO HINGE>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-B-19-09581214","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 9-5/8\" X 12-1/4\"OH\nTYPE: BOW SPRING\nCONFIGURATION: NO HINGED-NO BUTTONS\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","Centraliser for 9-5/8\" Casing inside 13-3/8\" casing\n(9-5/8\" x 12-1/4\" Stello-N-Centralizer -Bow - Single piece only\nNo Hinged - No Buttons)\nQA/QC: API 10D, API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 9-5/8\" X 12-1/4\"OH\nTYPE: BOW SPRING\nCONFIGURATION: NO HINGED-NO BUTTONS\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",0,0,0,51.48]
[1000246,"CTR:7\" X 8-1/2\" OH,BOW SPR,NO HINGED-ST>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-B-21-07000812","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 7\" X 8-1/2\" OH\nTYPE: BOW SPRING\nCONFIGURATION: NO HINGED-STELLO-N-CENTRALIZER\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","Centraliser for 7\" Liner in 8-1/2\" Open Hole\n(Bow - Single piece - No Hinged - Stello-N-Centralizer - w/buttons)\nQA/QC: API 10D, API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 7\" X 8-1/2\" OH\nTYPE: BOW SPRING\nCONFIGURATION: NO HINGED-STELLO-N-CENTRALIZER\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",0,0,0,43.56]
[1000247,"CTR:9-5/8\" X 12-1/4\"OH,BOW SPR,NO HINGE>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-B-21-09581214","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 9-5/8\" X 12-1/4\"OH\nTYPE: BOW SPRING\nCONFIGURATION: NO HINGED-W/ BUTTONS\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","Centraliser for 9-5/8\" Casing inside 13-3/8\" casing\n(9-5/8\" x 12-1/4\" Stello-N-Centralizer - Bow - Single piece only -\nNo Hinged - W/ Buttons)\nQA/QC: API 10D, API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 9-5/8\" X 12-1/4\"OH\nTYPE: BOW SPRING\nCONFIGURATION: NO HINGED-W/ BUTTONS\nSPECIFICATION: API 10D, API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",0,0,0,{"v":54.2,"d":"54.20"}]
[1000248,"CTR:5\" X 18.75\"(20\"),BOW,HNG,API Q1,ISO>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-O-01-05002000","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 5\" X 18.75\"(20\")\nTYPE: BOW\nCONFIGURATION: HINGED\nSPECIFICATION: API Q1, ISO 9001\n","Centraliser for 5\" Drill Pipe inside 20\" Casing (Bow)\nQA/QC: API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 5\" X 18.75\"(20\")\nTYPE: BOW\nCONFIGURATION: HINGED\nSPECIFICATION: API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",10,0,0,{"v":59.4,"d":"59.40"}]
[1000249,"CTR:13-3/8\"CASING X 17-1/2\"OH,HNG,RIGID>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-R-01-13381712","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 13-3/8\"CASING  X 17-1/2\"OH\nTYPE: HINGED\nCONFIGURATION:  RIGID POSITIVE\nSTYLE: NON WELD\nSPECIFICATION: API Q1, ISO 9001\n","Centraliser for 13-3/8\" Casing inside 20\" Conductor\n(13-3/8\" x 17-1/2\" Hinged Non Weld Rigid Positive Centralizer)\nQA/QC: API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 13-3/8\"CASING  X 17-1/2\"OH\nTYPE: HINGED\nCONFIGURATION:  RIGID POSITIVE\nSTYLE: NON WELD\nSPECIFICATION: API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",600,0,0,29.17]
[1000250,"CTR:13-3/8\" X 18-1/4\"OH (20\"),HNG,RIGID>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-R-01-13381814","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 13-3/8\" X 18-1/4\"OH (20\")\nTYPE: HINGED\nCONFIGURATION: RIGID POSITIVE\nSTYLE: NON WELD\nSPECIFICATION: API Q1, ISO 9001\n","Centraliser for 13-3/8\" Casing inside 20\" Conductor\n(13-3/8\" x 18 1/4\" Hinged Non Weld Rigid Positive Centralizer)\n","","","03","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 13-3/8\" X 18-1/4\"OH (20\")\nTYPE: HINGED\nCONFIGURATION: RIGID POSITIVE\nSTYLE: NON WELD\nSPECIFICATION: API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",0,0,0,28.34]
[1000251,"CTR:13-3/8\" X 26\" OH (30\"),HNG,RIGID PO>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-R-01-13382600","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 13-3/8\" X 26\" OH (30\")\nTYPE: HINGED\nCONFIGURATION: RIGID POSITIVE\nSTYLE: NON WELD\nSPECIFICATION: API Q1, ISO 9001\n","Centraliser for 13-3/8\" Casing in 30\" Conductor\n(13-3/8\" x 26\" - Hinged Non Weld Rigid Positive Centralizer\nQA/QC: API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 13-3/8\" X 26\" OH (30\")\nTYPE: HINGED\nCONFIGURATION: RIGID POSITIVE\nSTYLE: NON WELD\nSPECIFICATION: API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",20,0,0,29.17]
[1000252,"CTR:7\" X 8-1/2\" OH,RIGID,SPIROGLADER,AP>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-S-05-07000812","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 7\" X 8-1/2\" OH\nTYPE: RIGID\nCONFIGURATION: SPIROGLADER\nSPECIFICATION: API Q1, ISO 9001\n","Centraliser to aid rotation of 7\" Liner\n(7\" x 8-1/2\" hole Heavy Duty Spiroglader)\nQA/QC: API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 7\" X 8-1/2\" OH\nTYPE: RIGID\nCONFIGURATION: SPIROGLADER\nSPECIFICATION: API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",300,0,0,{"v":26.4,"d":"26.40"}]
[1000253,"CTR:9-5/8\" X 12-1/4\"OH,RIGID,HVY/D SPIR>","CTR","CENTRALISER","EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-S-05-09581214","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 9-5/8\" X 12-1/4\"OH\nTYPE: RIGID\nCONFIGURATION: HEAVY DUTY SPIROGLADER\nSPECIFICATION: API Q1, ISO 9001\n","Centraliser to aid rotation of 9-5/8\" Casing\n(9-5/8\" x 12-1/4\" Heavy Duty Spiroglader)\nQA/QC: API Q1, ISO 9001","","","","","","","CENTRALISER:\nCASING/TUBING SIZE X HOLE SIZE: 9-5/8\" X 12-1/4\"OH\nTYPE: RIGID\nCONFIGURATION: HEAVY DUTY SPIROGLADER\nSPECIFICATION: API Q1, ISO 9001\n","ZGMD_CTRLSER_NM","PD",0,0,0,29.04]
[1000254,"COLLAR:STOP;HNG SET SCRW,5\"",null,null,"EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-SC-04-0500","COLLAR:STOP;\nTYPE: HINGED SET SCREW\nCASING/TUBING SIZE: 5\"\n","Stop Collar for 5\" Drill Pipe (Hinged Set Screw Stop Collar)\nQA/QC: API 10D-2, API Q1, ISO 9001","","","","01","1047938","","COLLAR:STOP;\nTYPE: HINGED SET SCREW\nCASING/TUBING SIZE: 5\"\n","ZGMD_CLLR_STP","PD",50,0,0,4.29]
[1000255,"COLLAR:STOP;HNG SET SCRW,13-3/8\"",null,null,"EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-SC-04-1338","COLLAR:STOP;\nTYPE: HINGED SET SCREW\nCASING/TUBING SIZE: 13-3/8\"\n","Stop Collar for 13-3/8\" Casing (Hinged Set Screw Stop Collar)\nQA/QC: API 10D-2, API Q1, ISO 9001","","","","01","","","COLLAR:STOP;\nTYPE: HINGED SET SCREW\nCASING/TUBING SIZE: 13-3/8\"\n","ZGMD_CLLR_STP","PD",0,0,0,8.18]
[1000256,"COLLAR:STOP;HNG SET SCRW,20\"",null,null,"EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-SC-04-2000","COLLAR:STOP;\nTYPE: HINGED SET SCREW\nCASING/TUBING SIZE: 20\"\n","Stop Collar for 20\" Conductor (Hinged Set Screw Stop Collar)\nQA/QC: API 10D-2, API Q1, ISO 9001","","","","01","1047873","","COLLAR:STOP;\nTYPE: HINGED SET SCREW\nCASING/TUBING SIZE: 20\"\n","ZGMD_CLLR_STP","PD",0,0,0,12.94]
[1000257,"COLLAR:STOP;SET SCRW,7\",7.951\",7.125\",H>",null,null,"EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-SC-05-0700","COLLAR:STOP;\nTYPE: SET SCREW\nCASING/TUBING SIZE: 7\"\nOUTSIDE DIAMETER: 7.951\"\nINSIDE DIAMETER: 7.125\"\nMATERIAL: H.R IS 10748 GRADE 1\nNUMBER OF SCREWS: 6\nSCREW SIZE: M12\nSCREW MATERIAL: H.T.\nCASING/TUBING GRADE: L80\n","Stop Collar for 7\" Liner (Slip on Set Screw -no weld)\nQA/QC: API 10D-2, API Q1, ISO 9001","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","03","","","","COLLAR:STOP;\nTYPE: SET SCREW\nCASING/TUBING SIZE: 7\"\nOUTSIDE DIAMETER: 7.951\"\nINSIDE DIAMETER: 7.125\"\nMATERIAL: H.R IS 10748 GRADE 1\nNUMBER OF SCREWS: 6\nSCREW SIZE: M12\nSCREW MATERIAL: H.T.\nCASING/TUBING GRADE: L80\n","ZGMD_CLLR_STP","PD",0,0,0,8.72]
[1000258,"COLLAR:STOP;SET SCRW,9-5/8\"",null,null,"EA","DRL","4000247","NEOZ ENERGY PVT LTD","NE-SC-05-0958","COLLAR:STOP;\nTYPE: SLIP ON SET SCREW\nCASING/TUBING SIZE: 9-5/8\"\n","Stop Collar for 9-5/8\" Casing (Slip on Set Screw Stop Collar-no weld)\nQA/QC: API 10D-2, API Q1, ISO 9001","","","03","","","","COLLAR:STOP;\nTYPE: SLIP ON SET SCREW\nCASING/TUBING SIZE: 9-5/8\"\n","ZGMD_CLLR_STP","PD",0,0,0,9.92]
[1000259,"PLUG,DP,WIPER,5\" LD",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","0500 LD DPWP","PLUG: DP wiper plug\nDiameter: 5\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","PLUG: Latch Down DP Wiper Plug\nDiameter: 5\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","","","","","","","-","-","PD",0,0,0,{"v":439.6,"d":"439.60"}]
[1000260,"PLUG:CMT;TOP,BLK,NR,9-5/8\",40#,10.63\"+/>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","PLATN0950001NNSP","PLUG:CEMENTING;\nTYPE: TOP,BLACK,NR\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.63\"+/-0.25\"\nMATERIAL: NITRILE\nCORE MATERIAL: PHENOLIC\nMIN CASING ID: 8.375\"\nOUTSIDE DIAMETER: 9.31\"\nDRAWING/DOCUMENT REFERENCE-1: 963-LAPNNEW-TOP-PLUG","9-5/8\" Standard Cementing Top Plug with Non-Rotating (NR) Profile\nBlack colour\nDrawing attached\n\n","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","04","01","1047876","","PLUG:CEMENTING;\nTYPE: TOP,BLACK,NR\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.63\"+/-0.25\"\nMATERIAL: NITRILE\nCORE MATERIAL: PHENOLIC\nMIN CASING ID: 8.375\"\nOUTSIDE DIAMETER: 9.31\"\nDRAWING/DOCUMENT REFERENCE-1: 963-LAPNNEW-TOP-PLUG","ZGMD_PLG_CMT","PD",0,0,0,449.13]
[1000261,"PLUG:CMT;BTM,W/DSK,250-350PSI,NR,9-5/8\">",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","PLABN0950001HSSP","PLUG:CEMENTING;\nTYPE: BTM,W/DISK,250-350PSI,NR\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.68\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nMIN CASING ID: 8.375\"\nOUTSIDE DIAMETER: 9.25\"\nDRAWING/DOCUMENT REFERENCE-1: 963LAPNNEW-BTM-PLUG-NOCQ","9-5/8\" Standard Cementing Bottom Plug with Non-Rotating (NR) profile and\nNitrile Rupture Disk 250-350 psi\nOrange colour plug\n\nDrawing attached\n\n","CERTIFICATE OF CONFORMITY\nQC PATH 1 – FAT+DOC PRE-REVIEW+WH INSP","","","01","1047877","","PLUG:CEMENTING;\nTYPE: BTM,W/DISK,250-350PSI,NR\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.68\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nMIN CASING ID: 8.375\"\nOUTSIDE DIAMETER: 9.25\"\nDRAWING/DOCUMENT REFERENCE-1: 963LAPNNEW-BTM-PLUG-NOCQ","ZGMD_PLG_CMT","PD",0,0,0,431.03]
[1000262,"PLUG,CMT,13-3/8\",BTM,CONV",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","PSTT1330000001NPNS","PLUG: Conventional bottom plug for 13-3/8” conventional cementing\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","PLUG: Conventional bottom plug for 13-3/8” conventional cementing\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","","","","","","","-","-","PD",0,0,0,{"v":1068.93,"d":"1,068.93"}]
[1000263,"PLUG,CMT,13-3/8\",TOP,CONV",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","PSTB1330000001NPSS","PLUG: Conventional top plug for 13-3/8” conventional cementing\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","PLUG: Conventional top plug for 13-3/8” conventional cementing\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","","","","","","","-","-","PD",0,0,0,{"v":1068.93,"d":"1,068.93"}]
[1000264,"SHOE:FLOAT;DV - ECC,13-3/8\",L80,API 5CT>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","LA2GA000133LL380NAP","SHOE:FLOAT;\nMODEL: DV - ECCENTRIC\nCASING SIZE: 13-3/8\"\nGRADE: L80\nTHREADS: API 5CT/QP FE\nCONNECTION: SL-HC\nWEIGHT: 61#\n","DOWN JETS, ALUMINIUM ECCENTRIC NOSE FLOAT SHOE\n\nPLEASE REFER THE ATTACHED DRAWING.\n","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","100134163","SHOE:FLOAT;\nMODEL: DV - ECCENTRIC\nCASING SIZE: 13-3/8\"\nGRADE: L80\nTHREADS: API 5CT/QP FE\nCONNECTION: SL-HC\nWEIGHT: 61#\n","ZGMD_SHOE_FLOAT","PD",0,0,0,{"v":3934.92,"d":"3,934.92"}]
[1000265,"SHOE,FLOAT,7\",23#SL HT,DV,L-80",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","LA1BA000070LL282NA","Float Shoe: Float Shoe (DV)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-HT\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (DV)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-HT\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":1224.1,"d":"1,224.10"}]
[1000266,"SHOE,FLOAT,13-3/8\",61#SL BOSS,DV,K55",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","LA1AA000133KK374NA","Float Shoe: Float Shoe (DV)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (DV)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":2350.33,"d":"2,350.33"}]
[1000267,"SHOE,FLOAT,13-3/8\",61#SL HC,DV,K55",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","LA1AA000133KK380NAP","Float Shoe: Float Shoe (DV)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (DV)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",15,0,0,{"v":1901.06,"d":"1,901.06"}]
[1000268,"SHOE,FLOAT,20\"166.5#SL XLCS,SV,CONV,X65",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","AA1AA000200228D2NA","Float Shoe: Float Shoe (SV - Conventional)\nDiameter: 20”\nWeight: 166.56#\nGrad: X-65\nConnection: SL-XLC-SE\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (SV - Conventional)\nDiameter: 20”\nWeight: 166.56#\nGrad: X-65\nConnection: SL-XLC-SE\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":4246.8,"d":"4,246.80"}]
[1000269,"SHOE,FLOAT,7\",23#SL APEX,DV,L-80",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","LA1BA000070LL272NA","Float Shoe: Float Shoe (DV)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (DV)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":1204.61,"d":"1,204.61"}]
[1000270,"SHOE,FLOAT,9-5/8\",40#SL APEX,DV,L-80",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","LA1AA000095LL372NAP","Float Shoe: Float Shoe (DV)\nDiameter: 9-5/8\"\nWeight: 40#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (DV)\nDiameter: 9-5/8\"\nWeight: 40#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":1638.89,"d":"1,638.89"}]
[1000271,"SHOE,FLOAT,13-3/8\",61#SL-HC,DV,K55,RMR",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","OA1ZA0S0133KK380NA","Float Shoe: Float Shoe (DV - Reamer)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (DV - Reamer)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC: API 5CT / QP FE","","","03","","","199140825","-","-","PD",0,0,0,{"v":6412.4,"d":"6,412.40"}]
[1000272,"SHOE,FLOAT,20\"106.5#SL BOSS,SV,CONV,X56",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","AA1AA000200FF274NA","Float Shoe: Float Shoe (SV - Conventional)\nDiameter: 20”\nWeight: 106.5#\nGrad: X-56\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (SV - Conventional)\nDiameter: 20”\nWeight: 106.5#\nGrad: X-56\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":3470.83,"d":"3,470.83"}]
[1000273,"SHOE:FLOAT;SV-REAMER,9-5/8\",L-80,API 5C>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","DA2Z00S0095LL372NA","SHOE:FLOAT;\nMODEL: SV-REAMER\nCASING SIZE: 9-5/8\"\nGRADE: L-80\nTHREADS: API 5CT / QP FE\nCONNECTION: SL-APEX\nWEIGHT: 40#\n","","","","","","","","SHOE:FLOAT;\nMODEL: SV-REAMER\nCASING SIZE: 9-5/8\"\nGRADE: L-80\nTHREADS: API 5CT / QP FE\nCONNECTION: SL-APEX\nWEIGHT: 40#\n","ZGMD_SHOE_FLOAT","PD",0,0,0,{"v":3166.25,"d":"3,166.25"}]
[1000274,"SHOE,FLOAT,13-3/8\",61#SL-BOSS,SV,K55,RMR",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","DA1ZA0S0133KK374NA","Float Shoe: Float Shoe (SV - Reamer)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (SV - Reamer)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":6452.13,"d":"6,452.13"}]
[1000275,"SHOE,FLOAT,13-3/8\",61#SL-HC,SV,K55,RMR",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","DA1ZA0S0133KK380NA","Float Shoe: Float Shoe (SV - Reamer)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (SV - Reamer)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":6452.13,"d":"6,452.13"}]
[1000276,"SHOE,FLOAT,7\",23#SL APEX,SV,L-80,RMR JT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","DA1ZA0J0070LL272NA","Float Shoe: Float Shoe (DV - Reamer)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (SV - Reamer)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",3,0,0,{"v":2216.17,"d":"2,216.17"}]
[1000277,"SHOE,FLOAT,7\",23#SL HT,SV,L-80,RMR JT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","DA1UA0J0070LL282NAP","Float Shoe: Float Shoe (SV - Reamer)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-HT\nQA/QC:  API 5CT / QP FE","Float Shoe: Float Shoe (SV - Reamer)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-HT\nQA/QC:  API 5CT / QP FE","","Float Shoe: Float Shoe (SV - Reamer)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-HT\nQA/QC:  API 5CT / QP FE","","","","","-","-","PD",5,0,0,{"v":2238.61,"d":"2,238.61"}]
[1000278,"SHOE,FLOAT,20\"106.5#BUTTWELD,STAB-IN,X56",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","EA1ABJH0200FF212NA","20\" (106.5# - X-56) Stab-in Float Shoe, Buttweld Prep\nFloat Shoe: Stab-in Float Shoe, Buttweld Prep\nDiameter: 20\"\nWeight: 106.5#\nGrad: X-56\nQA/QC: API 5CT / QP FE","20\" (106.5# - X-56) Stab-in Float Shoe, Buttweld Prep\nFloat Shoe: Stab-in Float Shoe, Buttweld Prep\nDart latch option\nDiameter: 20\"\nWeight: 106.5#\nGrad: X-56\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":2003.15,"d":"2,003.15"}]
[1000279,"SHOE,FLOAT,20\"106.5#SL BOSS,STAB-IN,X56",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","EA1ABJH0200FF274NA","Float Shoe: Stab-in Float Shoe\nDiameter: 20\"\nWeight: 106.5#\nGrad: X-56\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","Float Shoe: Stab-in Float Shoe\nDart latch option\nDiameter: 20\"\nWeight: 106.5#\nGrad: X-56\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","","","","","","100088777","-","-","PD",0,0,0,{"v":3948.55,"d":"3,948.55"}]
[1000280,"(BLCK)SHOE:FLOAT;500TLP-PVTS,166.56#,SV,",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","EA1ABJF0200228KSNAP","SHOE:FLOAT;\nMODEL: 500TLP-PVTS\nCASING SIZE: 166.56#\nVALVE: SV\nTHREADS: BOX\nCONNECTION: XLC-SE\nWEIGHT: 166.56#\nFLOAT SHOE OD: 20\"\n","20\" XLCSE 500TLP X65\nTAG-IN FLOAT SHOE W RECEPTACLE FOR LATCH DOWN PLUG\nSINGLE VALVE\nTYPE 500TLP-PVTS, 166.56 PPF, X-65\n","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","06","","1047869","","SHOE:FLOAT;\nMODEL: 500TLP-PVTS\nCASING SIZE: 166.56#\nVALVE: SV\nTHREADS: BOX\nCONNECTION: XLC-SE\nWEIGHT: 166.56#\nFLOAT SHOE OD: 20\"\n","ZGMD_SHOE_FLOAT","PD",0,0,0,{"v":5287.09,"d":"5,287.09"}]
[1000281,"SHOE:FLOAT;SV-ECC,9-5/8\",L80,SLAPX,40#",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","AA2GA000095LL372NAP","SHOE:FLOAT;\nMODEL: SV-ECC\nCASING SIZE: 9-5/8\"\nGRADE: L80\nCONNECTION: SL APEX\nWEIGHT: 40#\n","(SV - Eccentric)\nQA/QC: API 5CT / QP FE","","","","","","","SHOE:FLOAT;\nMODEL: SV-ECC\nCASING SIZE: 9-5/8\"\nGRADE: L80\nCONNECTION: SL APEX\nWEIGHT: 40#\n","ZGMD_SHOE_FLOAT","PD",0,0,0,{"v":1746.25,"d":"1,746.25"}]
[1000282,"SHOE,FLOAT,7\",23#SL APEX,SV,L-80,ECC JT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","AA2GA000070LL272NA","Float Shoe: Float Shoe (DV - Eccentric)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (SV - Eccentric)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",3,0,0,{"v":1648.35,"d":"1,648.35"}]
[1000283,"SHOE,FLOAT,7\",23#SL HT,SV,L-80,ECC JT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","AA2GA000070LL282NA","Float Shoe: Float Shoe (DV - Eccentric)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-HT\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (SV - Eccentric)\nDiameter: 7\"\nWeight: 23#\nGrad: L-80\nConnection: SL-HT\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":1619.23,"d":"1,619.23"}]
[1000284,"SHOE,FLOAT,13-3/8\",61#SLBOSS,SV,K55,ECC",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","AA2GA000133KK374NA","Float Shoe: Float Shoe (SV - Eccentric)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (SV - Eccentric)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":2448.63,"d":"2,448.63"}]
[1000285,"SHOE,FLOAT,13-3/8\",61#SLHC,SV,K55,ECC JT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","AA2GA000133KK380NA","Float Shoe: Float Shoe (SV - Eccentric)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe (SV - Eccentric)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":2448.63,"d":"2,448.63"}]
[1000286,"SHOE,FLOAT,13-3/8\",61#SLBOSS,DV,K55,FPOR",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","LA3AA000133KK374NA","Float Shoe: Float Shoe  (DV - Flow ports pointing upwards)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","Float Shoe: Float Shoe  (DV - Flow ports pointing upwards)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",0,0,0,{"v":2066.5,"d":"2,066.50"}]
[1000287,"SHOE:FLOAT;DV-FPORT,13-3/8\",K55,SLHC,61#",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","LA3AA000133KK380NAP","SHOE:FLOAT;\nMODEL: DV-FPORT\nCASING SIZE: 13-3/8\"\nGRADE: K55\nCONNECTION: SLHC\nWEIGHT: 61#\n","(DV - Flow ports pointing upwards)\nQA/QC: API 5CT / QP FE","","","","","","","SHOE:FLOAT;\nMODEL: DV-FPORT\nCASING SIZE: 13-3/8\"\nGRADE: K55\nCONNECTION: SLHC\nWEIGHT: 61#\n","ZGMD_SHOE_FLOAT","PD",0,0,0,{"v":1982.12,"d":"1,982.12"}]
[1000288,"COLLAR:FLOAT;DV - N/R,40#,L-80,SL-APEX,>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","NA1BF000095LL37271P","COLLAR:FLOAT;\nMODEL: DV - NON ROTATING\nWEIGHT: 40#\nGRADE: L-80\nCONNECTION: SL-APEX\nVALVE: DOUBLE VALVE\nFLOAT COLLAR OD: 9-5/8\"\n","Float Collar:Float Collar (DV - Non Rotating)\n\nQA/QC: API 5CT / QP FE","","","","","","","COLLAR:FLOAT;\nMODEL: DV - NON ROTATING\nWEIGHT: 40#\nGRADE: L-80\nCONNECTION: SL-APEX\nVALVE: DOUBLE VALVE\nFLOAT COLLAR OD: 9-5/8\"\n","ZGMD_COLLAR_FLOAT","PD",0,0,0,{"v":2226.73,"d":"2,226.73"}]
[1000289,"COLLAR:FLOAT;700DV-PVTS,7\",7\",23#,L80,S>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","MAIBD000070LL27271","COLLAR:FLOAT;\nMODEL: 700DV-PVTS\nSIZE: 7\"\nCASING SIZE: 7\"\nWEIGHT: 23#\nGRADE: L80\nCONNECTION: SL APEX\nCONNECTION TYPE: BOX * PIN\nVALVE: PVTS\nVALVE ASSEMBLY: DOUBLE VALVE PVTS\nFLOAT COLLAR OD: 7.656\" (+/-0.05\")\nFLOAT COLLAR ID: 6.350\" (+/-0.01\")\nDRILL OUT OD: 6.25\" DRIFT\nLENGTH: 35.0\" (+/-0.5\")\n","SEE ATTACHED.","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","COLLAR:FLOAT;\nMODEL: 700DV-PVTS\nSIZE: 7\"\nCASING SIZE: 7\"\nWEIGHT: 23#\nGRADE: L80\nCONNECTION: SL APEX\nCONNECTION TYPE: BOX * PIN\nVALVE: PVTS\nVALVE ASSEMBLY: DOUBLE VALVE PVTS\nFLOAT COLLAR OD: 7.656\" (+/-0.05\")\nFLOAT COLLAR ID: 6.350\" (+/-0.01\")\nDRILL OUT OD: 6.25\" DRIFT\nLENGTH: 35.0\" (+/-0.5\")\n","ZGMD_COLLAR_FLOAT","PD",3,0,0,{"v":1886.24,"d":"1,886.24"}]
[1000290,"COLLAR:FLOAT;DV,23#,L-80,SL-HT,DBL VLV,>","VLV","VALVE","EA","DRL","4000246","FORUM US/ DAVIS LYNCH","MA1BA000070LL28281","COLLAR:FLOAT;\nMODEL: DV\nWEIGHT: 23#\nGRADE: L-80\nCONNECTION: SL-HT\nVALVE: DOUBLE VALVE\nFLOAT COLLAR OD: 7\"\n","Float Collar: Float Collar (DV)\n\nQA/QC: API 5CT / QP FE","","","","","","","COLLAR:FLOAT;\nMODEL: DV\nWEIGHT: 23#\nGRADE: L-80\nCONNECTION: SL-HT\nVALVE: DOUBLE VALVE\nFLOAT COLLAR OD: 7\"\n","ZGMD_COLLAR_FLOAT","PD",0,0,0,{"v":1842.15,"d":"1,842.15"}]
[1000291,"COLLAR:FLOAT;SV - N/R,40#,L-80,SL-APEX,>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","NA1BF000095LL37271","COLLAR:FLOAT;\nMODEL: SV - NON ROTATING\nWEIGHT: 40#\nGRADE: L-80\nCONNECTION: SL-APEX\nVALVE: SINGLE VALVE\nFLOAT COLLAR OD: 9-5/8\"\n","Float Collar:Float Collar (SV - Non Rotating)\n\nQA/QC: API 5CT / QP FE","","","","","","","COLLAR:FLOAT;\nMODEL: SV - NON ROTATING\nWEIGHT: 40#\nGRADE: L-80\nCONNECTION: SL-APEX\nVALVE: SINGLE VALVE\nFLOAT COLLAR OD: 9-5/8\"\n","ZGMD_COLLAR_FLOAT","PD",0,0,0,{"v":2143.58,"d":"2,143.58"}]
[1000292,"COLLAR:FLOAT;SV,13-3/8\",61#,K-55,SL-BOS>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","BA1BI060133KK37473","COLLAR:FLOAT;\nMODEL: SV\nSIZE: 13-3/8\"\nWEIGHT: 61#\nGRADE: K-55\nCONNECTION: SL-BOSS\nVALVE: SINGLE VALVE\n","Float Collar (SV)\nQA/QC: API 5CT / QP FE","","","","","","","COLLAR:FLOAT;\nMODEL: SV\nSIZE: 13-3/8\"\nWEIGHT: 61#\nGRADE: K-55\nCONNECTION: SL-BOSS\nVALVE: SINGLE VALVE\n","ZGMD_COLLAR_FLOAT","PD",0,0,0,{"v":4199.38,"d":"4,199.38"}]
[1000293,"COLLAR:FLOAT;SV,13-3/8\",61#,K-55,SL-HC,>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","BA1BI060133KK38079","COLLAR:FLOAT;\nMODEL: SV\nSIZE: 13-3/8\"\nWEIGHT: 61#\nGRADE: K-55\nCONNECTION: SL-HC\nVALVE: SINGLE VALVE\n","Float Collar (SV)\nQA/QC: API 5CT / QP FE","","","","","","","COLLAR:FLOAT;\nMODEL: SV\nSIZE: 13-3/8\"\nWEIGHT: 61#\nGRADE: K-55\nCONNECTION: SL-HC\nVALVE: SINGLE VALVE\n","ZGMD_COLLAR_FLOAT","PD",0,0,0,{"v":4199.38,"d":"4,199.38"}]
[1000294,"COLLAR:FLOAT;STAB-IN FC,106.5#,X-56,SL->",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","FA1ABJH0200FF27473","COLLAR:FLOAT;\nMODEL: STAB-IN FLOAT COLLAR\nWEIGHT: 106.5#\nGRADE: X-56\nCONNECTION: SL-BOSS\nFLOAT COLLAR OD: 20\"\n","Float Collar: Stab-in Float Collar\nDart latch option\nQA/QC: API 5CT / QP FE","","","","","","","COLLAR:FLOAT;\nMODEL: STAB-IN FLOAT COLLAR\nWEIGHT: 106.5#\nGRADE: X-56\nCONNECTION: SL-BOSS\nFLOAT COLLAR OD: 20\"\n","ZGMD_COLLAR_FLOAT","PD",0,0,0,{"v":6907.35,"d":"6,907.35"}]
[1000295,"COLLAR:FLOAT;STAB-IN FC,166.56#,X-65,SL>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","FA1ABJH0200228D2D1","COLLAR:FLOAT;\nMODEL: STAB-IN FLOAT COLLAR\nWEIGHT: 166.56#\nGRADE: X-65\nCONNECTION: SL-XLC-SE\nFLOAT COLLAR OD: 20”\n","Float Collar: Stab-in Float Collar\nDart latch option\nQA/QC: API 5CT / QP FE","","","","","","","COLLAR:FLOAT;\nMODEL: STAB-IN FLOAT COLLAR\nWEIGHT: 166.56#\nGRADE: X-65\nCONNECTION: SL-XLC-SE\nFLOAT COLLAR OD: 20”\n","ZGMD_COLLAR_FLOAT","PD",0,0,0,{"v":7149.15,"d":"7,149.15"}]
[1000296,"SEAL,STRING-IN ADAPT, 20\" - 5\" x 4.5\" IF",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","B-122C","Seal: Seal Adapter Compatible with 5\" Drill Pipe 4.5 IF\nDiameter: 20\"\nQA/QC: ISO 9001-2008 / API Q1 / QPM REV 4","Seal: Seal Adapter Compatible with 5\" Drill Pipe 4.5 IF\nDiameter: 20\"\nQA/QC: ISO 9001-2008 / API Q1 / QPM REV 4","","","","01","1047871","","-","-","PD",0,0,0,441.44]
[1000297,"PLUG:CMT;BTM,OR,FLOATATION,W250-350,9-5>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","PLABN0950001HSSQ","PLUG:CEMENTING;\nTYPE: BTM,ORANGE,FLOATATION,W250-350\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.68\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nMIN CASING ID: 8.375\"\nOUTSIDE DIAMETER: 9.25\"","Plug: Cement Bottom Plug, (Orange) Anti Rotation with Non-Rotating (NR)\nprofile\nSECOND BOTTOM PLUG for Floatation\nPressure: 250 - 350 psi Nitrile rupture disk\n\nDrawing attached.","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","PLUG:CEMENTING;\nTYPE: BTM,ORANGE,FLOATATION,W250-350\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.68\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nMIN CASING ID: 8.375\"\nOUTSIDE DIAMETER: 9.25\"","ZGMD_PLG_CMT","PD",2,0,0,467.56]
[1000298,"PLUG:CMT;BTM,GRN,FLOATATION,W/700-900,9>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","PLABN0950001HASP","PLUG:CEMENTING;\nTYPE: BTM,GREEN,FLOATATION,W/700-900\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.68\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nOUTSIDE DIAMETER: 9.25\"","Plug: Cement Bottom Plug, (Green) Anti Rotation with Non-Rotating (NR)\nprofile\nFIRST BOTTOM PLUG for Floatation\nPressure: 700 - 900 psi (4 x 1/4\" phenolic rupture disks)\n\nDrawing attached","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","PLUG:CEMENTING;\nTYPE: BTM,GREEN,FLOATATION,W/700-900\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.68\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nOUTSIDE DIAMETER: 9.25\"","ZGMD_PLG_CMT","PD",2,0,0,413.05]
[1000299,"PLUG:CMT;TOP,BLK,F/FLOATATION,NR,9-5/8\">",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","PLATN0950001HNSP","PLUG:CEMENTING;\nTYPE: TOP,BLACK,F/FLOATATION,NR\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.68\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nMIN CASING ID: 8.38\"\nOUTSIDE DIAMETER: 9.25\"","Plug: 9-5/8\" Cement Top Plug, (Black) Anti Rotation (For Floatation)\n\n7500 psi Max recommended bump pressure with bottom plug on float collar\n5000 psi max recommended bump pressure with multiple plugs on floatation\ncollar sleeves\n\nDrawing attached","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","PLUG:CEMENTING;\nTYPE: TOP,BLACK,F/FLOATATION,NR\nCASING SIZE: 9-5/8\"\nCASING WEIGHT: 40#\nLENGTH: 10.68\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nMIN CASING ID: 8.38\"\nOUTSIDE DIAMETER: 9.25\"","ZGMD_PLG_CMT","PD",2,0,0,460.96]
[1000300,"SHOE,FLOATATION,9-5/8\",40#SL APEX,DV,L80",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","LA1QA00H095LL372NAP","Float Shoe: Float shoe, (DV, Composite nose)\nDiameter: 9-5/8\"\nWeight: 40#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","Float Shoe: Float shoe, (DV, Composite nose)\nDiameter: 9-5/8\"\nWeight: 40#\nGrad: L-80\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","","","","","","","-","-","PD",2,0,0,{"v":3002.01,"d":"3,002.01"}]
[1000301,"COLLAR:BFLE;DIA 9-5/8\",SL-APEX,40#,API >",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","Y01BFI00095LL37271","COLLAR:BAFFLE;\nSIZE: DIA 9-5/8\"\nCONNECTION A: SL-APEX\nWEIGHT: 40#\nSPECIFICATION: API 5CT / QP FE\nGRADE: L-80\nFEATURE: ANTI-ROTATION\n","Baffle Collar (Anti-Rotation)\n","","","","","","","COLLAR:BAFFLE;\nSIZE: DIA 9-5/8\"\nCONNECTION A: SL-APEX\nWEIGHT: 40#\nSPECIFICATION: API 5CT / QP FE\nGRADE: L-80\nFEATURE: ANTI-ROTATION\n","ZGMD_CLLR_BFLE","PD",0,0,0,{"v":3030.94,"d":"3,030.94"}]
[1000302,"COLLAR:FLOTATION;A-ROT,9-5/8\",40#,L-80",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","X00BF00G095LL37271P","COLLAR:FLOTATION;\nTYPE: ANTI-ROTATION\nSIZE: 9-5/8\"\nWEIGHT: 40#\nMATERIAL: L-80\n","Floatation Collar (Anti-Rotation)\nConnection: SL-APEX\nQA/QC: API 5CT / QP FE","","","","","","","COLLAR:FLOTATION;\nTYPE: ANTI-ROTATION\nSIZE: 9-5/8\"\nWEIGHT: 40#\nMATERIAL: L-80\n","ZGMD_CLLR_FLTN","PD",0,0,0,{"v":5245.24,"d":"5,245.24"}]
[1000303,"COLLAR:BFLE;DIA 9-5/8\",SL-APEX,40#,API >",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","Y01BI0Y0095LL37271P","COLLAR:BAFFLE;\nSIZE: DIA 9-5/8\"\nCONNECTION A: SL-APEX\nWEIGHT: 40#\nSPECIFICATION: API 5CT / QP FE\nGRADE: L-80\nFEATURE: 2 STAGE\n","Baffle Collar (2-S)\n","","","","","","","COLLAR:BAFFLE;\nSIZE: DIA 9-5/8\"\nCONNECTION A: SL-APEX\nWEIGHT: 40#\nSPECIFICATION: API 5CT / QP FE\nGRADE: L-80\nFEATURE: 2 STAGE\n","ZGMD_CLLR_BFLE","PD",0,0,0,{"v":2878.2,"d":"2,878.20"}]
[1000304,"PLUG,CMT,2STG,9-5/8\",SHTOFF B/UP",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","FFOD074_073F7P","Plug:  Contingency Free Fall Opening Plug (2S)\nDiameter: 9-5/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","Plug:  Contingency Free Fall Opening Plug (2S)\nDiameter: 9-5/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","","","","","","","-","-","PD",0,0,0,514.91]
[1000305,"PLUG,CMT,2STG,9-5/8\",CLSG",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","CLP095_080SP","Plug:  Closing plug (2S)\nDiameter: 9-5/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","Plug:  Closing plug (2S)\nDiameter: 9-5/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","","","","","","","-","-","PD",0,0,0,598.35]
[1000306,"PLUG:CMT;SHUT-OFF,9.625\",40#,15.38+/-0.>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","SOP095 550B2P","PLUG:CEMENTING;\nTYPE: SHUT-OFF\nCASING SIZE: 9.625\"\nCASING WEIGHT: 40#\nLENGTH: 15.38+/-0.25\"\nOUTSIDE DIAMETER: 9.188\"","9-5/8\"  First stage Shut-off Plug with 5.5\"  aluminium nose\nFor Baffle collar ID of 5.5\"\n\nSee Drawing Attached.","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","PLUG:CEMENTING;\nTYPE: SHUT-OFF\nCASING SIZE: 9.625\"\nCASING WEIGHT: 40#\nLENGTH: 15.38+/-0.25\"\nOUTSIDE DIAMETER: 9.188\"","ZGMD_PLG_CMT","PD",0,0,0,525.07]
[1000307,"PKR,9-5/8\"X13-3/8\",SL APEX,L80,3FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","INC0953LL7271A3QMYP","Packer: Short Rubber Element (3 ft)\nDiameter: 9-5/8\"\nWeight: 40#\nGrad:  L-80\nConnection: SL-APEX\nQA/QC:  API 5CT / QP PK","Packer: Short Rubber Element (3 ft)\nDiameter: 9-5/8\"\nWeight: 40#\nGrad:  L-80\nConnection: SL-APEX\nQA/QC:  API 5CT / QP PK","","","","","","","-","-","PD",0,0,0,{"v":13606.85,"d":"13,606.85"}]
[1000308,"PKR,9-5/8\"X12-1/4\",SL APEX,L80,7FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","INC0953LL7271A7QMYP","Packer: Long Rubber Element (7 ft)\nDiameter: 9-5/8\"\nWeight: 40#\nGrad:  L-80\nConnection: SL-APEX\nQA/QC:  API 5CT / QP PK","Packer: Long Rubber Element (7 ft)\nDiameter: 9-5/8\"\nWeight: 40#\nGrad:  L-80\nConnection: SL-APEX\nQA/QC:  API 5CT / QP PK","","","","","","","-","-","PD",0,0,0,{"v":17873.5,"d":"17,873.50"}]
[1000309,"PKR,13-3/8\"X20\",SL BOSS,K55,3FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","ISC1333LL7473C3QMYP","Packer: Short Rubber Element (3 ft)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC:  API 5CT / QP PK","Packer: Short Rubber Element (3 ft)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC:  API 5CT / QP PK","","","","","","","-","-","PD",0,0,0,{"v":19469.75,"d":"19,469.75"}]
[1000310,"(BLCK)PKR,13-3/8\"X20\",SL HC,K55,3FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","ISC1333LL8079C3QMYP","Packer: Short Rubber Element (3 ft)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC:  API 5CT / QP PK","Packer: Short Rubber Element (3 ft)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC:  API 5CT / QP PK","","","06","","1047998","","-","-","PD",0,0,0,{"v":18919.12,"d":"18,919.12"}]
[1000311,"PKR,13-3/8\"X16\",SL BOSS,K55,7FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","ISC1333LL7473C7QMYP","Packer:  Long Rubber Element (7 ft)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC:  API 5CT / QP PK","Packer:  Long Rubber Element (7 ft)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-BOSS\nQA/QC:  API 5CT / QP PK","","","","","","","-","-","PD",0,0,0,{"v":19473.5,"d":"19,473.50"}]
[1000312,"PKR,13-3/8\"X16\",SL HC,K55,7FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","ISC1333LL8079C7QMYP","Packer:  Long Rubber Element (7 ft)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC:  API 5CT / QP PK","Packer:  Long Rubber Element (7 ft)\nDiameter: 13-3/8\"\nWeight: 61#\nGrad: K-55\nConnection: SL-HC\nQA/QC:  API 5CT / QP PK","","","03","","","","-","-","PD",0,0,0,{"v":23171.86,"d":"23,171.86"}]
[1000313,"COLLAR:BFLE;DIA 13-3/8\",SL-BOSS,61#,API>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","Y01BI020133KK37473P (2-S)","COLLAR:BAFFLE;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-BOSS\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 2 STAGE\n","Baffle Collar (2-S)\n","","","","","","","COLLAR:BAFFLE;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-BOSS\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 2 STAGE\n","ZGMD_CLLR_BFLE","PD",0,0,0,{"v":4185.8,"d":"4,185.80"}]
[1000314,"COLLAR:BFLE;DIA 13-3/8\",SL-HC,61#,API 5>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","Y01BI020133KK38079P(2-S)","COLLAR:BAFFLE;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-HC\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 2 STAGE\n","Baffle Collar (2-S)\n","","","","","","","COLLAR:BAFFLE;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-HC\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 2 STAGE\n","ZGMD_CLLR_BFLE","PD",0,0,0,{"v":3969.65,"d":"3,969.65"}]
[1000315,"COLLAR:BFLE;DIA 13-3/8\",SL-BOSS,61#,API>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","Y01BI020133KK37473P(3-S)","COLLAR:BAFFLE;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-BOSS\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 3 STAGE\n","Baffle Collar (3-S)\n","","","","","","","COLLAR:BAFFLE;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-BOSS\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 3 STAGE\n","ZGMD_CLLR_BFLE","PD",0,0,0,{"v":4225.6,"d":"4,225.60"}]
[1000316,"COLLAR:BFLE;13-3/8\" X 6.5\" ID,SLHC,61#,>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","Y01BI020133KK38079P(3-S)","COLLAR:BAFFLE;\nSIZE: 13-3/8\" X 6.5\" ID\nCONNECTION A: SLHC\nWEIGHT: 61#\nGRADE: K55\nFEATURE: 3STG","Baffle Collar (3-S)\nQA/QC:  API 5CT / QP SC\nBaffle seat ID of 6.5\"","","","","","","","COLLAR:BAFFLE;\nSIZE: 13-3/8\" X 6.5\" ID\nCONNECTION A: SLHC\nWEIGHT: 61#\nGRADE: K55\nFEATURE: 3STG","ZGMD_CLLR_BFLE","PD",0,0,0,{"v":3698.18,"d":"3,698.18"}]
[1000317,"PLUG:CMT;2STG CLSG,13-3/8\",61#,16.25\",H>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","CLP133_1171-GNP-HSN","PLUG:CEMENTING;\nTYPE: 2STG CLSG\nCASING SIZE: 13-3/8\"\nCASING WEIGHT: 61#\nLENGTH: 16.25\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nOUTSIDE DIAMETER: NOSE OD 11.63\"","75D HNBR-PHENOLIC BODY\nGLASS-FILLED NYLON NOSE\nNOSE OD: 11.63\"\n\nMAXIMUM RECOMMENDED PLUG BUMP PRESSURE: 2500PSI @ 375°F\n\nPlug:   Closing plug (2S)\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4\n\nREFER ATTACHED DRAWING","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","03","","","100092539","PLUG:CEMENTING;\nTYPE: 2STG CLSG\nCASING SIZE: 13-3/8\"\nCASING WEIGHT: 61#\nLENGTH: 16.25\"\nMATERIAL: HNBR\nCORE MATERIAL: PHENOLIC\nOUTSIDE DIAMETER: NOSE OD 11.63\"","ZGMD_PLG_CMT","PD",0,0,0,819.78]
[1000318,"PLUG,CMT,3STG,13-3/8\",CLSG",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","CLP133_100Y-GNP","Plug:   Closing plug (3S)\nDiameter: 13-3/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","Plug:   Closing plug (3S)\nDiameter: 13-3/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","","","03","","","100092653","-","-","PD",0,0,0,{"v":1219.4,"d":"1,219.40"}]
[1000319,"PLUG:CMT;2STG FFOD,13-3/8\",117 LBS,PHEN>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","FFOD108_105GNP","PLUG:CEMENTING;\nTYPE: 2STG FFOD\nCASING SIZE: 13-3/8\"\nCASING WEIGHT: 117 LBS\nMATERIAL: PHENOLIC WITH STEEL SHOT\nOUTSIDE DIAMETER: SEAL OD 10.49\"","Plug:   Free-Fall Opening Plug (2S)\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","","","03","","","","PLUG:CEMENTING;\nTYPE: 2STG FFOD\nCASING SIZE: 13-3/8\"\nCASING WEIGHT: 117 LBS\nMATERIAL: PHENOLIC WITH STEEL SHOT\nOUTSIDE DIAMETER: SEAL OD 10.49\"","ZGMD_PLG_CMT","PD",0,0,0,{"v":1006.49,"d":"1,006.49"}]
[1000320,"PLUG,CMT,3STG,13-3/8\",FFOD",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","FFOD084_073L7P","Plug:   Free-Fall Opening Plug (3S)\nDiameter: 13-3/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","Plug:   Free-Fall Opening Plug (3S)\nDiameter: 13-3/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","","","","","","100092651","-","-","PD",5,0,0,{"v":1496.23,"d":"1,496.23"}]
[1000321,"PLUG,CMT,2STG,13-3/8\",SHTOFF",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","SOP133_675K2P","Plug:  First stage Shut-off Baffle Plug (2S)\nDiameter: 13-3/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","Plug:  First stage Shut-off Baffle Plug (2S)\nDiameter: 13-3/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","","","","","","","-","-","PD",0,0,0,{"v":1255.15,"d":"1,255.15"}]
[1000322,"PLUG:CMT;3STG S/O,13-3/8\",6.75\" MAX. NO>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","SOP133_675K2P","PLUG:CEMENTING;\nTYPE: 3STG SHUT OFF\nCASING SIZE: 13-3/8\"\nOUTSIDE DIAMETER: 6.75\" MAX. NOSE OD","Plug:  First stage Shut-off Baffle Plug (3S)\nDiameter: 13-3/8\"\nQA/QC:  ISO 9001-2008 / API Q1 / QPM REV 4","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","03","","","100092606","PLUG:CEMENTING;\nTYPE: 3STG SHUT OFF\nCASING SIZE: 13-3/8\"\nOUTSIDE DIAMETER: 6.75\" MAX. NOSE OD","ZGMD_PLG_CMT","PD",0,0,0,{"v":1126.52,"d":"1,126.52"}]
[1000323,"COLLAR:CMT;DIA 9-5/8\",SL-APEX,40#,API 5>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","SH20953LL7271A64SP","COLLAR:CEMENTING;\nSIZE: DIA 9-5/8\"\nCONNECTION A: SL-APEX\nWEIGHT: 40#\nSPECIFICATION: API 5CT / QP SC\nGRADE: L-80\nFEATURE: 2-S, HYDRAULIC\n","","","","","","","","COLLAR:CEMENTING;\nSIZE: DIA 9-5/8\"\nCONNECTION A: SL-APEX\nWEIGHT: 40#\nSPECIFICATION: API 5CT / QP SC\nGRADE: L-80\nFEATURE: 2-S, HYDRAULIC\n","ZGMD_CLLR_CMT","PD",0,0,0,{"v":6151.2,"d":"6,151.20"}]
[1000324,"COLLAR:CMT;DIA 13-3/8\",SL-BOSS,61#,API >",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","SM21333KX7473A23SP","COLLAR:CEMENTING;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-BOSS\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 2-S, MECHANICAL PLUG BASED\n","","","","","","","","COLLAR:CEMENTING;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-BOSS\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 2-S, MECHANICAL PLUG BASED\n","ZGMD_CLLR_CMT","PD",0,0,0,{"v":7631.75,"d":"7,631.75"}]
[1000325,"COLLAR:CMT;D 13-3/8\",SL-HC,61#,API 5CT,>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","SM21333KX8079A23SP","COLLAR:CEMENTING;\nSIZE: DIAMETER 13-3/8\"\nCONNECTION A: SL-HC\nWEIGHT: 61#\nSPECIFICATION: API 5CT\nGRADE: K55\nFEATURE: 2-S, MECHANICAL PLUG BASED","","","","","","","","COLLAR:CEMENTING;\nSIZE: DIAMETER 13-3/8\"\nCONNECTION A: SL-HC\nWEIGHT: 61#\nSPECIFICATION: API 5CT\nGRADE: K55\nFEATURE: 2-S, MECHANICAL PLUG BASED","ZGMD_CLLR_CMT","PD",0,0,0,{"v":7715.35,"d":"7,715.35"}]
[1000326,"COLLAR:CMT;DIA 13-3/8\",SL-BOSS,61#,API >",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","SM31333KX7473A23SP","COLLAR:CEMENTING;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-BOSS\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 3-S, MECHANICAL PLUG BASED\n","","","","","","","","COLLAR:CEMENTING;\nSIZE: DIA 13-3/8\"\nCONNECTION A: SL-BOSS\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: K-55\nFEATURE: 3-S, MECHANICAL PLUG BASED\n","ZGMD_CLLR_CMT","PD",0,0,0,{"v":7674.15,"d":"7,674.15"}]
[1000327,"COLLAR:CMT;D 13-3/8\",SL-HC,61#,API 5CT/>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","SM31333KK8079A23SP","COLLAR:CEMENTING;\nSIZE: DIAMETER 13-3/8\"\nCONNECTION TYPE A: SL-HC\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: L80\nFEATURE: 3-S, MECHANICAL PLUG BASED","","","","","","","","COLLAR:CEMENTING;\nSIZE: DIAMETER 13-3/8\"\nCONNECTION TYPE A: SL-HC\nWEIGHT: 61#\nSPECIFICATION: API 5CT / QP SC\nGRADE: L80\nFEATURE: 3-S, MECHANICAL PLUG BASED","ZGMD_CLLR_CMT","PD",4,0,0,{"v":7986.36,"d":"7,986.36"}]
[1000330,"PKR:SWELL;3.5\" X 5.8\",SLAPX,3.5\" X 5.8\">",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-101","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: OIL\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","SWELL PACKER: OIL\n3.5\" x 5.8\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: OIL\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":3801.11,"d":"3,801.11"}]
[1000331,"PKR:SWELL;3.5\" X 5.8\",SLHT,B X P,5.8\",6>",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-102","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nCONNECTION TYPE: B X P\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: OIL\nELASTOMERS: SWELLRIGHT\nMATERIAL: L80 13%CR\nGRADE: L80 13%CR\n","SWELL PACKER: OIL\n3.5\" x 5.8\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nCONNECTION TYPE: B X P\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: OIL\nELASTOMERS: SWELLRIGHT\nMATERIAL: L80 13%CR\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":4868.74,"d":"4,868.74"}]
[1000332,"PKR:SWELL;3.5\" X 5.8\",SLAPX,3.5\" X 5.8\">",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-103","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: OIL\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","SWELL PACKER: OIL\n3.5\" x 5.8\" x 6ft Oil SwellRight FeedThru L80 1%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: OIL\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":5421.54,"d":"5,421.54"}]
[1000333,"PKR:SWELL;3.5\" X 5.8\",SLAPX,5.8\",6FT,OI>",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-104","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: OIL\nELASTOMERS: SWELLRIGHT FEEDTHRU\nGRADE: L80 13%CR\n","SWELL PACKER: OIL\n3.5\" x 5.8\" x 6ft Oil SwellRight FeedThru L80 13%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: OIL\nELASTOMERS: SWELLRIGHT FEEDTHRU\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":6489.59,"d":"6,489.59"}]
[1000334,"PKR,SWELL,4.5\"x5.8\",SLHT,1CR,BXP,OIL",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-101","PACKER: OIL\n3.5\" x 5.8\" x 6ft Oil SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n4.5\"\" x 5.8\"\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":3814.65,"d":"3,814.65"}]
[1000335,"PKR,SWELL,4.5\"x5.8\",SLHT,13CR,BXP,OIL",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-102","PACKER: OIL\n4.5\" x 5.8\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n4.5\"\" x 5.8\"\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":4386.57,"d":"4,386.57"}]
[1000336,"PKR,SWELL,4.5\"x5.8\",SLHT,1CR,FeeTh,OIL",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-103","PACKER: OIL\n4.5\" x 5.8\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n4.5\"\" x 5.8\"\" x 6ft Oil SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":5509.74,"d":"5,509.74"}]
[1000337,"PKR,SWELL,4.5\"x5.8\",SLHT,13CR,FeTh,OIL",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-104","PACKER: OIL\n4.5\" x 5.8\" x 6ft Oil SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n4.5\"\" x 5.8\"\" x 6ft Oil SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":6081.67,"d":"6,081.67"}]
[1000338,"PKR,SWELL,4.5\"x8.2\",SLHT,1CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-105","PACKER: OIL\n4.5\" x 5.8\" x 6ft Oil SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n4.5\"\" x 8.2\"\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":5068.59,"d":"5,068.59"}]
[1000339,"PKR,SWELL,4.5\"x8.2\",SLHT,13CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-106","PACKER: OIL\n4.5\" x 8.2\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n4.5\"\" x 8.2\"\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":5640.88,"d":"5,640.88"}]
[1000340,"PKR,SWELL,4.5\"x8.2\",SLHT,FeTh,1CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-107","PACKER: OIL\n4.5\" x 8.2\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n4.5\"\" x 8.2\"\" x 6ft Oil SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":5906.64,"d":"5,906.64"}]
[1000341,"PKR,SWELL,4.5\"x8.2\",SLHT,FeTh,13CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-108","PACKER: OIL\n4.5\" x 8.2\" x 6ft Oil SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n4.5\"\" x 8.2\"\" x 6ft Oil SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":6478.57,"d":"6,478.57"}]
[1000342,"PKR,SWELL,5.5\"x8.2\",SLHT,1CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-05500-NOC-101","PACKER: OIL\n4.5\" x 8.2\" x 6ft Oil SwellRight FeedThru L80 13%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n5.5\"\" x 8.2\"\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 5.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":4498,"d":"4,498.00"}]
[1000343,"PKR,SWELL,5.5\"x8.2\",SLHT,13CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-05500-NOC-102","PACKER: OIL\n5.5\" x 8.2\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n5.5\"\" x 8.2\"\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 5.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":7116.85,"d":"7,116.85"}]
[1000344,"PKR,SWELL,7\"x8.2\",SLHT,1CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-07000-NOC-101","PACKER: OIL\n5.5\" x 8.2\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 7.0\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n7.0\"\" x 8.2\"\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 7.0\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":4894.7,"d":"4,894.70"}]
[1000345,"PKR,SWELL,7\"x8.2\",SLHT,13CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-07000-NOC-102","PACKER: OIL\n7.0\" x 8.2\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 7.0\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n7.0\"\" x 8.2\"\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 7.0\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":8636.6,"d":"8,636.60"}]
[1000346,"PKR,SWELL,3.5\"x8.2\",SLHT,13CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-106","PACKER: OIL\n7.0\" x 8.2\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 3.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n3.5\"\" x 8.2\"\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 3.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":3543.75,"d":"3,543.75"}]
[1000347,"PKR,SWELL,3.5\"x8.2\",SLHT,1CR,OIL",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-105","PACKER: OIL\n3.5\" x 8.2\" x 6ft Oil SwellRight L80 13%Cr\nDiameter: 3.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL\n3.5\"\" x 8.2\"\" x 6ft Oil SwellRight L80 1%Cr\nDiameter: 3.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":3228.75,"d":"3,228.75"}]
[1000348,"PKR:SWELL;3.5\" X 5.8\",SLAPX,3.5\" X 5.8\">",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-201","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","SWELL PACKER: WATER\n3.5\" x 5.8\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":4554.42,"d":"4,554.42"}]
[1000349,"PKR:SWELL;3.5\" X 5.8\",SLAPX,BXP,5.8\",6F>",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-202","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nCONNECTION TYPE: BXP\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","SWELL PACKER: WATER\n3.5\" x 5.8\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nCONNECTION TYPE: BXP\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":5623.19,"d":"5,623.19"}]
[1000350,"PKR:SWELL;3.5\" X 5.8\",SLAPX,3.5\" X 5.8\">",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-203","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","SWELL PACKER: WATER\n3.5\" x 5.8\" x 6ft Water SwellRight FeedThru L80 1%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":6175.38,"d":"6,175.38"}]
[1000351,"PKR:SWELL;3.5\" X 5.8\",SLHT,5.8\",6FT,WTR>",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-204","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: WATER\nELASTOMERS: SWELLRIGHT FEEDTHRU\nGRADE: L80 13%CR\n","SWELL PACKER: WATER\n3.5\"\" x 5.8\"\" x 6ft Water SwellRight FeedThru L80 13%Cr\nDiameter: 3.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: WATER\nELASTOMERS: SWELLRIGHT FEEDTHRU\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":7243.43,"d":"7,243.43"}]
[1000352,"PKR,SWELL,4.5\"x5.8\",SLHT,1CR,BXP,W",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-201","PACKER: WATER\n3.5\" x 5.8\" x 6ft Water SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n4.5\"\" x 5.8\"\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":4339.72,"d":"4,339.72"}]
[1000353,"PKR,SWELL,4.5\"x5.8\",SLHT,13CR,BXP,W",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-202","PACKER: WATER\n4.5\" x 5.8\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n4.5\"\" x 5.8\"\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":4911.64,"d":"4,911.64"}]
[1000354,"PKR,SWELL,4.5\"x5.8\",SLHT,1CR,FeeTh,W",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-203","PACKER: WATER\n4.5\" x 5.8\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n4.5\"\" x 5.8\"\" x 6ft Water SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":6034.81,"d":"6,034.81"}]
[1000355,"PKR,SWELL,4.5\"x5.8\",SLHT,13CR,FeTh,W",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-204","PACKER: WATER\n4.5\" x 5.8\" x 6ft Water SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n4.5\"\" x 5.8\"\" x 6ft Water SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":6606.73,"d":"6,606.73"}]
[1000356,"PKR,SWELL,4.5\"x8.2\",SLHT,1CR,W",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-205","PACKER: WATER\n4.5\" x 5.8\" x 6ft Water SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n4.5\"\" x 8.2\"\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":6609.59,"d":"6,609.59"}]
[1000357,"PKR,SWELL,4.5\"x8.2\",SLHT,13CR,W",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-206","PACKER: WATER\n4.5\" x 8.2\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n4.5\"\" x 8.2\"\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":7181.06,"d":"7,181.06"}]
[1000358,"PKR,SWELL,4.5\"x8.2\",SLHT,FeTh,1CR,W",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-207","PACKER: WATER\n4.5\" x 8.2\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n4.5\"\" x 8.2\"\" x 6ft Water SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":7447.39,"d":"7,447.39"}]
[1000359,"PKR,SWELL,4.5\"x8.2\",SLHT,FeTh,13CR,W",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-208","PACKER: WATER\n4.5\" x 8.2\" x 6ft Water SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n4.5\"\" x 8.2\"\" x 6ft Water SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":8019.31,"d":"8,019.31"}]
[1000360,"PKR,SWELL,5.5\"x8.2\",SLHT,1CR,W",null,null,"EA","COM","4000248","TENDEKA","001-05500-NOC-201","PACKER: WATER\n4.5\" x 8.2\" x 6ft Water SwellRight FeedThru L80 13%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n5.5\"\" x 8.2\"\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 5.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":5738.02,"d":"5,738.02"}]
[1000361,"PKR,SWELL,5.5\"x8.2\",SLHT,13CR,W",null,null,"EA","COM","4000248","TENDEKA","001-05500-NOC-202","PACKER: WATER\n5.5\" x 8.2\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n5.5\"\" x 8.2\"\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 5.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":8356.7,"d":"8,356.70"}]
[1000362,"PKR,SWELL,7\"x8.2\",SLHT,1CR,W",null,null,"EA","COM","4000248","TENDEKA","001-07000-NOC-201","PACKER: WATER\n5.5\" x 8.2\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 7.0\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n7.0\"\" x 8.2\"\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 7.0\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":5611.5,"d":"5,611.50"}]
[1000363,"PKR,SWELL,7\"x8.2\",SLHT,13CR,W",null,null,"EA","COM","4000248","TENDEKA","001-07000-NOC-202","PACKER: WATER\n7.0\" x 8.2\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 7.0\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n7.0\"\" x 8.2\"\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 7.0\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":9352.74,"d":"9,352.74"}]
[1000364,"PKR,SWELL,3.5\"x8.2\",SLHT,13CR,W",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-206","PACKER: WATER\n7.0\" x 8.2\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 3.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n3.5\"\" x 8.2\"\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 3.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":4016.25,"d":"4,016.25"}]
[1000365,"PKR,SWELL,3.5\"x8.2\",SLHT,1CR,W",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-205","PACKER: WATER\n3.5\" x 8.2\" x 6ft Water SwellRight L80 13%Cr\nDiameter: 3.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: WATER\n3.5\"\" x 8.2\"\" x 6ft Water SwellRight L80 1%Cr\nDiameter: 3.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":3257.63,"d":"3,257.63"}]
[1000366,"PKR:SWELL;3.5\" X 5.8\",SLHT,3.5\" X 5.8\",>",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-301","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: HYBRID\nELASTOMERS: SWELLRIGHT\nGRADE: L80 1%CR\n","SWELL PACKER: HYBRID\n3.5\"\" x 5.8\"\" x 6ft Hybrid SwellRight L80 1%Cr\nDiameter: 3.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: HYBRID\nELASTOMERS: SWELLRIGHT\nGRADE: L80 1%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":4212.93,"d":"4,212.93"}]
[1000367,"PKR:SWELL;3.5\" X 5.8\",SLAPX,5.8\",6FT,HY>",null,null,"EA","COM","4000248","TENDEKA","001-03500-NOC-302","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: HYBRID\nELASTOMERS: SWELLRIGHT FEEDTHRU\nGRADE: L80 13%CR\n","SWELL PACKER: HYBRID\n3.5\" x 5.8\" x 6ft Hybrid SwellRight L80 13%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT\nREACTIVE MEDIUM: HYBRID\nELASTOMERS: SWELLRIGHT FEEDTHRU\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":5280.98,"d":"5,280.98"}]
[1000368,"PKR,SWELL,4.5\"x5.8\",SLHT,1CR,HYBR",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-301","PACKER: HYBRID\n3.5\" x 5.8\" x 6ft Hybrid SwellRight L80 13%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: HYBRID\n4.5\"\" x 5.8\"\" x 6ft Hybrid SwellRight L80 1%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":4104.06,"d":"4,104.06"}]
[1000369,"PKR,SWELL,4.5\"x5.8\",SLHT,13CR,HYBR",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-302","PACKER: HYBRID\n4.5\" x 5.8\" x 6ft Hybrid SwellRight L80 1%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: HYBRID\n4.5\"\" x 5.8\"\" x 6ft Hybrid SwellRight L80 13%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":4675.98,"d":"4,675.98"}]
[1000370,"PKR,SWELL,4.5\"x8.2\",SLHT,1CR,HYBR",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-303","PACKER: HYBRID\n4.5\" x 5.8\" x 6ft Hybrid SwellRight L80 13%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: HYBRID\n4.5\"\" x 8.2\"\" x 6ft Hybrid SwellRight L80 1%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":5908.02,"d":"5,908.02"}]
[1000371,"PKR,SWELL,4.5\"x8.2\",SLHT,13CR,HYBR",null,null,"EA","COM","4000248","TENDEKA","001-04500-NOC-304","PACKER: HYBRID\n4.5\" x 8.2\" x 6ft Hybrid SwellRight L80 1%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: HYBRID\n4.5\"\" x 8.2\"\" x 6ft Hybrid SwellRight L80 13%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":6479.94,"d":"6,479.94"}]
[1000372,"PKR,SWELL,5.5\"x8.2\",SLHT,1CR,HYBR",null,null,"EA","COM","4000248","TENDEKA","001-05500-NOC-301","PACKER: HYBRID\n4.5\" x 8.2\" x 6ft Hybrid SwellRight L80 13%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: HYBRID\n5.5\"\" x 8.2\"\" x 6ft Hybrid SwellRight L80 1%Cr\nDiameter: 5.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":5114.22,"d":"5,114.22"}]
[1000373,"PKR,SWELL,5.5\"x8.2\",SLHT,13CR,HYBR",null,null,"EA","COM","4000248","TENDEKA","001-05500-NOC-302","PACKER: HYBRID\n5.5\" x 8.2\" x 6ft Hybrid SwellRight L80 1%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: HYBRID\n5.5\"\" x 8.2\"\" x 6ft Hybrid SwellRight L80 13%Cr\nDiameter: 5.5\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":7732.66,"d":"7,732.66"}]
[1000374,"PKR,SWELL,7\"x8.2\",SLHT,1CR,HYBR",null,null,"EA","COM","4000248","TENDEKA","001-07000-NOC-301","PACKER: HYBRID\n5.5\" x 8.2\" x 6ft Hybrid SwellRight L80 13%Cr\nDiameter: 7.0\" x 8.2\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: HYBRID\n7.0\"\" x 8.2\"\" x 6ft Hybrid SwellRight L80 1%Cr\nDiameter: 7.0\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":5232.74,"d":"5,232.74"}]
[1000375,"PKR,SWELL,7\"x8.2\",SLHT,13CR,HYBR",null,null,"EA","COM","4000248","TENDEKA","001-07000-NOC-302","PACKER: HYBRID\n7.0\" x 8.2\" x 6ft Hybrid SwellRight L80 1%Cr\nDiameter: 7.0\" x 8.2\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: HYBRID\n7.0\"\" x 8.2\"\" x 6ft Hybrid SwellRight L80 13%Cr\nDiameter: 7.0\"\" x 8.2\"\"\nElement Length: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":8974.35,"d":"8,974.35"}]
[1000376,"PKR:SWELL;7.0\" X 8.2\",SLAPX,3.5\" X 5.8\">",null,null,"EA","COM","4000248","TENDEKA","009-03500-NOC-401","PACKER:SWELL;\nSIZE: 7.0\" X 8.2\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","SWELL PACKER: OIL<(>&<)>WATER\n3.5\" x 5.8\" x 6+6 ft Water + Oil SwellRight L80 1%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 7.0\" X 8.2\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":6211.36,"d":"6,211.36"}]
[1000377,"PKR:SWELL;3.5\" X 5.8\",SLHT,5.8\",6FT+6FT>",null,null,"EA","COM","4000248","TENDEKA","009-03500-NOC-402","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT+6FT\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT\nMATERIAL: L80-13%CR\nSEALING ELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\n","SWELL PACKER: OIL<(>&<)>WATER\n3.5\" x 5.8\" x 6+6 ft Water + Oil SwellRight L80 13%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT+6FT\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT\nMATERIAL: L80-13%CR\nSEALING ELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":6729.77,"d":"6,729.77"}]
[1000378,"PKR:SWELL;3.5\" X 5.8\",SLAPX,3.5\" X 5.8\">",null,null,"EA","COM","4000248","TENDEKA","009-03500-NOC-403","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","SWELL PACKER: OIL<(>&<)>WATER\n3.5\" x 5.8\" x 6+6 ft Water + Oil SwellRight FeedThru L80 1%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 3.5\" X 5.8\"\nELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":8509.92,"d":"8,509.92"}]
[1000379,"PKR:SWELL;3.5\" X 5.8\",SLAPX,5.8\",6FT(OI>",null,null,"EA","COM","4000248","TENDEKA","009-03500-NOC-404","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT FEEDTHRU\nMATERIAL: L80 13%CR\nGRADE: L80 13%CR\n","SWELL PACKER: OIL<(>&<)>WATER\n3.5\" x 5.8\" x 6+6 ft Water + Oil SwellRight FeedThru L80 13%Cr\nDiameter: 3.5\"x5.8\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLAPX\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT FEEDTHRU\nMATERIAL: L80 13%CR\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":9028.1,"d":"9,028.10"}]
[1000380,"PKR:SWELL;3.5\" X 5.8\",SLHT,5.8\",6FT(OIL>",null,null,"EA","COM","4000248","TENDEKA","009-04500-NOC-401","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT FEEDTHRU\nGRADE: L80 13%CR\n","SWELL PACKER: OIL<(>&<)>WATER\n3.5\" x 5.8\" x 6+6 ft Water + Oil SwellRight FeedThru L80 13%Cr\nDiameter: 3.5\" x 5.8\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","PACKER:SWELL;\nSIZE: 3.5\" X 5.8\"\nCONNECTION: SLHT\nOUTSIDE DIAMETER: 5.8\"\nELEMENT LENGTH: 6FT(OIL) + 6FT(WATER)\nREACTIVE MEDIUM: OIL+WATER\nELASTOMERS: SWELLRIGHT FEEDTHRU\nGRADE: L80 13%CR\n","ZGMD_PCKR_SWELL","PD",0,0,0,{"v":5808.8,"d":"5,808.80"}]
[1000381,"PKR,SWELL,4.5\"x5.8\",SLHT,13CR,6+6,O+W",null,null,"EA","COM","4000248","TENDEKA","009-04500-NOC-402","PACKER: OIL&WATER\n4.5\" x 5.8\" x 6+6 ft Water + Oil SwellRight L80 1%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n4.5\"\" x 5.8\"\" x 6+6 ft Water + Oil SwellRight L80 13%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":5643.42,"d":"5,643.42"}]
[1000382,"PKR,SWELL,4.5\"x5.8\",SLHT,1CR,FeTh,O+W",null,null,"EA","COM","4000248","TENDEKA","009-04500-NOC-403","PACKER: OIL&WATER\n4.5\" x 5.8\" x 6+6 ft Water + Oil SwellRight L80 13%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n4.5\"\" x 5.8\"\" x 6+6 ft Water + Oil SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":8678.05,"d":"8,678.05"}]
[1000383,"PKR,SWELL,4.5\"x5.8\",SLHT,13CR,FeTh,O+W",null,null,"EA","COM","4000248","TENDEKA","009-04500-NOC-404","PACKER: OIL&WATER\n4.5\" x 5.8\" x 6+6 ft Water + Oil SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\" x 5.8\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n4.5\"\" x 5.8\"\" x 6+6 ft Water + Oil SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\"\" x 5.8\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":8512.68,"d":"8,512.68"}]
[1000384,"PKR,SWELL,4.5\"x8.2\",SLHT,1CR,6+6,O+W",null,null,"EA","COM","4000248","TENDEKA","009-04500-NOC-405","PACKER: OIL&WATER\n4.5\" x 5.8\" x 6+6 ft Water + Oil SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n4.5\"\" x 8.2\"\" x 6+6 ft Water + Oil SwellRight L80 1%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":9011.78,"d":"9,011.78"}]
[1000385,"PKR,SWELL,4.5\"x8.2\",SLHT,13CR,6+6,O+W",null,null,"EA","COM","4000248","TENDEKA","009-04500-NOC-406","PACKER: OIL&WATER\n4.5\" x 8.2\" x 6+6 ft Water + Oil SwellRight L80 1%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n4.5\"\" x 8.2\"\" x 6+6 ft Water + Oil SwellRight L80 13%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":8846.25,"d":"8,846.25"}]
[1000386,"PKR,SWELL,4.5\"x8.2\",SLHT,1CR,FeTh,O+W",null,null,"EA","COM","4000248","TENDEKA","009-04500-NOC-407","PACKER: OIL&WATER\n4.5\" x 8.2\" x 6+6 ft Water + Oil SwellRight L80 13%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n4.5\"\" x 8.2\"\" x 6+6 ft Water + Oil SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","","","","","-","-","PD",0,0,0,{"v":11562.47,"d":"11,562.47"}]
[1000387,"PKR,SWELL,4.5\"x8.2\",SLHT,13CR,FeTh,O+W",null,null,"EA","COM","4000248","TENDEKA","009-04500-NOC-408","PACKER: OIL&WATER\n4.5\" x 8.2\" x 6+6 ft Water + Oil SwellRight FeedThru L80 1%Cr\nDiameter: 4.5\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n4.5\"\" x 8.2\"\" x 6+6 ft Water + Oil SwellRight FeedThru L80 13%Cr\nDiameter: 4.5\"\" x 8.2\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":11397.09,"d":"11,397.09"}]
[1000388,"(BLCK)PKR,SWELL,5.5\"x8.2\",SLHT,1CR,6+6,O",null,null,"EA","COM","4000248","TENDEKA","009-05500-NOC-401","PACKER: OIL&WATER\n4.5\" x 8.2\" x 6+6 ft Water + Oil SwellRight FeedThru L80 13%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n5.5\" x 8.2\" x 6+6 ft Water + Oil SwellRight L80 1%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","06","","1047211","","-","-","PD",0,0,0,{"v":7751.16,"d":"7,751.16"}]
[1000389,"(BLCK)PKR,SWELL,5.5\"x8.2\",SLHT,13CR,6+6",null,null,"EA","COM","4000248","TENDEKA","009-05500-NOC-402","PACKER: OIL&WATER\n5.5\" x 8.2\" x 6+6 ft Water + Oil SwellRight L80 1%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n5.5\" x 8.2\" x 6+6 ft Water + Oil SwellRight L80 13%Cr\nDiameter: 5.5\" x 8.2\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3\n","","","06","","1047210","","-","-","PD",0,0,0,{"v":9584.16,"d":"9,584.16"}]
[1000390,"PKR,SWELL,7\"x8.2\",SLHT,1CR,6+6,O+W",null,null,"EA","COM","4000248","TENDEKA","009-07000-NOC-401","PACKER: OIL&WATER\n5.5\" x 8.2\" x 6+6 ft Water + Oil SwellRight L80 13%Cr\nDiameter: 7.0\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n7.0\"\" x 8.2\"\" x 6+6 ft Water + Oil SwellRight L80 1%Cr\nDiameter: 7.0\"\" x 8.2\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":7101.85,"d":"7,101.85"}]
[1000391,"PKR,SWELL,7\"x8.2\",SLHT,13CR,6+6,O+W",null,null,"EA","COM","4000248","TENDEKA","009-07000-NOC-402","PACKER: OIL&WATER\n7.0\" x 8.2\" x 6+6 ft Water + Oil SwellRight L80 1%Cr\nDiameter: 7.0\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n7.0\"\" x 8.2\"\" x 6+6 ft Water + Oil SwellRight L80 13%Cr\nDiameter: 7.0\"\" x 8.2\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":10509.89,"d":"10,509.89"}]
[1000392,"PKR,SWELL,3.5\"x8.2\",SLHT,13CR,6+6,O+W",null,null,"EA","COM","4000248","TENDEKA","009-03500-NOC-406","PACKER: OIL&WATER\n7.0\" x 8.2\" x 6+6 ft Water + Oil SwellRight L80 13%Cr\nDiameter: 3.5\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n3.5\"\" x 8.2\"\" x 6ft Combo (O+W) SwellRight L80 13%Cr\nDiameter: 3.5\"\" x 8.2\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 13%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":6013.28,"d":"6,013.28"}]
[1000393,"PKR,SWELL,3.5\"x8.2\",SLHT,1CR,6+6,O+W",null,null,"EA","COM","4000248","TENDEKA","009-03500-NOC-405","PACKER: OIL&WATER\n3.5\" x 8.2\" x 6ft Combo (O+W) SwellRight L80 13%Cr\nDiameter: 3.5\" x 8.2\"\nElement Length Oil: 6ft & Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLAPX\nQA/QC: As per contract appendix 3","SWELL PACKER: OIL<(>&<)>WATER\n3.5\"\" x 8.2\"\" x 6ft Combo (O+W) SwellRight L80 1%Cr\nDiameter: 3.5\"\" x 8.2\"\"\nElement Length Oil: 6ft <(>&<)> Element Length Water: 6ft\nGrade: L80 1%Cr\nConnection: SLHT\nQA/QC: As per contract appendix 3","","","","","","","-","-","PD",0,0,0,{"v":5794.38,"d":"5,794.38"}]
[1000394,"XMT:SGL,5-1/8\",5000 PSI,13-5/8\" VG-137 >",null,null,"EA","XMT","4000005","GE-VETCO / UK","H424407-1","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 5-1/8\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13-5/8\" VG-137 ST NT2 BOX DOWN\nTRIM: HH-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (PSL-3G UPON ASSEMBLY)\nMATERIAL SPECIFICATION: CRA CLAD, ISO 15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: NOC-SD-COR-355 / VGS 6.1.27\nTREE CAP DESCRIPTION: 6GR52 HUB W/ 9/16\" HP PORT\nSWAB VALVE DESCRIPTION: 5-1/8” MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 5-1/8” SPLIT GATE (CSWC ACT)\nKILL VALVE DESCRIPTION: 2-1/6\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 5-1/8” SPLIT GATE (CSWC ACT)\nLOWER MASTER VALVE (LMV): 5-1/8” MANUAL SPLIT GATE\nTEE DESCRIPTION: 5-1/8\" TEE F/ FLOW WING\nSERVICE: H2S","ASSEMBLED AS PER DWG H424407\nTESTING AND MARKING PROCEDURE AS PER ENGINEERING PART SPECIFICATION\nH424407-1.\nUMV IS NON-WIRELINE SHEARING SPLIT GATE VALVE.\n\n(See attached drawing,BOM)","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nDATA BOOK\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 5-1/8\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13-5/8\" VG-137 ST NT2 BOX DOWN\nTRIM: HH-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (PSL-3G UPON ASSEMBLY)\nMATERIAL SPECIFICATION: CRA CLAD, ISO 15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: NOC-SD-COR-355 / VGS 6.1.27\nTREE CAP DESCRIPTION: 6GR52 HUB W/ 9/16\" HP PORT\nSWAB VALVE DESCRIPTION: 5-1/8” MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 5-1/8” SPLIT GATE (CSWC ACT)\nKILL VALVE DESCRIPTION: 2-1/6\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 5-1/8” SPLIT GATE (CSWC ACT)\nLOWER MASTER VALVE (LMV): 5-1/8” MANUAL SPLIT GATE\nTEE DESCRIPTION: 5-1/8\" TEE F/ FLOW WING\nSERVICE: H2S","ZGMD_XMT_NM","PD",0,0,0,{"v":359413.5,"d":"359,413.50"}]
[1000395,"XMT:SGL,5-1/8\",5000 PSI,13-5/8\" VG-137 >",null,null,"EA","XMT","4000005","GE-VETCO / UK","R148127-91","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 5-1/8\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13-5/8\" VG-137 ST NT2 BOX DOWN\nTRIM: EE-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nMATERIAL SPECIFICATION: PARTIAL CLAD ON SEAL FACES\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: NOC-SD-COR-355 / VGS 6.1.27\nTREE CAP DESCRIPTION: 6GR52 HUB C/W 1/2\" NPT\nSWAB VALVE DESCRIPTION: 5-1/8” MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 5-1/8” SPLIT GATE (CSWC ACT)\nKILL VALVE DESCRIPTION: 2-1/16\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 5-1/8” WLS SPLIT GATE CSWC ACT\nLOWER MASTER VALVE (LMV): 4-1/8” MANUAL SPLIT GATE\nTEE DESCRIPTION: 5-1/8\" TEE F/ FLOW WING\nSERVICE: H2S","ASSEMBLY, TESTING AND MARKING PROCEDURE AS PER ENGINEERING PART\nSPECIFICATION R148127-91.\nUMV IS WIRELINE SHEARING SPLIT GATE VALVE.\nNT2 BOLTS WITH UPDATED DESIGN HAVING EXTERNAL HEX PROFILE.\n\n(See attached BOM)","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nDATA BOOK\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","100071072","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 5-1/8\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13-5/8\" VG-137 ST NT2 BOX DOWN\nTRIM: EE-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nMATERIAL SPECIFICATION: PARTIAL CLAD ON SEAL FACES\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: NOC-SD-COR-355 / VGS 6.1.27\nTREE CAP DESCRIPTION: 6GR52 HUB C/W 1/2\" NPT\nSWAB VALVE DESCRIPTION: 5-1/8” MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 5-1/8” SPLIT GATE (CSWC ACT)\nKILL VALVE DESCRIPTION: 2-1/16\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 5-1/8” WLS SPLIT GATE CSWC ACT\nLOWER MASTER VALVE (LMV): 4-1/8” MANUAL SPLIT GATE\nTEE DESCRIPTION: 5-1/8\" TEE F/ FLOW WING\nSERVICE: H2S","ZGMD_XMT_NM","PD",0,0,0,{"v":266399.95,"d":"266,399.95"}]
[1000396,"HANGER:TBG;13-5/8\" X 5-1/2\",MS-NT,5000 >",null,null,"EA","DRL","4000005","GE-VETCO / UK","R116602-12","HANGER:TUBING;\nBOWL SIZE X CASING/TUBING SIZE: 13-5/8\" X 5-1/2\"\nPROFILE: MS-NT\nPRESSURE RATING: 5000 PSI\nTRIM: HH-NL\nTEMPERATURE RATING: U\nINSIDE DIAMETER: 4.875\"\nOUTSIDE DIAMETER: 13.430\"\nTOP SIZE/CONNECTION: 8-4TPI LH STUB ACME PIN TOP\nBOTTOM SIZE/CONNECTION: 5.5\" 15.5# SL APEX BOX BTM\nHANGER NECK SIZE: 7-3/4\" FOR CB-T SEAL\nFLOW BY AREA:\nMAX FLOW BY PARTICLE SIZE:\nCONTROL LINE FEEDTHROUGH: 7 X 1/4\" OD CONTROL LINES\nBPV PREPARATION: 4.875 CRQ PETROLINE PREP\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2\nMATERIAL: INC 718 BODY - INC 825 CB-T\nMATERIAL SPECIFICATION: 120 KSI\nCOATING:\nSPECIFICATION: API 6A\nSERVICE: H2S\nTYPE: FOR GEN-5 MS-T SEAL\nSTYLE: MS-NT\nADDITIONAL INFORMATION: C/W CB-T SEAL PARTS","5-1/2\" TUBING HANGER ASSEMBLED AS PER DRAWING NUMBER R116602-5 AND BILL\nOF MATERIAL PART NUMBER R116602-12\n\n(See attached)","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nDATA BOOK\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","HANGER:TUBING;\nBOWL SIZE X CASING/TUBING SIZE: 13-5/8\" X 5-1/2\"\nPROFILE: MS-NT\nPRESSURE RATING: 5000 PSI\nTRIM: HH-NL\nTEMPERATURE RATING: U\nINSIDE DIAMETER: 4.875\"\nOUTSIDE DIAMETER: 13.430\"\nTOP SIZE/CONNECTION: 8-4TPI LH STUB ACME PIN TOP\nBOTTOM SIZE/CONNECTION: 5.5\" 15.5# SL APEX BOX BTM\nHANGER NECK SIZE: 7-3/4\" FOR CB-T SEAL\nFLOW BY AREA:\nMAX FLOW BY PARTICLE SIZE:\nCONTROL LINE FEEDTHROUGH: 7 X 1/4\" OD CONTROL LINES\nBPV PREPARATION: 4.875 CRQ PETROLINE PREP\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2\nMATERIAL: INC 718 BODY - INC 825 CB-T\nMATERIAL SPECIFICATION: 120 KSI\nCOATING:\nSPECIFICATION: API 6A\nSERVICE: H2S\nTYPE: FOR GEN-5 MS-T SEAL\nSTYLE: MS-NT\nADDITIONAL INFORMATION: C/W CB-T SEAL PARTS","ZGMD_HGR_TBG","PD",0,0,0,{"v":79654.65,"d":"79,654.65"}]
[1000397,"WH,UNITIZED CONTINGENCY,13-5/8\"",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-501798-02-S0636","","Wellhead:\nWH,UNITIZED CONTINGENCY,13-5/8\"\nManufacturer part#6-501798-02-S0636\n","","","","","","","-","-","PD",0,0,0,{"v":42692,"d":"42,692.00"}]
[1000398,"WH,UNITIZED CONTINGENCY,13-5/8\",502676",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-502676-02","","Wellhead:\nWH,UNITIZED CONTINGENCY,13-5/8\"\nManufacturer part#6-502676-02\n13.62\",ASSEMBLY,CONTINGEN:ASSS UWS, ASSEMBLY, CONTINGENCY HOUSING,\n13.62\", 5,000 PSI, TYPE SU-902, API 6A, U, DD-NL, PSL-2, PR2, C/W ONE\n(1) OFF 2.06\" MANUAL GATE VALVE AND ONE (1) OFF BLIND FLANGE, SPECIAL,\nW/ EIGHT (8) OFF CONTROL LINE OUTLETS\n","","","","","","","-","-","PD",0,0,0,{"v":52618,"d":"52,618.00"}]
[1000399,"(BLCK)SEE 100086918,TBG,HANGER 13-5/",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-502446-02-S1351","","TUBING HANGER\nTBG,HANGER 13-5/8\",FF TRIM\nManufacturer part#6-502446-02-S1351","","","06","","","","-","-","PD",0,0,0,{"v":14803,"d":"14,803.00"}]
[1000400,"TBG,HANGER 13-5/8\",HH TRIM",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-502623-02","","TUBING HANGER\nTBG,HANGER 13-5/8\",HH TRIM\nTubing Hanger, 4-1/2\", 12.6# SL Apex Box down, w/ 8 off 1/4\" down-hole\ncontrol line ports, w/ 3.875\" QN petroline plug profile.\n","","","","","","","-","-","PD",0,0,0,{"v":24238.83,"d":"24,238.83"}]
[1000401,"XMT:SGL,4.06\",5000 PSI,13.625\" 10000 PS>",null,null,"EA","XMT","4000003","DRIL-QUIP / SINGAPORE","6-502624-02","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 4.06\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13.625\" 10000 PSI RBC DOWN\nTRIM: HH-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nMATERIAL SPECIFICATION: NACE, ISO-15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: SD-NOC-COR-355, 356\nTREE CAP DESCRIPTION: 6GR52 W/ 0.5\" NPT PLUG\nSWAB VALVE DESCRIPTION: 4.06\" MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 4.06\" SPLIT GATE DA2H ACTUATOR\nKILL VALVE DESCRIPTION: 2.06\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 4.06\" SPLIT GATE DA2H ACTUATOR\nLOWER MASTER VALVE (LMV): 4.06\" MANUAL SPLIT GATE\nTEE DESCRIPTION: 4.06\" TEE F/ FLOW WING\nSERVICE: H2S","TEE DESCRIPTION: 4.06\" FLANGED * 4.06\" STUDDED * 2-1/16\" STUDDED WITH\nINLAY.\n2NO 1/2\" NPT PORTS FOR PRESSURE/TEMPERATURE GAUGE\nXMAS TREE AND ALL VALVES ARE HYDRO TESTED TO PSL-2 AND GAS TESTED TO\nPSL-3G.\nALL VALVES TESTED AS SINGLE BLOCKED (TEST 1 SIDE AT A TIME) AND DOUBLE\nBLOCKED TESTED.\nXMAS TREE FUNCTION TEST PER SFT-053.\n\nHYD. MASTER VALVE WITH WIRELINE SHEAR CAPABILITY\n\nCOATING AS PER DQC-062\nIN CASE OF DIFFERENCES, FOLLOW NOC STANDARD SD-NOC-COR-355 (TSA), SD-\nNOC-COR-356 (FOR FASTENERS)\n\n(See attached drawing <(>&<)> BOM)\n","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nDATA BOOK\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 4.06\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13.625\" 10000 PSI RBC DOWN\nTRIM: HH-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nMATERIAL SPECIFICATION: NACE, ISO-15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: SD-NOC-COR-355, 356\nTREE CAP DESCRIPTION: 6GR52 W/ 0.5\" NPT PLUG\nSWAB VALVE DESCRIPTION: 4.06\" MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 4.06\" SPLIT GATE DA2H ACTUATOR\nKILL VALVE DESCRIPTION: 2.06\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 4.06\" SPLIT GATE DA2H ACTUATOR\nLOWER MASTER VALVE (LMV): 4.06\" MANUAL SPLIT GATE\nTEE DESCRIPTION: 4.06\" TEE F/ FLOW WING\nSERVICE: H2S","ZGMD_XMT_NM","PD",0,0,0,{"v":243840,"d":"243,840.00"}]
[1000402,"TBG,HANGER 5-1/2\",FF TRIM",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-502447-02","","TUBING HANGER:\nTBG,HANGER 5-1/2\",FF TRIM\nTubing Hanger, 5-1/2\", , 5-1/2\" 15.5# SL Apex Box down, , w/ 8 off 1/4\"\ndown-hole control line ports, w/ 4.875\" QN petroline plug profile.\n\n","","","","","","","-","-","PD",0,0,0,{"v":19150.27,"d":"19,150.27"}]
[1000403,"TBG,HANGER 5-1/2\",HH TRIM",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-502625-02","","TUBING HANGER:\nTBG,HANGER 5-1/2\",HH TRIM\nTubing Hanger, 5-1/2\", , 5-1/2\" 15.5# SL Apex Box down, w/ 8 off 1/4\"\ndown-hole control line ports, w/ 4.875\" QN petroline plug profile\n","","","","","","","-","-","PD",0,0,0,{"v":19450,"d":"19,450.00"}]
[1000404,"XMT:SGL,5.125\",5000 PSI,13.625\" 10000 P>",null,null,"EA","XMT","4000003","DRIL-QUIP / SINGAPORE","6-502309-02","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 5.125\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13.625\" 10000 PSI RBC DOWN\nTRIM: EE-NL+\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nMATERIAL SPECIFICATION: NACE, ISO-15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: SD-NOC-COR-355, 356\nTREE CAP DESCRIPTION: 6GR52 W/ 0.5\" NPT PLUG\nSWAB VALVE DESCRIPTION: 5.125\" MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 5.125\" SPLIT GATE DA2H ACTUATR\nKILL VALVE DESCRIPTION: 2.06\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 5.125\" SPLIT GATE DA2H ACTUATR\nLOWER MASTER VALVE (LMV): 5.125\" MANUAL SPLIT GATE\nTEE DESCRIPTION: 5.125\" TEE F/ FLOW WING\nSERVICE: H2S","XMT, 5-1/8\" ,EE TRIM\nTree Assembly, 5-1/8\", 5,000 psi, API 6A, EE-NL, U, PSL-2, PR-2, 13-\n5/8\"  Radial Bolt Connector down w/ 13-5/8\" inconel clad DX-1 gasket\nprep down, w/ internal Tubing Hanger neck seal pocket, w/ Grayloc 6GR52\nTree Cap and Wing Outlet LMV and PSV - 5-1/8\" Series DHS Manual Split\ntype gate valve  UMV - 5-1/8\" Series DHS Split type Gate Valve w/ Series\nDA5 Hydraulically Actuated w/ wire shear capability PWV - 5-1/8\" Series\nDHS Split type Gate Valve w/ Series DA5 Hydraulically Actuated\nSWV - 2-1/16\" Series DHS Split Type Manual Gate Valve  -  OR EQUIVALENT\n\n\n(See attached)","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nDATA BOOK\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 5.125\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13.625\" 10000 PSI RBC DOWN\nTRIM: EE-NL+\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nMATERIAL SPECIFICATION: NACE, ISO-15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: SD-NOC-COR-355, 356\nTREE CAP DESCRIPTION: 6GR52 W/ 0.5\" NPT PLUG\nSWAB VALVE DESCRIPTION: 5.125\" MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 5.125\" SPLIT GATE DA2H ACTUATR\nKILL VALVE DESCRIPTION: 2.06\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 5.125\" SPLIT GATE DA2H ACTUATR\nLOWER MASTER VALVE (LMV): 5.125\" MANUAL SPLIT GATE\nTEE DESCRIPTION: 5.125\" TEE F/ FLOW WING\nSERVICE: H2S","ZGMD_XMT_NM","PD",0,0,0,{"v":175243,"d":"175,243.00"}]
[1000405,"XMT:SGL,5.125\",5000 PSI,13.625\" 10000 P>",null,null,"EA","XMT","4000003","DRIL-QUIP / SINGAPORE","6-502626-02","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 5.125\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13.625\" 10000 PSI RBC DOWN\nTRIM: HH-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nMATERIAL SPECIFICATION: NACE, ISO-15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: SD-NOC-COR-355, 356\nTREE CAP DESCRIPTION: 6GR52 W/ 0.5\" NPT PLUG\nSWAB VALVE DESCRIPTION: 5.125\" MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 5.125\" SPLIT GATE DA2H ACTUATR\nKILL VALVE DESCRIPTION: 2.06\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 5.125\" SPLIT GATE DA2H ACTUATR\nLOWER MASTER VALVE (LMV): 5.125\" MANUAL SPLIT GATE\nTEE DESCRIPTION: 5.125\" TEE F/ FLOW WING\nSERVICE: H2S","TEE DESCRIPTION: 5.125\" FLANGED * 5.125\" STUDDED * 2-1/16\" STUDDED WITH\nINLAY.\n2NO 1/2\" NPT PORTS FOR PRESSURE/TEMPERATURE GAUGE\nXMAS TREE AND ALL VALVES ARE HYDRO TESTED TO PSL-2 AND GAS TESTED TO\nPSL-3G.\nALL VALVES TESTED AS SINGLE BLOCKED (TEST 1 SIDE AT A TIME) AND DOUBLE\nBLOCKED TESTED.\nXMAS TREE FUNCTION TEST PER SFT-053.\n\nHYD. MASTER VALVE WITH WIRELINE SHEAR CAPABILITY\n\nCOATING AS PER DQC-062\nIN CASE OF DIFFERENCES, FOLLOW NOC STANDARD SD-NOC-COR-355 (TSA), SD-\nNOC-COR-356 (FOR FASTENERS)\n\n(See attached drawing <(>&<)> BOM)\n","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nDATA BOOK\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 5.125\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13.625\" 10000 PSI RBC DOWN\nTRIM: HH-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nMATERIAL SPECIFICATION: NACE, ISO-15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: SD-NOC-COR-355, 356\nTREE CAP DESCRIPTION: 6GR52 W/ 0.5\" NPT PLUG\nSWAB VALVE DESCRIPTION: 5.125\" MANUAL SPLIT GATE\nWING VALVE DESCRIPTION: 5.125\" SPLIT GATE DA2H ACTUATR\nKILL VALVE DESCRIPTION: 2.06\" MANUAL SPLIT GATE\nUPPER MASTER VALVE (UMV): 5.125\" SPLIT GATE DA2H ACTUATR\nLOWER MASTER VALVE (LMV): 5.125\" MANUAL SPLIT GATE\nTEE DESCRIPTION: 5.125\" TEE F/ FLOW WING\nSERVICE: H2S","ZGMD_XMT_NM","PD",0,0,0,{"v":294515,"d":"294,515.00"}]
[1000406,"HANGER:TBG;13.625\" X 7\",5000 PSI,HH-NL,>",null,null,"EA","XMT","4000003","DRIL-QUIP / SINGAPORE","6-502627-02","HANGER:TUBING;\nBOWL SIZE X CASING/TUBING SIZE: 13.625\" X 7\"\nPRESSURE RATING: 5000 PSI\nTRIM: HH-NL\nTEMPERATURE RATING: P-U\nINSIDE DIAMETER: 6.25\"\nOUTSIDE DIAMETER: 13.542\"\nTOP SIZE/CONNECTION: 7.875\" 3-TPI SQUARE RH THREAD\nBOTTOM SIZE/CONNECTION: 7\" 23# SL APEX\nHANGER NECK SIZE: 7\"\nFLOW BY AREA: N/A\nMAX FLOW BY PARTICLE SIZE: N/A\nCONTROL LINE FEEDTHROUGH: 8 X 0.25\" C/L, INC825 FITTINGS\nBPV PREPARATION: 6.25\" QN PETROLINE\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2\nSERVICE: H2S\nTYPE: SU-902 DRIL-QUIP WELLHEAD\n","SEE ATTACHED.","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","HANGER:TUBING;\nBOWL SIZE X CASING/TUBING SIZE: 13.625\" X 7\"\nPRESSURE RATING: 5000 PSI\nTRIM: HH-NL\nTEMPERATURE RATING: P-U\nINSIDE DIAMETER: 6.25\"\nOUTSIDE DIAMETER: 13.542\"\nTOP SIZE/CONNECTION: 7.875\" 3-TPI SQUARE RH THREAD\nBOTTOM SIZE/CONNECTION: 7\" 23# SL APEX\nHANGER NECK SIZE: 7\"\nFLOW BY AREA: N/A\nMAX FLOW BY PARTICLE SIZE: N/A\nCONTROL LINE FEEDTHROUGH: 8 X 0.25\" C/L, INC825 FITTINGS\nBPV PREPARATION: 6.25\" QN PETROLINE\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2\nSERVICE: H2S\nTYPE: SU-902 DRIL-QUIP WELLHEAD\n","ZGMD_HGR_TBG","PD",0,0,0,{"v":72350,"d":"72,350.00"}]
[1000407,"XMT:SGL,6.375\",5000 PSI,13.625\" 10000 P>",null,null,"EA","XMT","4000003","DRIL-QUIP / SINGAPORE","6-502628-02","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 6.375\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13.625\" 10000 PSI RBC DOWN\nTRIM: HH-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2\nMATERIAL SPECIFICATION: NACE, ISO-15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: SD-NOC-COR-355, 356\nTREE CAP DESCRIPTION: 8GR72 GRAYLOC TOP C/W 1/2\" NPT\nSWAB VALVE DESCRIPTION: 6.375\" MANUAL DHS SPLIT GATE\nWING VALVE DESCRIPTION: 6.375\" ACTUATED DHS SPLIT GATE\nKILL VALVE DESCRIPTION: 2.06\" MANUAL DHS SPLIT GATE\nUPPER MASTER VALVE (UMV): 6.375\" ACTUATED DAS SPLIT GATE\nLOWER MASTER VALVE (LMV): 6.375\" MANUAL DHS SPLIT GATE\nTEE DESCRIPTION: 6.375\" TEE F/ FLOW WING\nSERVICE: H2S\nDRAWING/DOCUMENT REFERENCE-1:\nDRAWING/DOCUMENT REFERENCE-2:","\n(See attached)\n","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION\nMATERIAL CERTIFICATE EN 10204 3.1\nDATA BOOK","","","","","","XMAS TREE:\nTYPE: SINGLE\nBORE SIZE: 6.375\"\nWORKING PRESSURE: 5000 PSI\nBOTTOM SIZE/CONNECTION: 13.625\" 10000 PSI RBC DOWN\nTRIM: HH-NL\nTEMPERATURE RATING: U\nPERFORMANCE REQUIREMENT: PR2\nPRODUCT SPECIFICATION LEVEL: PSL-2\nMATERIAL SPECIFICATION: NACE, ISO-15156\nSPECIFICATION: API 6A\nBODY TEST PRESSURE: 5000 PSI MWP\nGATE & SEAT PRESSURE: 5000 PSI MWP\nCOATING: SD-NOC-COR-355, 356\nTREE CAP DESCRIPTION: 8GR72 GRAYLOC TOP C/W 1/2\" NPT\nSWAB VALVE DESCRIPTION: 6.375\" MANUAL DHS SPLIT GATE\nWING VALVE DESCRIPTION: 6.375\" ACTUATED DHS SPLIT GATE\nKILL VALVE DESCRIPTION: 2.06\" MANUAL DHS SPLIT GATE\nUPPER MASTER VALVE (UMV): 6.375\" ACTUATED DAS SPLIT GATE\nLOWER MASTER VALVE (LMV): 6.375\" MANUAL DHS SPLIT GATE\nTEE DESCRIPTION: 6.375\" TEE F/ FLOW WING\nSERVICE: H2S\nDRAWING/DOCUMENT REFERENCE-1:\nDRAWING/DOCUMENT REFERENCE-2:","ZGMD_XMT_NM","PD",0,0,0,{"v":410342,"d":"410,342.00"}]
[1000408,"SEAL,NECK 7\",HH TRIM",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-502622-02","","SEAL NECK:\nSEAL,NECK 7\",HH TRIM\nManufacturer part#6-502622-02\nTubing Hanger, 7\", 7\" 23# SL Apex Box down, w/8 off 1/4\" down-hole\ncontrol line ports, w/ 6.25\" QN petroline plug profile\n","","","","","","","-","-","PD",0,0,0,0.01]
[1000410,"CSG,EMERGENCY SUB, 9-5/8\"",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-503224-02","","CASING:\nCSG,EMERGENCY SUB, 9-5/8\"\nManufacturer part#6-503224-02\n9-5/8\" Emergency Casing Sub, 9-5/8\" 40# SL Apex Box Up x Pin down\n","","","","","","","-","-","PD",0,0,0,{"v":9381,"d":"9,381.00"}]
[1000411,"COLLAR:BFLE;20\",SL-BOSS,106.5#,X56,2 STG",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","701SB/X56","COLLAR:BAFFLE;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 106.5#\nGRADE: X56\nFEATURE: 2 STAGE\n","Collar: Baffle (2-S)\nDiameter: 20\"\nWeight: 106.5#\nGrad: X56\nConnection: SL-BOSS\n\n\n\n\n\n\n","","","","","","","COLLAR:BAFFLE;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 106.5#\nGRADE: X56\nFEATURE: 2 STAGE\n","ZGMD_CLLR_BFLE","PD",0,0,0,0.01]
[1000412,"ASSY:EMERGENCY SEAL;13.62\" ELASTOMERIC,>",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-501880-02","ASSEMBLY:EMERGENCY SEAL;\nSIZE: 13.62\" ELASTOMERIC\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: U\nOUTSIDE DIAMETER: 13.559\"\nINSIDE DIAMETER: 11\" 3-PITCH 45° FLANK RH THRD\nINTERNAL THREADS: F/ H2S\nELASTOMERS: PR2\nPERFORMANCE REQUIREMENT: PSL-2\nMATERIAL SPECIFICATION: DUAL ELASTOMERS\n","","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","03","","","","ASSEMBLY:EMERGENCY SEAL;\nSIZE: 13.62\" ELASTOMERIC\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: U\nOUTSIDE DIAMETER: 13.559\"\nINSIDE DIAMETER: 11\" 3-PITCH 45° FLANK RH THRD\nINTERNAL THREADS: F/ H2S\nELASTOMERS: PR2\nPERFORMANCE REQUIREMENT: PSL-2\nMATERIAL SPECIFICATION: DUAL ELASTOMERS\n","ZGMD_ASSY_EMG_SL","PD",0,0,0,{"v":1552.49,"d":"1,552.49"}]
[1000413,"C/L,LINE SUB,1/4\"",null,null,"EA","DRL","4000003","DRIL-QUIP / SINGAPORE","6-501938-02","","CONTROL LINE SUB\nC/L,LINE SUB,1/4\"\nManufacturer part#6-501938-02","","","","","","","-","-","PD",0,0,0,{"v":1786,"d":"1,786.00"}]
[1000414,"COLLAR:CMT;20\",SL-BOSS,106.5#,X56,2-S,M>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","778MC/X56","COLLAR:CEMENTING;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 106.5#\nGRADE: X56\nFEATURE: 2-S, MECHANICAL PLUG BASED\n","Collar: Cementing Collar (2-S, Mechanical plug based)\nDiameter: 20\"\nWeight: 106.5#\nGrad: X56\nConnection: SL-BOSS\n\n\n\n\n\n\n\n","","","","","","","COLLAR:CEMENTING;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 106.5#\nGRADE: X56\nFEATURE: 2-S, MECHANICAL PLUG BASED\n","ZGMD_CLLR_CMT","PD",0,0,0,0.01]
[1000415,"COLLAR:CMT;20\",SL-BOSS,106.5#,X56,2-S,H>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","777HY/X56","COLLAR:CEMENTING;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 106.5#\nGRADE: X56\nFEATURE: 2-S, HYDRAULIC\n","Collar: Cementing Collar (2-S, Hydraulic)\nDiameter: 20\"\nWeight: 106.5#\nGrad: X56\nConnection: SL-BOSS\n\n","","","","","","","COLLAR:CEMENTING;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 106.5#\nGRADE: X56\nFEATURE: 2-S, HYDRAULIC\n","ZGMD_CLLR_CMT","PD",0,0,0,0.01]
[1000416,"PKR,20\",106.5#,SL BOSS,X56,7FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","ICP 7\"/X56","","Packer: Short Rubber Element (7 ft)\nDiameter: 20\"\nWeight: 106.5#\nGrad:  X-56\nConnection: SL-BOSS\n","","","","","","","-","-","PD",0,0,0,0.01]
[1000417,"PKR,20\",106.5#,SL BOSS,X56,10FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","ICP 10\"/X56","","Packer: Short Rubber Element (10 ft)\nDiameter: 20\"\nWeight: 106.5#\nGrad:  X-56\nConnection: SL-BOSS\n","","","","","","","-","-","PD",0,0,0,0.01]
[1000418,"PLUG,CMT,2STG,20\",FULL SET,MECA",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","PM2","","Plug: Cement Plug Set, Mechanical (2S)\nDiameter: 20\"\n\n","","","","","","","-","-","PD",0,0,0,0.01]
[1000419,"PLUG,CMT,2STG,20\",FULL SET,HYD",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","PH2","","Plug: 3 Pieces Plug Set, Hydraulic (2S)\nDiameter: 20\"\n","","","","","","","-","-","PD",0,0,0,0.01]
[1000420,"COLLAR:BFLE;20\",SL-BOSS,166.5#,X65,2 STG",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","701SB/X65","COLLAR:BAFFLE;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 166.5#\nGRADE: X65\nFEATURE: 2 STAGE\n","Collar: Baffle Collar (2-S)\nDiameter: 20\"\nWeight: 166.5#\nGrad: X65\nConnection: SL-BOSS\n\n","","","","","","","COLLAR:BAFFLE;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 166.5#\nGRADE: X65\nFEATURE: 2 STAGE\n","ZGMD_CLLR_BFLE","PD",0,0,0,0.01]
[1000421,"COLLAR:CMT;20\",SL-BOSS,166.5#,X65,2-S,M>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","778MC/X65","COLLAR:CEMENTING;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 166.5#\nGRADE: X65\nFEATURE: 2-S, MECHANICAL PLUG BASED\n","Collar: Cementing Collar (2-S, Mechanical plug based)\nDiameter: 20\"\nWeight: 166.5#\nGrad: X65\nConnection: SL-BOSS\n\n\n\n","","","","","","","COLLAR:CEMENTING;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 166.5#\nGRADE: X65\nFEATURE: 2-S, MECHANICAL PLUG BASED\n","ZGMD_CLLR_CMT","PD",0,0,0,0.01]
[1000422,"COLLAR:CMT;20\",SL-BOSS,166.5#,X65,2-S,H>",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","777HY/X65","COLLAR:CEMENTING;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 166.5#\nGRADE: X65\nFEATURE: 2-S, HYDRAULIC\n","Collar: Cementing Collar (2-S, Hydraulic)\nDiameter: 20\"\nWeight: 166.5#\nGrad: X65\nConnection: SL-BOSS\n","","","","","","","COLLAR:CEMENTING;\nSIZE: 20\"\nCONNECTION A: SL-BOSS\nWEIGHT: 166.5#\nGRADE: X65\nFEATURE: 2-S, HYDRAULIC\n","ZGMD_CLLR_CMT","PD",0,0,0,{"v":17030,"d":"17,030.00"}]
[1000423,"PKR,20\",166.5#,SL BOSS,X65,7FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","ICP 7\"/X65","","Packer: ACP Long Rubber Element (7 ft)\nDiameter: 20\"\nWeight: 166.5#\nGrad:  X-65\nConnection: SL-BOSS","","","","","","","-","-","PD",0,0,0,0.01]
[1000424,"PKR,20\",166.5#,SL BOSS,X65,10FT",null,null,"EA","DRL","4000246","FORUM US/ DAVIS LYNCH","ICP 10\"/X65","","Packer: ACP Long Rubber Element (10 ft)\nDiameter: 20\"\nWeight: 166.5#\nGrad:  X-65\nConnection: SL-BOSS","","","","","","","-","-","PD",0,0,0,0.01]
[1000431,"(BLCK)CHEM,GLYCLOL CORROSION INHIB,KI-30",null,null,"L","CHE","","","","","CHEM,GLYCLOL CORROSION INHIB,KI-3013,BK\nRecommended Use Corrosion inhibitor\nSee MSDS for details attached in Palm\"\n","","","06","","100161005","","-","-","ND",{"v":0,"d":"0.000"},{"v":0,"d":"0.000"},{"v":0,"d":"0.000"},0.01]
[1000432,"COVERALL:FLME RETDNT,280 GR/M²,1(SMALL)>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 1(SMALL)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARB\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","COVERALL ORANGE FLAME RETARDANT WITH LOGO\n280 GR/M² 75% COTTON-24% POLYESTER-1%CARBONE\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n\n\n\n\n\n\n","","","","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 1(SMALL)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARB\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","ZGMD_C_ALL_NM","V1",0,100,200,87.79]
[1000433,"COVERALL:FLME RETDNT,280 GR/M²,2(M),OR,>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 2(M)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","COVERALL ORANGE FLAME RETARDANT WITH LOGO\n280 GR/M² 75% COTTON-24% POLYESTER-1%CARBONE\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n\n\n\n\n\n","","","","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 2(M)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","ZGMD_C_ALL_NM","V1",0,100,250,54.97]
[1000434,"COVERALL:FLME RETDNT,280 GR/M²,3 (L),OR>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 3 (L)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","COVERALL ORANGE FLAME RETARDANT WITH LOGO\n280 GR/M² 75% COTTON-24% POLYESTER-1%CARBONE\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n\n\n\n\n\n","","","","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 3 (L)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","ZGMD_C_ALL_NM","V1",0,100,200,{"v":55.2,"d":"55.20"}]
[1000435,"COVERALL:FLME RETDNT,280 GR/M²,4 (XL),O>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 4 (XL)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","COVERALL ORANGE FLAME RETARDANT WITH LOGO\n280 GR/M² 75% COTTON-24% POLYESTER-1%CARBONE\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n\n\n\n\n\n","","","","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 4 (XL)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","ZGMD_C_ALL_NM","V1",0,120,200,68.99]
[1000436,"COVERALL:FLME RETDNT,280 GR/M²,5 (XXL),>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 5 (XXL)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","COVERALL ORANGE FLAME RETARDANT WITH LOGO\n280 GR/M² 75% COTTON-24% POLYESTER-1%CARBONE\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n\n\n\n\n\n","","","","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 5 (XXL)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","ZGMD_C_ALL_NM","V1",0,150,250,84.39]
[1000437,"COVERALL:FLME RETDNT,280 GR/M²,6 (XXXL)>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 6 (XXXL)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","ORANGE COVERALL WITH LOGO\n280 GR/M² 75% COTTON-24% POLYESTER-1%CARBONE\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n\n\n\n","","","","","","","COVERALL:\nTYPE: FLAME RETARDANT, 280 GR/M²\nSIZE: 6 (XXXL)\nCOLOUR: ORANGE\nMATERIAL: 75% COT-24% POLY-1% CARBONE\nSTANDARD: ISO11612:2008 A1 B1 C1 F1","ZGMD_C_ALL_NM","V1",0,50,80,83.28]
[1000438,"COVERALL:FLME RETDNT,210 GR/M²,1 (S),LT>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 1 (S)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ANTISTATIC FLAME RETARDANT LIGHT ORANGE COVERALL WITH LOGO\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n\n\n","","","","01","1047081","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 1 (S)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ZGMD_C_ALL_NM","V1",0,150,250,50.27]
[1000439,"(BLCK)COVERALL:FLME RETDNT,210 GR/M²,2 (",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 2 (M)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ANTISTATIC FLAME RETARDANT LIGHT ORANGE COVERALL WITH LOGO\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.","","LIGHT ORANGE COVERALL 210 GR/M² 54% MODA 44% LYOCELL 2%  WITH LOGO\nISO11612:2008 A1 A2 B1 C1 F1\nEN1149-5:2008\nSIZE 2 (M)\nManufacturer:DMD France\n\n14 Sept 2017 PO Long text as per below:\nLIGHT ORANGE COVERALL 210 GR/M² 54% MODA 44% LYOCELL 2%  WITH LOGO\nISO11612:2008 A1 A2 B1 C1 F1\nEN1149-5:2008\nSIZE 2 (M)","06","","1047085","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 2 (M)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ZGMD_C_ALL_NM","PD",0,0,0,50.26]
[1000440,"(BLCK)COVERALL:FLME RETDNT,210 GR/M²,3 (",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 3 (L)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ANTISTATIC FLAME RETARDANT LIGHT ORANGE COVERALL WITH LOGO\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n","","LIGHT ORANGE COVERALL 210 GR/M² 54% MODA 44% LYOCELL 2% WITH LOGO\nISO11612:2008 A1 A2 B1 C1 F1\nEN1149-5:2008\nSIZE 3 (L)\nManufacturer:DMD France\n\n14 Sept 2017 PO Long text as per below:\nLIGHT ORANGE COVERALL 210 GR/M² 54% MODA 44% LYOCELL 2% WITH LOGO\nISO11612:2008 A1 A2 B1 C1 F1\nEN1149-5:2008\nSIZE 3 (L)","06","","1047086","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 3 (L)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ZGMD_C_ALL_NM","PD",0,0,0,50.27]
[1000441,"COVERALL:FLME RETDNT,210 GR/M²,4 (XL),L>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 4 (XL)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ANTISTATIC FLAME RETARDANT LIGHT ORANGE COVERALL WITH LOGO\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n","","","","01","1047089","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 4 (XL)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ZGMD_C_ALL_NM","PD",0,0,0,50.41]
[1000442,"COVERALL:FLME RETDNT,210 GR/M²,5 (XXL),>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 5 (XXL)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ANTISTATIC FLAME RETARDANT LIGHT ORANGE COVERALL WITH LOGO\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n","","LIGHT ORANGE COVERALL 210 GR/M² 54% MODA 44% LYOCELL 2% WITH LOGO\nISO11612:2008 A1 A2 B1 C1 F1\nEN1149-5:2008\nSIZE 5 (XXL)\nManufacturer:DMD France\n\n14 Sept 2017 PO Long text as per below:\nLIGHT ORANGE COVERALL 210 GR/M² 54% MODA 44% LYOCELL 2% WITH LOGO\nISO11612:2008 A1 A2 B1 C1 F1\nEN1149-5:2008\nSIZE 5 (XXL)","04","01","1047087","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 5 (XXL)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ZGMD_C_ALL_NM","PD",0,0,0,51.82]
[1000443,"COVERALL:FLME RETDNT,210 GR/M²,6 (XXXL)>",null,null,"EA","PPE","","","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 6 (XXXL)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ANTISTATIC FLAME RETARDANT LIGHT ORANGE COVERALL WITH LOGO\nEN1149-5:2008\n\nSEE ATTACHED CATALOGUE.\n","","LIGHT ORANGE COVERALL 210 GR/M² 54% MODA 44% LYOCELL 2%  WITH LOGO\nISO11612:2008 A1 A2 B1 C1 F1\nEN1149-5:2008\nSIZE 6 (XXXL)\nManufacturer:DMD France\n\n14 Sept 2017 PO Long text as per below:\nLIGHT ORANGE COVERALL 210 GR/M² 54% MODA 44% LYOCELL 2%  WITH LOGO\nISO11612:2008 A1 A2 B1 C1 F1\nEN1149-5:2008\nSIZE 6 (XXXL)","","01","1047088","","COVERALL:\nTYPE: FLAME RETARDANT, 210 GR/M²\nSIZE: 6 (XXXL)\nCOLOUR: LIGHT ORANGE\nMATERIAL: 54%MODA 44%LYOCELL 2%ANTISTIC\nSTANDARD: ISO11612:2008 A1 A2 B1 C1 F1","ZGMD_C_ALL_NM","V1",0,200,300,57.29]
[1000445,"(BLCK)SHOES:SAF,36/US 5.5,BLK,FULL LTH,E",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY\nSIZE: 36/ US 5.5\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC\nEN ISO 20345:2011 S3 HRO SRC\n\nSEE THE ATTACHMENT","","","06","","1040765","","SHOES:\nTYPE: SAFETY\nSIZE: 36/ US 5.5\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,54.14]
[1000446,"(BLCK)SHOES:SAF,37/US 6,BLK,FULL LTH,EN",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY\nSIZE: 37/ US 6\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC.\nEN ISO 20345:2011 S3 HRO SRC\n\n","","","06","","1040764","","SHOES:\nTYPE: SAFETY\nSIZE: 37/ US 6\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,53.42]
[1000447,"(BLCK)SHOES:SAF,38/US 6.5,BLK,FULL LTH,E",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY\nSIZE: 38/ US 6.5\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE, FULL LEATHER, WATER\nRESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION FLEXI-\nMIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING, ANTISTATIC,\nBLACK COLOUR.\n\nSEE THE ATTACHMENT ..\n\n","","","06","","1040759","","SHOES:\nTYPE: SAFETY\nSIZE: 38/ US 6.5\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,52.64]
[1000448,"(BLCK)SHOES:SAF,39/US 7,BLK,FULL LTH,EN",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY\nSIZE: 39/ US 7\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC.\n","","","06","","1040761","","SHOES:\nTYPE: SAFETY\nSIZE: 39/ US 7\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,52.05]
[1000449,"(BLCK)SHOES:SAF,40/US 7.5,BLK,FULL LTH,E",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY\nSIZE: 40/ US 7.5\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC\n\n","","","06","","1040762","","SHOES:\nTYPE: SAFETY\nSIZE: 40/ US 7.5\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,51.57]
[1000450,"(BLCK)SHOES:SAF,41/US 8,BLK,FULL LTH,EN",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY\nSIZE: 41/ US 8\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC\n","","","06","","1040755","","SHOES:\nTYPE: SAFETY\nSIZE: 41/ US 8\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,50.97]
[1000451,"(BLCK)SHOES:SAF,42/US 9,BLK,FULL LTH,EN",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY\nSIZE: 42/ US 9\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC\n\n","","","06","","1040754","","SHOES:\nTYPE: SAFETY\nSIZE: 42/ US 9\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,51.02]
[1000452,"(BLCK)SHOES:SAF,43/US 10,BLK,FULL LTH,EN",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY\nSIZE: 43/ US 10\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC.\n\n","","","06","","1040753","","SHOES:\nTYPE: SAFETY\nSIZE: 43/ US 10\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,50.71]
[1000453,"(BLCK)SHOES:SAF,HELIOS+S3 ANKLE,44/US10.",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY,HELIOS+S3 ANKLE\nSIZE: 44/US10.5\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC.\n\n","","","06","","1040752","","SHOES:\nTYPE: SAFETY,HELIOS+S3 ANKLE\nSIZE: 44/US10.5\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 SRC","ZGMD_SHOES_NM","PD",0,0,0,48.81]
[1000454,"(BLCK)SHOES:SAF HELIOS S3,45/US 11,BLK,F",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY HELIOS S3\nSIZE: 45/ US 11\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC.\n","","","06","","1040760","","SHOES:\nTYPE: SAFETY HELIOS S3\nSIZE: 45/ US 11\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,50.08]
[1000455,"(BLCK)SHOES:SAF HELIOS S3,46/US 12,BLK,F",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY HELIOS S3\nSIZE: 46/ US 12\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC.\n\n","","","06","","1040766","","SHOES:\nTYPE: SAFETY HELIOS S3\nSIZE: 46/ US 12\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,54.11]
[1000456,"(BLCK)SHOES:SAF HELIOS S3,47/US 13,BLK,F",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY HELIOS S3\nSIZE: 47/ US 13\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","FOR PERMANENT STAFF, MODEL Rock Fall RF170 GRANITE,\nWATER RESISTANT, PROTECTIVE STEEL TOECAP AND COMPOSITE ANTI-PENETRATION\nFLEXI-MIDSOLE, MOISTURE WICKING BREATHABLE MESH FABRIC LINING,\nANTISTATIC.\n","","","06","","1040748","","SHOES:\nTYPE: SAFETY HELIOS S3\nSIZE: 47/ US 13\nCOLOUR: BLACK\nMATERIAL: FULL LEATHER\nSTANDARD: EN ISO 20345:2011 S3 HRO SRC","ZGMD_SHOES_NM","PD",0,0,0,53.77]
[1000457,"HELMET:V GARD 200,NON-VENTILATED,WHT,EN>",null,null,"EA","PPE","","","","HELMET:\nTYPE: V GARD 200, NON-VENTILATED\nCOLOUR: WHITE\nSTANDARD: EN13463-1, EN397, EN50365","","","","","","","199197465","HELMET:\nTYPE: V GARD 200, NON-VENTILATED\nCOLOUR: WHITE\nSTANDARD: EN13463-1, EN397, EN50365","ZGMD_HELM_NM","V1",0,200,600,10.31]
[1000458,"HELMET:SAF V-GARD 200 VNT,RD",null,null,"EA","PPE","","","","HELMET:\nTYPE: SAFETY V-GARD 200 VENTILATED\nCOLOUR: RED\n","HELMET V GARD 200 RED VENTILATED\nREGULAR WITH FAS-TRAC (RATCHET) SUSPENSION\nWITH LOGO\nEN13463-1, EN397, EN50366\n\n","","","","","","","HELMET:\nTYPE: SAFETY V-GARD 200 VENTILATED\nCOLOUR: RED\n","ZGMD_HELM_NM","V1",0,20,30,14.75]
[1000459,"STRAP:CHIN STRP,SUITABLE F/MSA V-GARD",null,null,"EA","PPE","","","","STRAP:\nTYPE: CHIN STRAP\nSIZE: SUITABLE FOR MSA V-GARD\n","CHIN STRAP FOR SAFETY HELMET V GARD 200\n","","","","","","1000672","STRAP:\nTYPE: CHIN STRAP\nSIZE: SUITABLE FOR MSA V-GARD\n","ZGMD_STRAP_NM","V1",0,500,{"v":1000,"d":"1,000"},0.76]
[1000460,"(BLCK)PROT:HEAR;EAR MUFF,ADAPTABLE HELM",null,null,"EA","PPE","","","","PROTECTOR:HEARING;\nTYPE: EAR MUFF, ADAPTABLE HELMET\n","EAR CUPS OPTIMEIII H540P3E-413-SVTO ADAPT ON THE HELMET V GARD 200\n\n\n","","","06","","199197451","","PROTECTOR:HEARING;\nTYPE: EAR MUFF, ADAPTABLE HELMET\n","ZGMD_PROT_HEARING","PD",0,0,0,13.88]
[1000461,"GLASSES:SAF;PREMIUM 2750,CLR",null,null,"EA","PPE","","","","GLASSES:SAFETY;\nTYPE: PREMIUM 2750\nLENS: CLEAR\n","SAFETY GLASSES, CLEAR PREMIUM 2750\n\n","","","","","","100091140","GLASSES:SAFETY;\nTYPE: PREMIUM 2750\nLENS: CLEAR\n","ZGMD_GLASSES_SAF","V1",0,400,700,5.24]
[1000462,"GLASSES:SAF;PREMIUM 2751,TINTED",null,null,"EA","PPE","","","","GLASSES:SAFETY;\nTYPE: PREMIUM 2751\nLENS: TINTED\n","GLASSES, SAFETY TINTED PREMIUM 2751\n\n","","","","","","199197445","GLASSES:SAFETY;\nTYPE: PREMIUM 2751\nLENS: TINTED\n","ZGMD_GLASSES_SAF","V1",0,600,{"v":1000,"d":"1,000"},5.03]
[1000463,"CORD:COR F/SAF GLASSES",null,null,"EA","PPE","","","","CORD:\nTYPE: CORDS FOR SAFETY GLASSES\n","","","","","","","199145876","CORD:\nTYPE: CORDS FOR SAFETY GLASSES\n","ZGMD_CORD_NM","V1",0,{"v":1000,"d":"1,000"},{"v":2000,"d":"2,000"},{"v":0.6,"d":"0.60"}]
[1000464,"CASE:SOFT CSE F/SAF GLS",null,null,"EA","PPE","","","","CASE:\nTYPE: SOFT CASE FOR SAFETY GLASS\n","SOFT CASE FOR SAFETY GLASSES CLIC-CLAC\n\n","","","","","","","CASE:\nTYPE: SOFT CASE FOR SAFETY GLASS\n","ZGMD_CASE_NM","V1",0,150,450,1.78]
[1000465,"GLOVES:WATERPROOF SAF,8,LTH",null,null,"EA","PPE","","","","GLOVES:\nTYPE: WATERPROOF SAFETY\nSIZE: 8\nMATERIAL: LEATHER\n","WATERPROOF SAFETY LEATHER GLOVE\nSTARLAST 03/27000-30\n\n\n","","","","","","199140653","GLOVES:\nTYPE: WATERPROOF SAFETY\nSIZE: 8\nMATERIAL: LEATHER\n","ZGMD_GLOVES_NM","V1",0,600,{"v":1500,"d":"1,500"},3.72]
[1000466,"GLOVES:WATERPROOF SAF,9,LTH",null,null,"EA","PPE","","","","GLOVES:\nTYPE: WATERPROOF SAFETY\nSIZE: 9\nMATERIAL: LEATHER\n","WATERPROOF SAFETY LEATHER GLOVE\nSTARLAST 03/27000-30\n\n\n","","","","","","199140654","GLOVES:\nTYPE: WATERPROOF SAFETY\nSIZE: 9\nMATERIAL: LEATHER\n","ZGMD_GLOVES_NM","V1",0,700,{"v":1500,"d":"1,500"},3.57]
[1000467,"GLOVES:WATERPROOF SAF,10,LTH",null,null,"EA","PPE","","","","GLOVES:\nTYPE: WATERPROOF SAFETY\nSIZE: 10\nMATERIAL: LEATHER\n","WATERPROOF SAFETY LEATHER GLOVE\nSTARLAST 03/27000-30\n\n","","","","","","199192543","GLOVES:\nTYPE: WATERPROOF SAFETY\nSIZE: 10\nMATERIAL: LEATHER\n","ZGMD_GLOVES_NM","V1",0,300,600,3.72]
[1000468,"GLOVES:WATERPROOF SAF,11,LTH",null,null,"EA","PPE","","","","GLOVES:\nTYPE: WATERPROOF SAFETY\nSIZE: 11\nMATERIAL: LEATHER\n","WATERPROOF SAFETY LEATHER GLOVE\nSTARLAST 03/27000-30\n\n\n","","","","","","199192553","GLOVES:\nTYPE: WATERPROOF SAFETY\nSIZE: 11\nMATERIAL: LEATHER\n","ZGMD_GLOVES_NM","V1",0,300,600,3.92]
[1000469,"(BLCK)SHOES:BALKAN S1P,EUR 39,US 7,BLK,E",null,null,"EA","PPE","","","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 39,US 7\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","","","","06","","1040761","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 39,US 7\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","ZGMD_SHOES_NM","PD",0,0,0,14.27]
[1000470,"(BLCK)SHOES:BALKAN S1P,EUR 40,US 7.5,BLK",null,null,"EA","PPE","","","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 40, US 7.5\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","","","","06","","1040762","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 40, US 7.5\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","ZGMD_SHOES_NM","PD",0,0,0,15.06]
[1000471,"(BLCK)SHOES:BALKAN S1P,EUR 41,US 8,BLK",null,null,"EA","PPE","","","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 41, US 8\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","","","","06","","1040755","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 41, US 8\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","ZGMD_SHOES_NM","PD",0,0,0,14.74]
[1000472,"(BLCK)SHOES:BALKAN S1P,EUR 42 US 9,BLK,E",null,null,"EA","PPE","","","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 42 US 9\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","","","","06","","1040754","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 42 US 9\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","ZGMD_SHOES_NM","PD",0,0,0,16.33]
[1000473,"SHOES:BALKAN S1P,EUR 45,US 11.5,BLK,EN >",null,null,"EA","PPE","","","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 45, US 11.5\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","","","","","01","1040760","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 45, US 11.5\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","ZGMD_SHOES_NM","V1",0,30,60,{"v":14.2,"d":"14.20"}]
[1000474,"(BLCK)SHOES:BALKAN S1P,EUR 44 US 10.5,BL",null,null,"EA","PPE","","","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 44 US 10.5\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","","","","06","","1040752","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 44 US 10.5\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","ZGMD_SHOES_NM","PD",0,0,0,14.26]
[1000475,"(BLCK)SHOES:SAF,EUR 45,US 11,BLK,BALKAN",null,null,"EA","PPE","","","","SHOES:\nTYPE: SAFETY\nSIZE: EUR 45, US 11\nCOLOUR: BLACK\nMATERIAL: BALKAN S1P\nSTANDARD: EN ISO 20345:2011","","","","06","","1040760","","SHOES:\nTYPE: SAFETY\nSIZE: EUR 45, US 11\nCOLOUR: BLACK\nMATERIAL: BALKAN S1P\nSTANDARD: EN ISO 20345:2011","ZGMD_SHOES_NM","PD",0,0,0,26.75]
[1000477,"(BLCK)SHOES:BALKAN S1P,EUR 46,US 12,BLK,",null,null,"EA","PPE","","","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 46, US 12\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","","","","06","","1040766","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 46, US 12\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","ZGMD_SHOES_NM","PD",0,0,0,14.21]
[1000478,"GLASSES:SAF;UV PROT,CLR,PC,ASDCA-10-S07>",null,null,"EA","PPE","","","","GLASSES:SAFETY;\nTYPE: UV PROTECTION\nLENS: CLEAR\nFRAME: POLYCARBONATE\nDRAWING/DOCUMENT REFERENCE-1: ASDCA-10-S07052-0003_SH.5,22","VEGA BLUE BRANCH\n\n","","GALLAF BATCH 1 INPUT FROM DIETSMANN - MODIFIED AS PER REV 11 (MANASA)\n(APPROVED BY TADM), 10 Sep 2020\n","","","","","GLASSES:SAFETY;\nTYPE: UV PROTECTION\nLENS: CLEAR\nFRAME: POLYCARBONATE\nDRAWING/DOCUMENT REFERENCE-1: ASDCA-10-S07052-0003_SH.5,22","ZGMD_GLASSES_SAF","V1",0,300,800,{"v":2,"d":"2.00"}]
[1000479,"(BLCK)GLASSES, SAFETY TINTED VEGA BLUE",null,null,"EA","PPE","","","","","GLASSES, SAFETY TINTED VEGA BLUE BRANCH,\nSCREEN POLYCARBONAT TINTED\n\n","","","06","","","199145885","-","-","PD",0,0,0,5.09]
[1000480,"GLOVES:CUT/R;7,HDPE&GLS FIBER,EN388(4.4>",null,null,"EA","PPE","","","","GLOVES:CUT RESISTANT;\nSIZE: 7\nMATERIAL: HDPE AND GLASS FIBER\nSTANDARD: EN388(4.4.4.2.)\n","GLOVES, SAFETY CUT RESISTANT SIZE 7 STARTCUT MAX 4\nHDPE AND GLASS FIBER\nPOLYURETHANE\nEN388 : 4.4.4.2.\n\n","","","","","","199192812","GLOVES:CUT RESISTANT;\nSIZE: 7\nMATERIAL: HDPE AND GLASS FIBER\nSTANDARD: EN388(4.4.4.2.)\n","ZGMD_GLOVES_CUT_R","V1",0,100,400,3.38]
[1000481,"GLOVES:CUT/R;8,HDPE&GLS FIBER,EN388 (4.>",null,null,"EA","PPE","","","","GLOVES:CUT RESISTANT;\nSIZE: 8\nMATERIAL: HDPE AND GLASS FIBER\nSTANDARD: EN388 (4.4.4.2.)\n","GLOVES, SAFETY CUT RESISTANT SIZE 8\nSTARTCUT MAX 4\nHDPE AND GLASS FIBER\nPOLYURETHANE\nEN388 : 4.4.4.2.\n\n","","","","","","199192565","GLOVES:CUT RESISTANT;\nSIZE: 8\nMATERIAL: HDPE AND GLASS FIBER\nSTANDARD: EN388 (4.4.4.2.)\n","ZGMD_GLOVES_CUT_R","V1",0,{"v":1200,"d":"1,200"},{"v":2000,"d":"2,000"},3.61]
[1000482,"GLOVES:CUT/R;9,HDPE&GLS FIBER,EN388 (4.>",null,null,"EA","PPE","","","","GLOVES:CUT RESISTANT;\nSIZE: 9\nMATERIAL: HDPE AND GLASS FIBER\nSTANDARD: EN388 (4.4.4.2.)\n","GLOVES, SAFETY CUT RESISTANT SIZE 9\nSTARTCUT MAX 4\nHDPE AND GLASS FIBER\nPOLYURETHANE\nEN388 : 4.4.4.2.\n\n\n","","","","","","199192703","GLOVES:CUT RESISTANT;\nSIZE: 9\nMATERIAL: HDPE AND GLASS FIBER\nSTANDARD: EN388 (4.4.4.2.)\n","ZGMD_GLOVES_CUT_R","V1",0,{"v":1500,"d":"1,500"},{"v":3000,"d":"3,000"},3.61]
[1000483,"GLOVES:CUT/R;10,HDPE,GLS FIBER,EN388 : >",null,null,"EA","PPE","","","","GLOVES:CUT RESISTANT;\nSIZE: 10\nMATERIAL: HDPE, GLASS FIBER\nSTANDARD: EN388 : 4.4.4.2.\n","GLOVES, SAFETY CUT RESISTANT SIZE 10\nSTARTCUT MAX 4\nHDPE AND GLASS FIBER\nPOLYURETHANE\nEN388 : 4.4.4.2.\n\n","","","","","","199192885","GLOVES:CUT RESISTANT;\nSIZE: 10\nMATERIAL: HDPE, GLASS FIBER\nSTANDARD: EN388 : 4.4.4.2.\n","ZGMD_GLOVES_CUT_R","V1",0,{"v":1000,"d":"1,000"},{"v":2200,"d":"2,200"},3.61]
[1000484,"GLOVE,IMPACT,CUT RESISTANT CAYMAN SIZE 8",null,null,"EA","PPE","","","","","GLOVES, SAFETY IMPACT <(>&<)> CUT RESISTANT CAYMAN SIZE 8\nHPPE AND GLASS FIBER\nEN 388 : 4.5.4.3\n\n\n","","","04","01","","FOLLOW UP 1038929","-","-","PD",0,0,0,11.17]
[1000485,"(BLCK)GLOVE,IMPACT CUT RESISTANT CAYMAN",null,null,"EA","PPE","","","","","GLOVES, SAFETY IMPACT <(>&<)> CUT RESISTANT CAYMAN SIZE 9\nHPPE AND GLASS FIBER\nEN 388 : 4.5.4.4\n\n","","","06","","","FOLLOW UP 1038928","-","-","PD",0,0,0,11.17]
[1000486,"GLOVE,IMPACT CUT RESISTANT CAYMAN SIZE10",null,null,"EA","PPE","","","","","GLOVES, SAFETY IMPACT <(>&<)> CUT RESISTANT CAYMAN SIZE 10\nHPPE AND GLASS FIBER\nEN 388 : 4.5.4.4\n\n\n","","","","01","","FOLLOW UP 1038927","-","-","PD",0,0,0,11.17]
[1000487,"GLOVE,IMPACT CUT RESISTANT CAYMAN SIZE11",null,null,"EA","PPE","","","","","GLOVES, SAFETY IMPACT <(>&<)> CUT RESISTANT CAYMAN SIZE 11\nHPPE AND GLASS FIBER\nEN 388 : 4.5.4.5\n\n\n","","","","01","","FOLLOW UP 1038926","-","-","PD",0,0,0,11.17]
[1000488,"GLOVES:CR;7,NAT LATEX,EN 374,BL",null,null,"EA","PPE","","","","GLOVES:CHEMICAL RESISTANT;\nSIZE: 7\nMATERIAL: NATURAL LATEX\nSTANDARD: EN 374\nCOLOUR: BLUE\n","GLOVES, SAFETY CHEMICAL, JERSETTE 300 LATEX\nCAT 2\n\n","","","","","","199156892","GLOVES:CHEMICAL RESISTANT;\nSIZE: 7\nMATERIAL: NATURAL LATEX\nSTANDARD: EN 374\nCOLOUR: BLUE\n","ZGMD_GLOVES_CR","V1",0,15,20,3.25]
[1000489,"GLOVES:CR;8,NAT LATEX,EN 374,BL",null,null,"EA","PPE","","","","GLOVES:CHEMICAL RESISTANT;\nSIZE: 8\nMATERIAL: NATURAL LATEX\nSTANDARD: EN 374\nCOLOUR: BLUE\n","GLOVES, SAFETY CHEMICAL, JERSETTE 300 LATEX\nCAT 2\n\n","","","","","","","GLOVES:CHEMICAL RESISTANT;\nSIZE: 8\nMATERIAL: NATURAL LATEX\nSTANDARD: EN 374\nCOLOUR: BLUE\n","ZGMD_GLOVES_CR","V1",0,400,700,10.99]
[1000490,"GLOVES:CR;9,NAT LATEX,EN 374,BL",null,null,"EA","PPE","","","","GLOVES:CHEMICAL RESISTANT;\nSIZE: 9\nMATERIAL: NATURAL LATEX\nSTANDARD: EN 374\nCOLOUR: BLUE\n","GLOVES, SAFETY CHEMICAL, JERSETTE 300 LATEX\nCAT 2\n\n\n","","","","","","199193227","GLOVES:CHEMICAL RESISTANT;\nSIZE: 9\nMATERIAL: NATURAL LATEX\nSTANDARD: EN 374\nCOLOUR: BLUE\n","ZGMD_GLOVES_CR","V1",0,400,800,10.99]
[1000491,"GLOVES:CR;10,RBR LATEX NEO,STR,EN 374,3>",null,null,"EA","PPE","","","","GLOVES:CHEMICAL RESISTANT;\nSIZE: 10\nMATERIAL: RUBBER LATEX NEOPRENE\nCUFF: STRAIGHT\nSTANDARD: EN 374\nLENGTH: 300MM\nDRAWING/DOCUMENT REFERENCE-1: ASDCA-10-S07052-0003_SH.4,37","Chemical Safety Gloves,Size:10/XL\n","","GALLAF BATCH 1 INPUT FROM DIETSMANN - MODIFIED AS PER REV 11 (MANASA)\n(APPROVED BY TADM), 10 Sep 2020\n","","","","","GLOVES:CHEMICAL RESISTANT;\nSIZE: 10\nMATERIAL: RUBBER LATEX NEOPRENE\nCUFF: STRAIGHT\nSTANDARD: EN 374\nLENGTH: 300MM\nDRAWING/DOCUMENT REFERENCE-1: ASDCA-10-S07052-0003_SH.4,37","ZGMD_GLOVES_CR","V1",0,150,350,3.56]
[1000492,"GLOVES:WLD;9,EN420,EN407,EN12477",null,null,"EA","PPE","","","","GLOVES:WELDING;\nSIZE: 9\nSTANDARD: EN420, EN407, EN12477\n","GLOVES, SAFETY WELDING\nSTARTHOT 03/03520-30\nEN388: 3.1.4.4.\nEN407: 4.1.3.X.4.X.\nEN12477: Type A\n\n\n\n","","","","","","","GLOVES:WELDING;\nSIZE: 9\nSTANDARD: EN420, EN407, EN12477\n","ZGMD_GLV_WLD","V1",0,50,100,3.44]
[1000493,"GLOVES:WLD;10,EN420,EN407,EN12477",null,null,"EA","PPE","","","","GLOVES:WELDING;\nSIZE: 10\nSTANDARD: EN420, EN407, EN12477\n","GLOVES, SAFETY WELDING\nSTARTHOT 03/03520-30\nEN388 : 3.1.4.4.\nEN407 : 4.1.3.X.4.X.\nEN12477 : Type A\n\n\n\n\n","","","","","","199193286","GLOVES:WELDING;\nSIZE: 10\nSTANDARD: EN420, EN407, EN12477\n","ZGMD_GLV_WLD","V1",0,60,100,3.68]
[1000494,"GLOVES:ELEC;500V,7,36CM,LATEX",null,null,"EA","PPE","","","","GLOVES:ELECTRICAL;\nVOLTAGE: 500V\nSIZE: 7\nLENGTH: 36CM\nMATERIAL: LATEX\n","ELECTROSOFT LATEX CL00 (500V)\nEN 60903-2003\nCLASS 00\nPRODUCT NUMBER: 2091903\n\n\n\n\n\n","","","","","","","GLOVES:ELECTRICAL;\nVOLTAGE: 500V\nSIZE: 7\nLENGTH: 36CM\nMATERIAL: LATEX\n","ZGMD_GLOVES_ELEC","PD",20,0,0,15.65]
[1000495,"GLOVES:ELEC;500V,8,36CM,LATEX",null,null,"EA","PPE","","","","GLOVES:ELECTRICAL;\nVOLTAGE: 500V\nSIZE: 8\nLENGTH: 36CM\nMATERIAL: LATEX\n","GLOVES, SAFETY ELECTRICAL\nELECTROSOFT LATEX CL00 (500V)\nCLASS 00\nEN 60903-2003\nPRODUCT NUMBER: 2091903\n\n\n\n\n\n","","","","","","199192909","GLOVES:ELECTRICAL;\nVOLTAGE: 500V\nSIZE: 8\nLENGTH: 36CM\nMATERIAL: LATEX\n","ZGMD_GLOVES_ELEC","V1",0,150,500,16.45]
[1000496,"GLOVES:ELEC;500V,9,36CM,LATEX",null,null,"EA","PPE","","","","GLOVES:ELECTRICAL;\nVOLTAGE: 500V\nSIZE: 9\nLENGTH: 36CM\nMATERIAL: LATEX\n","GLOVES, SAFETY ELECTRICAL\nELECTROSOFT LATEX CL00 (500V)\nCLASS 00\nEN 60903-2003\nPRODUCT NUMBER: 2091903\n\n\n\n","","","","","","100163615","GLOVES:ELECTRICAL;\nVOLTAGE: 500V\nSIZE: 9\nLENGTH: 36CM\nMATERIAL: LATEX\n","ZGMD_GLOVES_ELEC","V1",0,100,200,15.66]
[1000497,"GLOVES:ELEC;500V,10,36CM,LATEX",null,null,"EA","PPE","","","","GLOVES:ELECTRICAL;\nVOLTAGE: 500V\nSIZE: 10\nLENGTH: 36CM\nMATERIAL: LATEX\n","GLOVES, SAFETY ELECTRICAL\nELECTROSOFT LATEX CL00 (500V)\nCLASS 00\nEN 60903-2003\nPRODUCT NUMBER: 2091903\n\n\n\n\n\n","","","","","","","GLOVES:ELECTRICAL;\nVOLTAGE: 500V\nSIZE: 10\nLENGTH: 36CM\nMATERIAL: LATEX\n","ZGMD_GLOVES_ELEC","V1",0,15,20,15.68]
[1000498,"(BLCK)HELMET:SAF,53-63CM,PLYMDE,YL,ASDCA",null,null,"EA","PPE","4000390","Draeger","IRIS 2","HELMET:\nTYPE: SAFETY\nSIZE: 53-63CM\nMATERIAL: POLYAMIDE\nCOLOUR: YELLOW\nDRAWING/DOCUMENT REFERENCE-1: ASDCA-10-S07052-0003_SH.4,5\nDRAWING/DOCUMENT REFERENCE-2: COMPANY EXTRACT PALM","HELMET, SAFETY IRIS 2 WHITE\nRATCHET SYSTEM AND GLASSES 420G LOGO\n\n\n","","GALLAF BATCH 1 INPUT FROM DIETSMANN - MODIFIED AS PER REV 11 (MANASA)\n(APPROVED BY TADM), 13 Sep 2020\nITEM WAS BLOCKED AT TIME OF ABOVE MODIFICATION AND SO ENTERED ONLY\nTECHNICAL DETAILS PROVIDED BY DIETSMANN","06","","1000671","","HELMET:\nTYPE: SAFETY\nSIZE: 53-63CM\nMATERIAL: POLYAMIDE\nCOLOUR: YELLOW\nDRAWING/DOCUMENT REFERENCE-1: ASDCA-10-S07052-0003_SH.4,5\nDRAWING/DOCUMENT REFERENCE-2: COMPANY EXTRACT PALM","ZGMD_HELM_NM","ND",0,0,0,0.01]
[1000499,"(BLCK)HELMET,INTEGRATED GOOGLES IRIS 2",null,null,"EA","PPE","","","","","HELMET, SAFETY IRIS 2 RED\nRATCHET SYSTEM AND GLASSES 420G LOGO\n\n\n\n","","","06","","1000670","","-","-","ND",0,0,0,0.01]
[1000500,"(BLCK)CHIN STRAP, SUITABLE FOR IRIS 2",null,null,"EA","PPE","","","","","COTTON CHIN STRAP 12MM 0351 FOR SAFETY HELMET IRIS 2\n\n\n","","","06","","","","-","-","PD",0,0,0,0.01]
[1000501,"(BLCK)PROT,HEAR;EAR PLUG TYP 1100,200/PK",null,null,"EA","PPE","4000125","3M PRODUCTS","1100","PROTECTOR:HEARING\nSTANDARD: EN352-2:2002\n","NON CORDED EAR PLUG 1100\nBOX OF 200 PAIRS\n\n\n\n","","","06","","","FOLLOW UP 1036023","-","-","ND",0,0,0,17.95]
[1000502,"(BLCK)PROT:HEAR;EAR PLUG",null,null,"EA","PPE","","","","PROTECTOR:HEARING;\nTYPE: EAR PLUG\n","REUSABLE CORDED THERMOPLASTIC ELASTOMERE EAR PLUG\n\n\n","","","06","","","FOLLOW UP 1035838","PROTECTOR:HEARING;\nTYPE: EAR PLUG\n","ZGMD_PROT_HEARING","ND",0,0,0,{"v":1.3,"d":"1.30"}]
[1000503,"MASK:FF SARI 011680",null,null,"EA","PPE","","","","MASK:\nTYPE: FULL FACE SARI 011680\n","FULL FACE SARI 011680\nEN 136. Class 3\n\n\n\n","","","","","","199136035","MASK:\nTYPE: FULL FACE SARI 011680\n","ZGMD_MASK_NM","V1",0,30,120,62.44]
[1000504,"MASK:HLF 3M SERIE 6200,M",null,null,"EA","PPE","","","","MASK:\nTYPE: HALF 3M SERIE 6200\nSIZE: MEDIUM\n","HALF3M SERIE 6200 MASK\nPARTICULATESS, GAS AND VAPORS\n\n\n\n","","","","","","199113115","MASK:\nTYPE: HALF 3M SERIE 6200\nSIZE: MEDIUM\n","ZGMD_MASK_NM","V1",0,100,200,10.54]
[1000505,"FILTER:FLT GF22 A2B2,SUITABLE FF MASK",null,null,"EA","PPE","","","","FILTER:\nTYPE: FILTER GF22 A2B2\nSIZE: SUITABLE FULL FACE MASK\n","FILTER GF22 A2B2 FOR FULL FACE MASK SARI 042874 EN 14387\n\n\n\n","","","","","","","FILTER:\nTYPE: FILTER GF22 A2B2\nSIZE: SUITABLE FULL FACE MASK\n","ZGMD_FLT_NM","V1",0,60,210,11.48]
[1000506,"(BLCK)MASK:DUST FFP3,BOX OF 10 PCS",null,null,"EA","PPE","","","","MASK:\nTYPE: DUST FFP3\nSIZE: BOX OF 10 PCS\n","MASK SIROCCO FFP3V WITH VALVE\nBOX OF 10 PCS\n\n\n\n","","","06","","1040396","","MASK:\nTYPE: DUST FFP3\nSIZE: BOX OF 10 PCS\n","ZGMD_MASK_NM","PD",0,0,0,24.13]
[1000507,"CART:FILTER;GAS&VAP,ABE1,F/SUITABLE HLF>",null,null,"EA","PPE","4000125","3M PRODUCTS","6003","CARTRIDGE:FILTER;\nTYPE: GAS AND VAPOUR, ABE1\nSIZE: FOR SUITABLE HALF MASK 3M 6200","FILTER 6003 FOR HALF MASK 3M 6200\nEN 141 ABE1 PACK OF 2P\n\n","","","","","","199189546","CARTRIDGE:FILTER;\nTYPE: GAS AND VAPOUR, ABE1\nSIZE: FOR SUITABLE HALF MASK 3M 6200","ZGMD_CART_FLT","V1",0,350,600,8.51]
[1000508,"FILTER:PRE,F/P3 HLF MASK 3M 6200",null,null,"EA","PPE","","","","FILTER:\nTYPE: PRE,FOR P3 HALF MASK 3M 6200","PREFILTER P3SL 5935 PACK OF 2P\n\n\n\n","","","","","","","FILTER:\nTYPE: PRE,FOR P3 HALF MASK 3M 6200","ZGMD_FLT_NM","V1",0,30,60,4.01]
[1000509,"RING:501 TO MAINTAIN P3 FLT,2 PCS/PK",null,null,"EA","PPE","","","","RING:\nTYPE: 501 TO MAINTAIN P3 FILTER\nADDITIONAL INFORMATION: 2 PCS/PACK\n","RING 501 TO MAINTAIN P3 FILTER WITH ABE1\nONE PACK OF 2 PCS\n\n\n","","","","","","","RING:\nTYPE: 501 TO MAINTAIN P3 FILTER\nADDITIONAL INFORMATION: 2 PCS/PACK\n","ZGMD_RNG_NM","PD",0,0,0,1.92]
[1000510,"SHIELD:SAF/EQ;F,CHEM PROT",null,null,"EA","PPE","","","","SHIELD:SAFETY EQUIPMENT;\nTYPE: FACE,CHEMICAL PROTECTION","METAL FRAME V-GUARD 10121268 +\nFACE SHIELD POLYCARBONATE 10115836\nCHEMICAL PROTECTION\n\n\n","","","","","","1000662","SHIELD:SAFETY EQUIPMENT;\nTYPE: FACE,CHEMICAL PROTECTION","ZGMD_SHIELD_SAF_EQ","V1",0,100,200,12.05]
[1000511,"GOGGLES:CHEM PROT,CLR,ACETATE",null,null,"EA","PPE","","","","GOGGLES:\nTYPE: CHEMICAL PROTECTION\nLENS COLOUR: CLEAR\nLENS MATERIAL: ACETATE\n","CHEMICAL ACETATE GOOGLES FAHREINHEIT 71360-00015M\n\n\n","","","","","","100112406","GOGGLES:\nTYPE: CHEMICAL PROTECTION\nLENS COLOUR: CLEAR\nLENS MATERIAL: ACETATE\n","ZGMD_GOGGLES_NM","V1",0,100,200,8.43]
[1000512,"GOGGLES:COVERSALL WLD,SHADE 5",null,null,"EA","PPE","","","","GOGGLES:\nTYPE: COVERSALL WELDING\nLENS COLOUR: SHADE 5\n","WELDING GOGGLES COVERSALL\nSHADE 5\n\n\n","","","","","","199185625","GOGGLES:\nTYPE: COVERSALL WELDING\nLENS COLOUR: SHADE 5\n","ZGMD_GOGGLES_NM","PD",0,0,0,8.12]
[1000513,"SHIELD:SAF/EQ;F SHLD,WLD,CB4000",null,null,"EA","PPE","","","","SHIELD:SAFETY EQUIPMENT;\nTYPE: FACE SHIELD,WELDING,CB4000","WELDING FACE SHIELD CB4000, MASK\n\n\n","","","","","","","SHIELD:SAFETY EQUIPMENT;\nTYPE: FACE SHIELD,WELDING,CB4000","ZGMD_SHIELD_SAF_EQ","V1",0,25,50,14.93]
[1000514,"(BLCK)BAG:W/NOC LOGO,SEE DIMS IN PO TXT",null,null,"EA","PPE","","","","BAG:\nTYPE: WITH NOC LOGO\nSIZE: SEE DIMENSIONS IN PO TEXT\n","Offshore use, BLUE color,\n\nAcceptable sizes:\n\n60 X 38 X 38 CM, 72L\n60 X 40 X 21 CM\n\n(See attached pic)\n\n","","","06","","1045914","","BAG:\nTYPE: WITH NOC LOGO\nSIZE: SEE DIMENSIONS IN PO TEXT\n","ZGMD_BAG_NM","PD",0,0,0,{"v":25.5,"d":"25.50"}]
[1000520,"BLD:PIPE;RF,12\",150#,LTCS,A350,LF2 CL1,>",null,null,"EA","PIP","","","","BLIND:PIPE;\nTYPE: RF\nSIZE: 12\"\nRATING: 150#\nMATERIAL: LTCS\nSPECIFICATION: ASTM A350\nGRADE: LF2 CL1\nDIMENSION STANDARD: ASME B16.5\nNOC STANDARD: SD-NOC-PVV-145\nMATERIAL DATASHEET: DS-PVV-145-02\nADDITIONAL REQUIREMENTS: AS PER NACE MR0175/ISO 15156","","MATERIAL CERTIFICATE EN 10204 3.1\nQUALITY CHECK AT GOODS RECIEPT\nISO 15156 CONFIRMATORY STATEMENT\nCHARPY IMPACT TEST REQUIREMENT AT -46C\n\nNDT DOCUMENTATION (IN ACCORDANCE WITH SD-NOC-PVV-145 MDS)\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","100074575","BLIND:PIPE;\nTYPE: RF\nSIZE: 12\"\nRATING: 150#\nMATERIAL: LTCS\nSPECIFICATION: ASTM A350\nGRADE: LF2 CL1\nDIMENSION STANDARD: ASME B16.5\nNOC STANDARD: SD-NOC-PVV-145\nMATERIAL DATASHEET: DS-PVV-145-02\nADDITIONAL REQUIREMENTS: AS PER NACE MR0175/ISO 15156","ZGMD_BLD_PIPE","V1",0,4,6,227.79]
[1000530,"COND:SEA WTR COOLD,100KW","COND","CONDUCTOR","PC","HVC","4000277","BITZER","K1053HB","CONDENSER:\nTYPE: SEA WATER COOLED\nSIZE: 100KW","SEA WATER COOLED CONDENSER,\nFOR R22 HVAC UNIT,\n2 PASSES,\nCAPACITY: 100KW,\nALLOWED MAX CAPACITY: 176KW,\nCONDENSING SDT: 32.6DEG.C.,\nWATER OUTLET TEMP: 28.6 DEG.C.,\nVOLUME FLOW RATE: 10 M3/H,\nPRESSURE DROP: 0.10 BAR,\nOPTION: PRV ADAPTER\n","","","","","","","CONDENSER:\nTYPE: SEA WATER COOLED\nSIZE: 100KW","ZGMD_CONDSR_NM","PD",1,0,0,{"v":4749.91,"d":"4,749.91"}]
[1000540,"(BLCK)SHOES:BALKAN S1P,EUR 43,US 10,BLK,",null,null,"EA","PPE","","","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 43, US 10\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","","","","06","","1040753","","SHOES:\nTYPE: BALKAN S1P\nSIZE: EUR 43, US 10\nCOLOUR: BLACK\nSTANDARD: EN ISO 20345:2011\n","ZGMD_SHOES_NM","PD",0,0,0,{"v":14.3,"d":"14.30"}]
[1000544,"GLASSES:SAF;TINTED,VEGA OR,PC",null,null,"EA","PPE","","","","GLASSES:SAFETY;\nTYPE: TINTED, VEGA ORANGE\nLENS: POLYCARBONATE\n","GLASSES, SAFETY TINTED VEGA ORANGE  BRANCH,\nSCREEN POLYCARBONAT TINTED\n\n\n\n\n\n\n\n\n\n\n\n\n\n","","","","","","199145881","GLASSES:SAFETY;\nTYPE: TINTED, VEGA ORANGE\nLENS: POLYCARBONATE\n","ZGMD_GLASSES_SAF","V1",0,200,400,3.92]
[1000551,"CLAMP:C/L;X-CPL,3.5\",TGL,POLYMER",null,null,"EA","COM","4000002","EMERSON-ROXAR / UK","PCP-5835-05-03","CLAMP:CONTROL LINE;\nTYPE: CROSS COUPLING\nSIZE: 3.5\"\nMODEL/CLOSING FEATURE: TOGGLE\nMETALLURGY: POLYMER","","","","","","","","CLAMP:CONTROL LINE;\nTYPE: CROSS COUPLING\nSIZE: 3.5\"\nMODEL/CLOSING FEATURE: TOGGLE\nMETALLURGY: POLYMER","ZGMD_CLMP_CTRL_L","PD",0,0,0,167.96]
[1000560,"BONNET:VLV;BNNT ASSY,RV ACT,4.0125\",VET>","VLV","VALVE","EA","XMT","4000782","CAMERON / SINGAPORE","2149697-04-31","BONNET:VALVE;\nVALVE STYLE: BONNET ASSEMBLY, RV ACTUATOR\nVALVE SIZE: 4.0125\"\nVALVE MODEL: VETCO VG-300\nTRIM: EE-NL\nTEMPERATURE RATING: P-U\nRATING: 5000 PSI\nMATERIAL: BONNET 4130, STEM ALLOY 718\nCOATING: X-401438-01 REV 01\nACTUATOR MODEL/TYPE: RV 0304\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nPERFORMANCE REQUIREMENT: PR2\nSPECIFICATION: API 6A","CONTRACT 4600000221, PG 19/103, ITEM NO. 4\nPRIMER COATED 4\" RV BONNET ASSEMBLY, SMALL NUB,\nAPI 6A 20TH EDITION ED/ISO 10423, SSV,\nPACKING CARTRIDGE MATERIAL: ALLOY 718, SUR-SEAL DESIGN\nSP-009010-01 TO BE FINALISED","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nDATA BOOK\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","BONNET:VALVE;\nVALVE STYLE: BONNET ASSEMBLY, RV ACTUATOR\nVALVE SIZE: 4.0125\"\nVALVE MODEL: VETCO VG-300\nTRIM: EE-NL\nTEMPERATURE RATING: P-U\nRATING: 5000 PSI\nMATERIAL: BONNET 4130, STEM ALLOY 718\nCOATING: X-401438-01 REV 01\nACTUATOR MODEL/TYPE: RV 0304\nPRODUCT SPECIFICATION LEVEL: PSL-2 (W/ PSL-3G GAS TEST)\nPERFORMANCE REQUIREMENT: PR2\nSPECIFICATION: API 6A","ZGMD_BONNET_VLV","PD",0,0,0,{"v":10249,"d":"10,249.00"}]
[1000561,"KIT:REP,SGHT GLS",null,null,"EA","DRL","4000782","CAMERON / SINGAPORE","2149750-04-01","KIT:\nTYPE: REPAIR\nAPPLICATION: SIGHT GLASS","SIGHT GLASS, FOR MODEL 0304\n\"CSWC' 7B-88464F34R HYDRAULIC ACTUATOR\"","MATERIAL CERTIFICATE EN 10204 2.1\nCOMPLIANCE TO DATA SHEET\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","KIT:\nTYPE: REPAIR\nAPPLICATION: SIGHT GLASS","ZGMD_KIT_NM","V1",0,5,15,{"v":595,"d":"595.00"}]
[1000562,"ACT:HYD;CSWC 0506,API 6A,6000 PSI,PSL-3>",null,null,"EA","DRL","4000782","CAMERON / SINGAPORE","2149713-05-00-01","ACTUATOR:HYDRAULIC;\nTYPE: CSWC 0506\nPRESSURE RATING: API 6A, 6000 PSI, PSL-3, PR2\nOPERATION: HYDRAULIC\nFEEDBACK: W/ P<(>&<)>F PROXIMITY SENSORS\nSIZE: 5\"\n","ACTUATOR ASSEMBLY, CSWC, 0506,\nAPI 6A, SSV, PR 2, W/PEPPERL<(>&<)> FUCHS PROXIMITY SENSORS, W/SPECIAL\nSWITCH\nCOVER <(>&<)> WINDOW,\nLARGE NUB, 6000 PSI MAX. W.P,\nTEMP RANGE -20 TO 250 DEG. F,\nNAS 9 CLEANLINESS, (SP-009010-01),","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nHYDRAULIC CLEANLINESS REPORT\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","ACTUATOR:HYDRAULIC;\nTYPE: CSWC 0506\nPRESSURE RATING: API 6A, 6000 PSI, PSL-3, PR2\nOPERATION: HYDRAULIC\nFEEDBACK: W/ P<(>&<)>F PROXIMITY SENSORS\nSIZE: 5\"\n","ZGMD_ACT_HYD","PD",0,0,0,{"v":20575.6,"d":"20,575.60"}]
[1000563,"BONNET ASSBY,5-1/8\" 5K VETCO VG300,EE-NL",null,null,"EA","DRL","4000782","CAMERON / SINGAPORE","2149697-05-11","","\"BONNET ASSEMBLY 5-1/8\"\" 5K VETCO MODEL\nVG 300, API 6A 20TH ED/ISO 10423,\nPSL-2 (PSL-3G GAS TEST), T/C P-U,\nMC:EE-NL, LARGE NUB, F/ CSWC HYDRAULIC\nACTUATOR, (BONNET MAT'L: 4140 LAS,\nSTEM MAT'L: ALLOY 718 STEM,\nPACKING CARTRIDGE MAT'L: ALLOY 718,\nSUR-SEAL DESIGN, (SP-009010-01),(PRIMER ONLY)\n","","","","","","","-","-","PD",0,0,0,{"v":17177.15,"d":"17,177.15"}]
[1000564,"BONNET ASSBY,5-1/8\" 5K VETCO VG300,HH-NL",null,null,"EA","DRL","4000782","CAMERON / SINGAPORE","2149697-05-31","","\"BONNET ASSEMBLY 5-1/8\"\" 5K VETCO MODEL VG\n300, API 6A 20TH ED/ISO 10423, SSV,\nPSL-3G, TC:P-U, MC: HH-NL, LARGE NUB,\nF/ MODEL CSWC HYDRAULIC ACTUATOR,\n(BONNET MAT'L: 4130 LAS W/ FULL ALLOY\n625 WELD CLAD, STEM MAT'L: ALLOY 718,\nPACKING CARTRIDGE MAT'L: ALLOY 718),\nSUR-SEAL DESIGN, (SP-009010-01),(PRIMER ONLY)\"\n","","","","","","","-","-","PD",0,0,0,{"v":26280.43,"d":"26,280.43"}]
[1000568,"ASSY,PBP AND LTCH,4.5\",SL-APEX,6FT",null,null,"EA","DRL","","","","","\"Tubing Seal Locator w/ Latch and Polished Bore Receptacle\nVendor JDE Number 1002017038\nSize (in.) 7 x 4-1/2\nMax OD (in.) 5.750\nMin ID (in.) 3.875 (Through Seals)\nStroke (in.) 72”\nMin. Working Pressure (psi) 5,000\nDrift (in.) 3.833\nThread Up 4-1/2\"\" 12.6 lb/ft SL Apex Box\nThread Down 4-1/2\"\" 12.6 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi conformance to NACE\nMR-0175 Flow Wetted\nElastomers Dual Molded Nitrile Seals\nShear Rating (lbs) 85,000\"\n","","05 May 2017: PO Long Text as per below\n\"Tubing Seal Locator w/ Latch and Polished Bore Receptacle\nVendor JDE Number 1002017038\nSize (in.) 7 x 4-1/2\nMax OD (in.) 5.750\nMin ID (in.) 3.875 (Through Seals)\nStroke (in.) 72”\nMin. Working Pressure (psi) 5,000\nDrift (in.) 3.833\nThread Up 4-1/2\"\" 12.6 lb/ft SL Apex Box\nThread Down 4-1/2\"\" 12.6 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi conformance to NACE\nMR-0175 Flow Wetted\nElastomers Dual Molded Nitrile Seals\nShear Rating (lbs) 85,000\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000569,"ASSY,TIE-BACK,I,LTCH,4.5\",SL-APEX,10FT",null,null,"EA","COM","","","","","\"Petrowell Latch w/ Indexing Mule Shoe\nModel Petrowell 4.750 85k Shear Out Latch\nAnchor 10ft. Stroke w/ Indexing Muleshoe\nVendor JDE Number 1002017034\nSize (in.) 4-1/2\nMax OD (in.) 5.500\nMin ID (in.) 3.110\nStroke Length (ft.) 10\nSeals Dual Molded Nitrile\nConnection 4-1/2\"\" 12.6 lb/ft SL Apx Box up x\nIndexing\nMule Shoe down\nMaterial AISI 420 MOD-80K psi\nShear Rating (lbs) 85,000\nWorking Pressure (psi) 5,000\"\n","","05 May 2017: PO Long Text as per below\n\"Petrowell Latch w/ Indexing Mule Shoe\nModel Petrowell 4.750 85k Shear Out Latch\nAnchor 10ft. Stroke w/ Indexing Muleshoe\nVendor JDE Number 1002017034\nSize (in.) 4-1/2\nMax OD (in.) 5.500\nMin ID (in.) 3.110\nStroke Length (ft.) 10\nSeals Dual Molded Nitrile\nConnection 4-1/2\"\" 12.6 lb/ft SL Apx Box up x\nIndexing\nMule Shoe down\nMaterial AISI 420 MOD-80K psi\nShear Rating (lbs) 85,000\nWorking Pressure (psi) 5,000\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000570,"ASSY,TIE-BACK,I,LTCH,4.5\",SL-APEX,15FT",null,null,"EA","COM","","","","","\"Petrowell Latch w/ Indexing Mule Shoe\nModel Petrowell 4.750 85k Shear Out Latch Anchor 15ft. Stroke w/\nIndexing Muleshoe\nVendor JDE Number 1002017035\nSize (in.) 4-1/2\nMax OD (in.) 5.500\nMin ID (in.) 3.110\nStroke Length (ft.) 15\nSeals Dual Molded Nitrile\nConnection 4-1/2\"\" 12.6 lb/ft SL Apx Box up x\nIndexing Mule Shoe down\nMaterial AISI 420 MOD-80K psi\nShear Rating (lbs) 85,000\nWorking Pressure (psi) 5,000\"\n","","05 May 2017: PO Long Text as per below\n\"Petrowell Latch w/ Indexing Mule Shoe\nModel Petrowell 4.750 85k Shear Out Latch Anchor 15ft. Stroke w/\nIndexing Muleshoe\nVendor JDE Number 1002017035\nSize (in.) 4-1/2\nMax OD (in.) 5.500\nMin ID (in.) 3.110\nStroke Length (ft.) 15\nSeals Dual Molded Nitrile\nConnection 4-1/2\"\" 12.6 lb/ft SL Apx Box up x\nIndexing Mule Shoe down\nMaterial AISI 420 MOD-80K psi\nShear Rating (lbs) 85,000\nWorking Pressure (psi) 5,000\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000571,"LATCH:M LTCH RDRSS SEALS,DUAL MOLDED NB>",null,null,"EA","COM","4000008","WEATHERFORD USA","008149-00","LATCH:\nTYPE: MALE LATCH REDRESS SEALS\nMATERIAL: DUAL MOLDED NITRILE SEALS","Petrowell Male Latch Redress Seals\nModel: Petrowell Seal, nitrile bonded 4.500 12.6 lb/ft Shear Out Anchor\nLatch\nVendor JDE Number: 1619387\n","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","05 May 2017: PO Long Text as per below\n\"Petrowell Seal bonded 4-1/2”\n12.6 lb/ft Shear Out Anchor Latch\nModel Petrowell Seal, nitrile bonded 4.500\n12.6 lb/ft Shear Out Anchor Latch\nVendor JDE Number 1619387\nMax OD (in.) 5.500\nMin ID (in.) 3.110\nStroke Length (in.) 72\nSeals Dual Molded Nitrile\nConnection 4-1/2\"\" 13Cr 12.6 lb/ft SL Apx Pin down\nMaterial AISI 420 MOD-80K psi-13Cr\nShear Rating (lbs) 85,000\nWorking Pressure (psi) 5,000\"\n","","","","","LATCH:\nTYPE: MALE LATCH REDRESS SEALS\nMATERIAL: DUAL MOLDED NITRILE SEALS","ZGMD_LATCH_NM","PD",0,0,0,{"v":1283.4,"d":"1,283.40"}]
[1000572,"ASSY,TIE-BACK,S,LTCH,4.5\",SL-APEX,10FT",null,null,"EA","COM","","","","","\"Petrowell Latch w/ Standard Mule Shoe\nModel Petrowell 4.750 85k Shear Out Latch Anchor 10ft. Stroke w/\nStandard Muleshoe\nVendor JDE Number 1002017036\nSize (in.) 4-1/2\nMax OD (in.) 5.500\nMin ID (in.) 3.110\nStroke Length (ft.) 10\nSeals Dual Molded Nitrile\nConnection 4-1/2\"\" 12.6 lb/ft SL Apx Box up x\nIndexing Mule Shoe down\nMaterial AISI 420 MOD-80K psi\nShear Rating (lbs) 85,000\nWorking Pressure (psi) 5,000\"\n","","05 May 2017: PO Long Text as per below\n\"Petrowell Latch w/ Standard Mule Shoe\nModel Petrowell 4.750 85k Shear Out Latch Anchor 10ft. Stroke w/\nStandard Muleshoe\nVendor JDE Number 1002017036\nSize (in.) 4-1/2\nMax OD (in.) 5.500\nMin ID (in.) 3.110\nStroke Length (ft.) 10\nSeals Dual Molded Nitrile\nConnection 4-1/2\"\" 12.6 lb/ft SL Apx Box up x\nIndexing Mule Shoe down\nMaterial AISI 420 MOD-80K psi\nShear Rating (lbs) 85,000\nWorking Pressure (psi) 5,000\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000573,"ICD,AUT,SSD,3.5\",SLHT,13CR","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without  Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017073\nSize: 3-1/2\"\"\nMax OD: 4.75 inch\nMin ID of Profile: 2.810 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without  Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017073\nSize: 3-1/2\"\"\nMax OD: 4.75 inch\nMin ID of Profile: 2.810 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000574,"ICD,AUT,SSD,3.5\",SLHT,13CR,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017069\nSize: 3-1/2\"\"\nMax OD: 4.75 inch\nMin ID of Profile: 2.810 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017069\nSize: 3-1/2\"\"\nMax OD: 4.75 inch\nMin ID of Profile: 2.810 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000575,"ICD,AUT,SSD,3.5\",SLHT,13CR,GROOVE","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017057\nSize: 3-1/2\"\"\nMax OD: 6.450 inch\nMin ID of Profile: 2.810 inch\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017057\nSize: 3-1/2\"\"\nMax OD: 6.450 inch\nMin ID of Profile: 2.810 inch\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000576,"ICD,AUT,SSD,3.5\",SLHT,13CR,GROOVE,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017053\nSize: 3-1/2\"\"\nMax OD: 6.450 inch\nMin ID of Profile: 2.810 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017053\nSize: 3-1/2\"\"\nMax OD: 6.450 inch\nMin ID of Profile: 2.810 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000577,"ICD,AUT,SSD,4.5\",SLHT,13CR","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without  Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017074\nSize: 4-1/2\"\"\nMax OD: 5.630 inch\nMin ID of Profile: 2.810 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\n\"\n","","05 May 2017: PO Long Text as per below\n\"\"ICD with SSD without  Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017074\nSize: 4-1/2\"\"\nMax OD: 5.630 inch\nMin ID of Profile: 2.810 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\n\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000578,"ICD,AUT,SSD,4.5\",SLHT,13CR,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017070\nSize: 4-1/2\"\"\nMax OD: 5.630 inch\nMin ID of Profile: 3.008 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017070\nSize: 4-1/2\"\"\nMax OD: 5.630 inch\nMin ID of Profile: 3.008 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000579,"ICD,AUT,SSD,4.5\",SLHT,13CR,GROOVE","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017058\nSize: 4-1/2\"\"\nMax OD: 6.805 inch\nMin ID of Profile: 3.008 inch\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017058\nSize: 4-1/2\"\"\nMax OD: 6.805 inch\nMin ID of Profile: 3.008 inch\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000580,"ICD,AUT,SSD,4.5\",SLHT,13CR,GROOVE,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017054\nSize: 4-1/2\"\"\nMax OD: 6.805 inch\nMin ID of Profile: 3.008 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit:\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","\"ICD with SSD with Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017054\nSize: 4-1/2\"\"\nMax OD: 6.805 inch\nMin ID of Profile: 3.008 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit:\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000581,"ICD,AUT,SSD,5.5\",SLHT,13CR","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without  Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017075\nSize: 5-1/2\"\"\nMax OD: 6.900 inch\nMin ID of Profile: 3.625 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without  Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017075\nSize: 5-1/2\"\"\nMax OD: 6.900 inch\nMin ID of Profile: 3.625 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000582,"ICD,AUT,SSD,5.5\",SLHT,13CR,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017071\nSize: 5-1/2\"\"\nMax OD: 6.900 inch\nMin ID of Profile: 3.625 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017071\nSize: 5-1/2\"\"\nMax OD: 6.900 inch\nMin ID of Profile: 3.625 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000583,"ICD,AUT,SSD,5.5\",SLHT,13CR,GROOVE","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017059\nSize: 5-1/2\"\"\nMax OD: 8.075 inch\nMin ID of Profile: 3.625 inch\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017059\nSize: 5-1/2\"\"\nMax OD: 8.075 inch\nMin ID of Profile: 3.625 inch\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000584,"ICD,AUT,SSD,5.5\",SLHT,13CR,GROOVE,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017055\nSize: 5-1/2\"\"\nMax OD: 8.075 inch\nMin ID of Profile: 3.625 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017055\nSize: 5-1/2\"\"\nMax OD: 8.075 inch\nMin ID of Profile: 3.625 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000585,"ICD,AUT,SSD,6.625\",SLHT,13CR","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without  Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017076\nSize: 6-5/8\"\"\nMax OD: 8.130 inch\nMin ID of Profile: 4.696 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without  Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017076\nSize: 6-5/8\"\"\nMax OD: 8.130 inch\nMin ID of Profile: 4.696 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000586,"ICD,AUT,SSD,6.625\",SLHT,13CR,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017072\nSize: 6-5/8\"\"\nMax OD: 8.130 inch\nMin ID of Profile: 4.696 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model AICD\nVendor JDE Number 1002017072\nSize: 6-5/8\"\"\nMax OD: 8.130 inch\nMin ID of Profile: 4.696 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000587,"ICD,AUT,SSD,6.625\",SLHT,13CR,GROOVE","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017060\nSize: 6-5/8\"\"\nMax OD: 9.305 inch\nMin ID of Profile: 4.696 inch\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017060\nSize: 6-5/8\"\"\nMax OD: 9.305 inch\nMin ID of Profile: 4.696 inch\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000588,"ICD,AUT,SSD,6.625\",SLHT,13CR,GROOVE,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017056\nSize: 6-5/8\"\"\nMax OD: 9.305 inch\nMin ID of Profile: 4.696 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier\nWeatherford Model AICD\nVendor JDE Number 1002017056\nSize: 6-5/8\"\"\nMax OD: 9.305 inch\nMin ID of Profile: 4.696 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000589,"ICD,SSD,3.5\",SLHT,13CR","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017065\nSize: 3-1/2\"\"\nMax OD: 4.75 inch\nMin ID of Profile: 2.810 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017065\nSize: 3-1/2\"\"\nMax OD: 4.75 inch\nMin ID of Profile: 2.810 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000590,"ICD,SSD,3.5\",SLHT,13CR,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017061\nSize: 3-1/2\"\"\nMax OD: 4.75 inch\nMin ID of Profile: 2.810 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6.19 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017061\nSize: 3-1/2\"\"\nMax OD: 4.75 inch\nMin ID of Profile: 2.810 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6.19 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000591,"ICD,SSD,3.5\",SLHT,13CR,GROOVE","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017049\nSize: 3-1/2\"\"\nMax OD: 5.450 inch\nMin ID of Profile: 2.812 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017049\nSize: 3-1/2\"\"\nMax OD: 5.450 inch\nMin ID of Profile: 2.812 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000592,"ICD,SSD,3.5\",SLHT,13CR,GROOVE,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017045\nSize: 3-1/2\"\"\nMax OD: 5.450 inch\nMin ID of Profile: 2.810 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017045\nSize: 3-1/2\"\"\nMax OD: 5.450 inch\nMin ID of Profile: 2.810 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 3-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 3-1/2\"\" 9.2ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000593,"ICD,SSD,4.5\",SLHT,13CR","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017066\nSize: 4-1/2\"\"\nMax OD: 5.630 inch\nMin ID of Profile: 3.812 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017066\nSize: 4-1/2\"\"\nMax OD: 5.630 inch\nMin ID of Profile: 3.812 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000594,"ICD,SSD,4.5\",SLHT,13CR,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017062\nSize: 4-1/2\"\"\nMax OD: 5.630 inch\nMin ID of Profile: 3.812 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017062\nSize: 4-1/2\"\"\nMax OD: 5.630 inch\nMin ID of Profile: 3.812 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000595,"ICD,SSD,4.5\",SLHT,13CR,GROOVE","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017050\nSize: 4-1/2\"\"\nMax OD: 6.805 inch\nMin ID of Profile: 3.812 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017050\nSize: 4-1/2\"\"\nMax OD: 6.805 inch\nMin ID of Profile: 3.812 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000596,"ICD,SSD,4.5\",SLHT,13CR,GROOVE,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017046\nSize: 4-1/2\"\"\nMax OD: 6.805 inch\nMin ID of Profile: 3.812 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 -3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\" control\nline <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017046\nSize: 4-1/2\"\"\nMax OD: 6.805 inch\nMin ID of Profile: 3.812 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 -3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 4-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 4-1/2\"\" 12.6ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\" control\nline <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000598,"ICD,SSD,5.5\",SLHT,13CR","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017067\nSize: 5-1/2\"\"\nMax OD: 6.900 inch\nMin ID of Profile: 4.625 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017067\nSize: 5-1/2\"\"\nMax OD: 6.900 inch\nMin ID of Profile: 4.625 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000599,"ICD,SSD,5.5\",SLHT,13CR,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017063\nSize: 5-1/2\"\"\nMax OD: 6.900 inch\nMin ID of Profile: 4.625 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017063\nSize: 5-1/2\"\"\nMax OD: 6.900 inch\nMin ID of Profile: 4.625 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000601,"ICD,SSD,5.5\",SLHT,13CR,GROOVE","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017051\nSize: 5-1/2\"\"\nMax OD: 8.075 inch\nMin ID of Profile: 4.625 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD without Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017051\nSize: 5-1/2\"\"\nMax OD: 8.075 inch\nMin ID of Profile: 4.625 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000603,"ICD,SSD,5.5\",SLHT,13CR,GROOVE,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017047\nSize: 5-1/2\"\"\nMax OD: 8.075 inch\nMin ID of Profile: 4.625 inche\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017047\nSize: 5-1/2\"\"\nMax OD: 8.075 inch\nMin ID of Profile: 4.625 inche\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 5-1/2\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 5-1/2\"\" 15.5ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000604,"ICD,SSD,6.625\",SLHT,13CR","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017068\nSize: 6-5/8\"\"\nMax OD: 8.130 inch\nMin ID of Profile: 5.696 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017068\nSize: 6-5/8\"\"\nMax OD: 8.130 inch\nMin ID of Profile: 5.696 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\"\n","03","","","","-","-","PD",0,0,0,0.01]
[1000605,"ICD,SSD,6.625\",SLHT,13CR,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017064\nSize: 6-5/8\"\"\nMax OD: 8.130 inch\nMin ID of Profile: 5.696 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier and without Grooves\nWeatherford Model FloReg RC\nVendor JDE Number 1002017064\nSize: 6-5/8\"\"\nMax OD: 8.130 inch\nMin ID of Profile: 5.696 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 6 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000606,"ICD,SSD,6.625\",SLHT,13CR,GROOVE","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD without Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017052\nSize: 6-5/8\"\"\nMax OD: 9.305\nMin ID of Profile: 5.696 inch\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD <(>&<)> SSD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\n\"\n","","","","","","","-","-","PD",0,0,0,0.01]
[1000607,"ICD,SSD,6.625\",SLHT,13CR,GROOVE,DB","SSD","SLIDING SLEEVE","EA","COM","","","","","\"ICD with SSD with Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017048\nSize: 6-5/8\"\"\nMax OD: 9.305 inch\nMin ID of Profile: 5.696 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","05 May 2017: PO Long Text as per below\n\"ICD with SSD with Debris Barrier\nWeatherford Model FloReg RC\nVendor JDE Number 1002017048\nSize: 6-5/8\"\"\nMax OD: 9.305 inch\nMin ID of Profile: 5.696 inch\nDebris Barrier type: Wire-Wrap Strainer\nDebris Barrier Gauge: 20 gauge/500 microns\nLength of Debris Barrier: 1 - 3 ft\nMaterial of Debris Barrier: SS 316L\nType of ICD: Nozzle type\nNo. of Nozzle per ICD: 10\nSize of each Nozzle: 1/8\"\"\nMaterial of Nozzle: Tungsten Carbide\nMaterial of ICD <(>&<)> SSD: 13Cr-80ksi\nLength of ICD unit: 20 ft\nOpen Direction of SSD: shift UP to Open\nOAL of base pipe: +/- 30 ft (Range 2)\nSize of base pipe: 6-5/8\"\"\nMaterial of base pipe: 13Cr-80ksi\nConnections: 6-5/8\"\" 24ppf SLHT Box x Pin\nGroove Configuration: 2 Grooves for 3 x 1/4\"\"\ncontrol line <(>&<)> 1 x DTS cable.\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000608,"RECEP,TBG, 4.4.5\",SLAPEX P,10FT STRK",null,null,"EA","COM","","","","","\"Polished Sealbore Extension (for Latch)\nModel Petrowell 4.750 Seal Bore Extension 10 ft. Stroke\nVendor JDE Number 1002017037\nSize (in.) 4.750\nMax OD (in.) 6.090\nMin ID (in.) 3.948\nStroke Length (ft.) 10\nSeals Dual Molded Nitrile\nConnection 4-1/2\"\" 12.6 lb/ft SL Apx Pin down\nMaterial AISI 420 MOD-80K psi\nShear Rating (lbs) 85,000\nWorking Pressure (psi) 5,000\"\n","","05 May 2017: PO LONG Text as per Below\n\"Polished Sealbore Extension (for Latch)\nModel Petrowell 4.750 Seal Bore Extension 10 ft. Stroke\nVendor JDE Number 1002017037\nSize (in.) 4.750\nMax OD (in.) 6.090\nMin ID (in.) 3.948\nStroke Length (ft.) 10\nSeals Dual Molded Nitrile\nConnection 4-1/2\"\" 12.6 lb/ft SL Apx Pin down\nMaterial AISI 420 MOD-80K psi\nShear Rating (lbs) 85,000\nWorking Pressure (psi) 5,000\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000609,"SHOE,MULE,5.5\",15.5#,SLAPX,13CR,6\"MAX",null,null,"EA","COM","","","","","\"Self-Orientating Mule Shoe\nModel Indexing Mule Shoe\nVendor JDE Number 1002017033\nSize (in.) 5-1/2\nMax OD (in.) 5.985\nMin ID (in.) 4.813\nMin. Axial Compression Strength (lbs) 77,490\nThread Up 5-1/2\"\" 15.5 lb/ft SL Apex Box\nMetallurgy 13Cr, 80K psi\"\n","","05 May 2017: PO Long Text as per below\n\"Self-Orientating Mule Shoe\nModel Indexing Mule Shoe\nVendor JDE Number 1002017033\nSize (in.) 5-1/2\nMax OD (in.) 5.985\nMin ID (in.) 4.813\nMin. Axial Compression Strength (lbs) 77,490\nThread Up 5-1/2\"\" 15.5 lb/ft SL Apex Box\nMetallurgy 13Cr, 80K psi\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000610,"SPM,SBRO,4.5\",12.6#,SLAPX,BXP,13CR",null,null,"EA","COM","","","","","\"Side Pocket Mandrel with Guard Rails for Encapsulated Control Line\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DVX\nVendor JDE Number 1002017006\nSize (in.) 4-1/2\nMin. Working Pressure (psi) >7000\nMin ID (in.) 3.865\nDrift (in.) 3.833\nMax OD (in.) (considering 7 encapsulated feed\ntroughs) <(><<)>7.230\nThread Up 4-1/2\"\" 12.6 lb/ft SL Apex Box\nThread Down 4-1/2\"\" 12.6 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi minimum yield 18-\n22 HRC\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature Yes. Surface testing: 6,000 psi\nInternal and 5,000 psi External.\nTorsional Yield Strength thru Body (ftlb) 4,500\nTensile Strength thru Body (Ibs) 466,062\nWith two external premium check valves CVDVX,with DVX profile <(>&<)>\nCV-SO\nDebris Barrier\n,Elastomers Viton,Metallurgy Monel K-500\n\"\n","","05 May 2017: PO Long Text as per below\n\"Side Pocket Mandrel with Guard Rails for Encapsulated Control Line\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DVX\nVendor JDE Number 1002017006\nSize (in.) 4-1/2\nMin. Working Pressure (psi) >7000\nMin ID (in.) 3.865\nDrift (in.) 3.833\nMax OD (in.) (considering 7 encapsulated feed\ntroughs) <(><<)>7.230\nThread Up 4-1/2\"\" 12.6 lb/ft SL Apex Box\nThread Down 4-1/2\"\" 12.6 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi minimum yield 18-\n22 HRC\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature Yes. Surface testing: 6,000 psi\nInternal and 5,000 psi External.\nTorsional Yield Strength thru Body (ftlb) 4,500\nTensile Strength thru Body (Ibs) 466,062\nWith two external premium check valves CVDVX,with DVX profile <(>&<)>\nCV-SO\nDebris Barrier\n,Elastomers Viton,Metallurgy Monel K-500\n\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000611,"SPM,SBRO,4.5\",12.6#,SLAPX,BXP,9CR",null,null,"EA","COM","","","","","\"Side Pocket Mandrel with Guard Rails for Encapsulated Control Line\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DVX\nVendor JDE Number 1002017005\nSize (in.) 4-1/2\n*Min. Working Pressure (psi) >7000\nMin ID (in.) 3.865\nDrift (in.) 3.833\nMax OD (in.) (considering 7 encapsulated feed\ntroughs) <(><<)>7.230\nThread Up 4-1/2\"\" 12.6 lb/ft SL Apex Box\nThread Down 4-1/2\"\" 12.6 lb/ft SL Apex Pin\nMetallurgy 9Cr 1Mo, 80K psi minimum yield\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature\nYes. Surface testing: 6,000 psi\nInternal and 5,000 psi External.\nTorsional Yield Strength thru Body (ftlb) 4,500\nTensile Strength thru Body (Ibs) 466,062\nWith two external premium check valves CV-DVX with,DVX profile <(>&<)>\nCV-SO\nDebris Barrier\nElastomers Viton,Metallurgy Monel K-500\"\n","","06 May 2017 PO long Text as per below:\n\"Side Pocket Mandrel with Guard Rails for Encapsulated Control Line\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DVX\nVendor JDE Number 1002017005\nSize (in.) 4-1/2\n*Min. Working Pressure (psi) >7000\nMin ID (in.) 3.865\nDrift (in.) 3.833\nMax OD (in.) (considering 7 encapsulated feed\ntroughs) <(><<)>7.230\nThread Up 4-1/2\"\" 12.6 lb/ft SL Apex Box\nThread Down 4-1/2\"\" 12.6 lb/ft SL Apex Pin\nMetallurgy 9Cr 1Mo, 80K psi minimum yield\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature\nYes. Surface testing: 6,000 psi\nInternal and 5,000 psi External.\nTorsional Yield Strength thru Body (ftlb) 4,500\nTensile Strength thru Body (Ibs) 466,062\nWith two external premium check valves CV-DVX with,DVX profile <(>&<)>\nCV-SO\nDebris Barrier\nElastomers Viton,Metallurgy Monel K-500\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000612,"SPM,SBRO,5.5\",15.5#,SLAPX,BXP,13CR",null,null,"EA","COM","","","","","\"Side Pocket Mandrel with Guard Rails for Encapsulated Control Line\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DVX\nVendor JDE Number 1002017010\nSize (in.) 5-1/2\n*Min. Working Pressure (psi) >7000\n*Min ID (in.) >4.886\nDrift (in.) 4.825\nMax OD (in.) (considering 7 encapsulated\nfeed troughs) <(><<)>8.506\nThread Up 5-1/2\"\" 15.5 lb/ft SL Apex Box\nThread Down 5-1/2\"\" 15.5 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi minimum yield 18-22 HRC\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature\nYes. Surface testing: 7,370 psi\nInternal and 6,990 psi External.\nTorsional Yield Strength thru Body (ftlb) 5,400\nTensile Strength thru Body (Ibs) 519,383\"\n","","07 May 2017: PO Long Text as per below\n\"Side Pocket Mandrel with Guard Rails for Encapsulated Control Line\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DVX\nVendor JDE Number 1002017010\nSize (in.) 5-1/2\n*Min. Working Pressure (psi) >7000\n*Min ID (in.) >4.886\nDrift (in.) 4.825\nMax OD (in.) (considering 7 encapsulated\nfeed troughs) <(><<)>8.506\nThread Up 5-1/2\"\" 15.5 lb/ft SL Apex Box\nThread Down 5-1/2\"\" 15.5 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi minimum yield 18-22 HRC\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature\nYes. Surface testing: 7,370 psi\nInternal and 6,990 psi External.\nTorsional Yield Strength thru Body (ftlb) 5,400\nTensile Strength thru Body (Ibs) 519,383\"\n\n","","","","","-","-","PD",0,0,0,0.01]
[1000613,"SPM,SBRO,5.5\",15.5#,SLAPX,BXP,9CR",null,null,"EA","COM","","","","","\"Side Pocket Mandrel with Guard Rails for Encapsulated Control Line\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DVX\nVendor JDE Number 1002017009\nSize (in.) 5-1/2\n*Min. Working Pressure (psi) >7000\n*Min ID (in.) >4.886\nDrift (in.) 4.825\nMax OD (in.) (considering 7 encapsulated\nfeed troughs) <(><<)>8.506\nThread Up 5-1/2\"\" 15.5 lb/ft SL Apex Box\nThread Down 5-1/2\"\" 15.5 lb/ft SL Apex Pin\nMetallurgy 9Cr 1Mo, 80K psi minimum yield\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature Yes. Surface testing: 7,370 psi\nInternal and 6,990 psi External.\nTorsional Yield Strength thru Body (ftlb) 5,400\nTensile Strength thru Body (Ibs) 519,383\"\n","","06 May 2017 PO long Text as per below:\n\"Side Pocket Mandrel with Guard Rails for Encapsulated Control Line\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DVX\nVendor JDE Number 1002017009\nSize (in.) 5-1/2\n*Min. Working Pressure (psi) >7000\n*Min ID (in.) >4.886\nDrift (in.) 4.825\nMax OD (in.) (considering 7 encapsulated\nfeed troughs) <(><<)>8.506\nThread Up 5-1/2\"\" 15.5 lb/ft SL Apex Box\nThread Down 5-1/2\"\" 15.5 lb/ft SL Apex Pin\nMetallurgy 9Cr 1Mo, 80K psi minimum yield\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature Yes. Surface testing: 7,370 psi\nInternal and 6,990 psi External.\nTorsional Yield Strength thru Body (ftlb) 5,400\nTensile Strength thru Body (Ibs) 519,383\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000614,"SPM,SBRO,GR,4.5\",12.6#,SLAPX,BXP,13CR",null,null,"EA","COM","","","","","\"Side Pocket Mandrel with Grooves for by-pass of Encapsulated Control\nLine\nModel SBRO-2GR\nVendor JDE Number 1002017013\nSize (in.) 4-1/2\nMin. Working Pressure (psi) 9,000\nMin ID (in.) 3.933\nDrift (in.) 3.833\nMax OD (in.) (considering 7 encapsulated\nfeed troughs)\n7.060\nThread Up 4-1/2\"\" 12.6 lb/ft SL Apex Box\nThread Down 4-1/2\"\" 12.6 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi minimum yield 18-22\nHRC\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature Yes\nTorsional Yield Strength thru Body (ftlb) 80,000\nTensile Strength thru Body (Ibs) 462,374\"\n","","06 May 2017 PO long Text as per below:\n\"Side Pocket Mandrel with Grooves for by-pass of Encapsulated Control\nLine\nModel SBRO-2GR\nVendor JDE Number 1002017013\nSize (in.) 4-1/2\nMin. Working Pressure (psi) 9,000\nMin ID (in.) 3.933\nDrift (in.) 3.833\nMax OD (in.) (considering 7 encapsulated\nfeed troughs)\n7.060\nThread Up 4-1/2\"\" 12.6 lb/ft SL Apex Box\nThread Down 4-1/2\"\" 12.6 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi minimum yield 18-22\nHRC\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature Yes\nTorsional Yield Strength thru Body (ftlb) 80,000\nTensile Strength thru Body (Ibs) 462,374\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000615,"SPM,SBRO,GR,5.5\",15.5#,SLAPX,BXP,13CR",null,null,"EA","COM","","","","","\"Side Pocket Mandrel with Grooves for by-pass of Encapsulated Control\nLine\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DGR\nVendor JDE Number 1002017014\nSize (in.) 5-1/2\nMin. Working Pressure (psi) 6,450\nMin ID (in.) 4.892\nDrift (in.) 4.825\nMax OD (in.) (considering 7 encapsulated\nfeed troughs) 8.506\nThread Up 5-1/2\"\" 15.5 lb/ft SL Apex Box\nThread Down 5-1/2\"\" 15.5 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi minimum yield 18-22 HRC\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature\nYes. Surface testing: 7,370 psi\nInternal and 6,990 psi External.\nTorsional Yield Strength thru Body (ftlb) 5,400\nTensile Strength thru Body (Ibs) 519,383\n\"\n","","06 May 2017 PO long Text as per below:\n\"Side Pocket Mandrel with Grooves for by-pass of Encapsulated Control\nLine\nw / 6-11x11MM FLAT PACKS\nModel SBRO-2DGR\nVendor JDE Number 1002017014\nSize (in.) 5-1/2\nMin. Working Pressure (psi) 6,450\nMin ID (in.) 4.892\nDrift (in.) 4.825\nMax OD (in.) (considering 7 encapsulated\nfeed troughs) 8.506\nThread Up 5-1/2\"\" 15.5 lb/ft SL Apex Box\nThread Down 5-1/2\"\" 15.5 lb/ft SL Apex Pin\nMetallurgy 13Cr, 80K psi minimum yield 18-22 HRC\nOrientating Profile Yes\nPocket Size (in.) 1.500\nLatching Profile RK\nSurface Testing Feature\nYes. Surface testing: 7,370 psi\nInternal and 6,990 psi External.\nTorsional Yield Strength thru Body (ftlb) 5,400\nTensile Strength thru Body (Ibs) 519,383\n\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000616,"LATCH:M LTCH RDRSS O-RINGS,NBR 90 HI TE>",null,null,"EA","COM","4000008","WEATHERFORD USA","050-90-244","LATCH:\nTYPE: MALE LATCH REDRESS O-RINGS\nMATERIAL: NBR 90 HI TEMP","Petrowell Male Latch Redress O-rings\nModel: Petrowell Elastomeric redress kit O-ring -244 WE115\n(NBR 90 HI TEMP) SAE\nVendor JDE Number: 767333\n","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","06 May 2017 PO long Text as per below:\n\"Petrowell Elastomeric redress kit for latch including Bonded seal\nand O-ring 244 WE115 (NBR 90HI TEMP) SAE AS568\nModel Petrowell Elastomeric redress kit O-ring\n-244 WE115 (NBR 90 HI TEMP) SAE\nVendor JDE Number 767333\nMax OD (in.) N/A\nMin ID (in.) N/A\nStroke Length (in.) N/A\nSeals N/A\nConnection N/A\nMaterial NBR 90 HI TEMP\nShear Rating (lbs) N/A\nWorking Pressure (psi) N/A\"\n","","","","","LATCH:\nTYPE: MALE LATCH REDRESS O-RINGS\nMATERIAL: NBR 90 HI TEMP","ZGMD_LATCH_NM","PD",0,0,0,{"v":4,"d":"4.00"}]
[1000617,"VLV:1\",WLRETRV DUMMY,MDL RD-1,MNL K-500","VLV","VALVE","EA","WSI","4000008","WEATHERFORD USA","2754210","VALVE:\nSIZE: 1\"\nTYPE: WIRELINE RETRIEVABLE DUMMY\nSTYLE: MODEL RD-1\nBODY MATERIAL: MONEL K-500\n","Vendor JDE Number 1002017029\nElastomers MGFT Packing\n\n","","07 May 2017 PO Long Text as per below:\n\"Wireline Retrievable Dummy Valve\nModel RD-1\nVendor JDE Number 1002017029\nSize (in.) 1\nElastomers MGFT Packing\nMetallurgy Monel K-500\"\n","","","","","VALVE:\nSIZE: 1\"\nTYPE: WIRELINE RETRIEVABLE DUMMY\nSTYLE: MODEL RD-1\nBODY MATERIAL: MONEL K-500\n","ZGMD_VLV_NM","PD",6,0,0,{"v":736,"d":"736.00"}]
[1000618,"VLV,GLV,VENT,1\",0.25\",RDDK MGFT","VLV","VALVE","EA","WSI","","","","","\"Wireline Retrievable Venturi Orifice Valve with Dual Check Valve\nShearable\nModel RDDK-1BVDC\nVendor JDE Number 1002017027\nSize (in.) 1.000\nBurst rating (psi) Annulus to tubing 2,000\nPort Size (in.) 1/4\nElastomers MGFT Packing\nMetallurgy Monel K-500, with Inconel seats and\nTungsten Carbide Orifice\"\n","","07 May 2017 PO Long Text as per below:\n\"Wireline Retrievable Venturi Orifice Valve with Dual Check Valve\nShearable\nModel RDDK-1BVDC\nVendor JDE Number 1002017027\nSize (in.) 1.000\nBurst rating (psi) Annulus to tubing 2,000\nPort Size (in.) 1/4\nElastomers MGFT Packing\nMetallurgy Monel K-500, with Inconel seats and\nTungsten Carbide Orifice\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000619,"VLV,GLV,VENT,1\",0.25\",RV MGFT","VLV","VALVE","EA","WSI","","","","","\"Wireline Retrievable Venturi Orifice Valve with dual check valve\nModel RV-1HVDC\nVendor JDE Number 1002017025\nSize (in.) 1.000\nPort Size (in.) 1/4\nElastomers MGFT Packing\nMetallurgy Monel K-500, with Inconel seats and Tungsten Carbide orifice\"\n","","07 May 2017 PO Long Text as per below:\n\"Wireline Retrievable Venturi Orifice Valve with dual check valve\nModel RV-1HVDC\nVendor JDE Number 1002017025\nSize (in.) 1.000\nPort Size (in.) 1/4\nElastomers MGFT Packing\nMetallurgy Monel K-500, with Inconel seats and Tungsten Carbide orifice\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000620,"VLV,GLV,VENT,1.5\",0.25\",RDDK MGFT","VLV","VALVE","EA","WSI","","","","","\"Wireline Retrievable Venturi Orifice Valve with Dual Check Valve\nShearable\nModel RDDK-2AVDC\nVendor JDE Number 1002017028\nSize (in.) 1-1/2\nBurst rating (psi). Annulus to tubing 2,000\nPort Size (in.) 1/4\nElastomers MGFT Packing\nMetallurgy Monel K-500, with Inconel seats,\nTungsten Carbide Orifice\"\n\n","","07 May 2017 PO Long Text as per below:\n\"Wireline Retrievable Venturi Orifice Valve with Dual Check Valve\nShearable\nModel RDDK-2AVDC\nVendor JDE Number 1002017028\nSize (in.) 1-1/2\nBurst rating (psi). Annulus to tubing 2,000\nPort Size (in.) 1/4\nElastomers MGFT Packing\nMetallurgy Monel K-500, with Inconel seats,\nTungsten Carbide Orifice\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000621,"VLV,GLV,VENT,1.5\",0.25\",RV MGFT","VLV","VALVE","EA","WSI","","","","","\"Wireline Retrievable Venturi Orifice Valve with Dual Check Valve\nModel RV-2HVDC\nVendor JDE Number 1002017026\nSize (in.) 1-1/2\nPort Size (in.) 1/4\nElastomers MGFT Packing\nMetallurgy Monel K-500, with Inconel seats\"\n","","07 May 2017 PO Long Text as per below:\n\"Wireline Retrievable Venturi Orifice Valve with Dual Check Valve\nModel RV-2HVDC\nVendor JDE Number 1002017026\nSize (in.) 1-1/2\nPort Size (in.) 1/4\nElastomers MGFT Packing\nMetallurgy Monel K-500, with Inconel seats\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000622,"KIT:BNNT ASSY,4-1/8\",HH-NL,LMV ON 4.125>",null,null,"EA","WEL","4000005","GE-VETCO / UK","R199491-4","KIT:\nTYPE: BONNET ASSEMBLY\nAPPLICATION: 4-1/8\",HH-NL,LMV ON 4.125\" XMT","KIT BONNET ASSEMBLY, 4-1/8\", HH-NL\nKITS, 4-1/8 5M VG-300 FULL MANUAL BONNET ASSEMBLY FOR LMV AND SV\nINCLUDING STEM, BONNET, SEALS, FITTINGS AND STUDS/NUTS WITHOUT GATE AND\nSEAT ASSEMBLY.FOR XMAS TREE PN:H386259-1PSL-2, T/C:U, HH-NL","","07 May 2017: PO Long Text as per below\nKITS, 4-1/8 5M VG-300 FULL MANUAL BONNET ASSEMBLY FOR LMV AND SV\nINCLUDING STEM, BONNET, SEALS, FITTINGS AND STUDS/NUTS WITHOUT GATE AND\nSEAT ASSEMBLY.FOR XMAS TREE PN:H386259-1PSL-2, T/C:U, HH-NL","","","","","KIT:\nTYPE: BONNET ASSEMBLY\nAPPLICATION: 4-1/8\",HH-NL,LMV ON 4.125\" XMT","ZGMD_KIT_NM","PD",1,0,0,{"v":20470,"d":"20,470.00"}]
[1000624,"KIT:BNNT ASSY,EE-NL,LMV ON 4.125\" XMT",null,null,"EA","DRL","4000005","GE-VETCO / UK","R199491-3","KIT:\nTYPE: BONNET ASSEMBLY\nAPPLICATION: EE-NL,LMV ON 4.125\" XMT","KIT BONNET ASSEMBLY, 4-1/8\", EE-NL\nKITS, 4-1/8 5M VG-300 FULL MANUAL BONNET ASSEMBLY FOR LMV AND SV\nINCLUDING STEM, BONNET, SEALS, FITTINGS AND STUDS/NUTS, WITHOUT GATE AND\nSEAT ASSEMBLY, W/PARTIAL CLAD, FOR XMAS TREE PN: R131289-12 PSL-2,\nT/C:U, EE-NL","","07 May 2017: PO Long Text as per below\nKIT BONNET ASSEMBLY, 4-1/8\", EE-NL\nKITS, 4-1/8 5M VG-300 FULL MANUAL BONNET ASSEMBLY FOR LMV AND SV\nINCLUDING STEM, BONNET, SEALS, FITTINGS AND STUDS/NUTS, WITHOUT GATE AND\nSEAT ASSEMBLY, W/PARTIAL CLAD, FOR XMAS TREE PN: R131289-12 PSL-2,\nT/C:U, EE-NL","","","","","KIT:\nTYPE: BONNET ASSEMBLY\nAPPLICATION: EE-NL,LMV ON 4.125\" XMT","ZGMD_KIT_NM","PD",0,0,0,{"v":15916,"d":"15,916.00"}]
[1000625,"DUCT:ASSY,12M X 300MM (12M X 12\")",null,null,"EA","MEC","","","","DUCT:\nTYPE: ASSEMBLY\nSIZE: 12M X 300MM (12M X 12\")\n","DUCT ASSEMBLY 12M X 300MM (12M X 12\") MAWP 275MBAR C/W 5MM SS PLATE\nFLANGE BOTH ENDS. DRILLED TO FIT 12-INCH ASME B16.5 150LB RF FLANGE.\nFLANGES FASTENED TO DUCT WITH SS BANDING.\n\n\nREFERENCE PART NO: DM90340","","DUCT ASSEMBLY 12M X 300MM (12M X 12\") MAWP 275MBAR C/W 5MM SS PLATE\nFLANGE BOTH ENDS. DRILLED TO FIT 12-INCH ASME B16.5 150LB RF FLANGE.\nFLANGES FASTENED TO DUCT WITH SS BANDING.\n","","","","","DUCT:\nTYPE: ASSEMBLY\nSIZE: 12M X 300MM (12M X 12\")\n","ZGMD_DUCT_NM","PD",0,0,0,0.01]
[1000626,"TBG:MTLC;INST,1/4\",6M,0.035\",6MO,A269/U>",null,null,"EA","INS","","","","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/4\"\nLENGTH: 6M\nWALL THICKNESS: 0.035\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","DESIGN PRESSURE AND TEMPERATURE: 520 Barg @ 93 Deg C\nDocumentation required as per NOC standard SD-NOC-INS-114\n","STATEMENT OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 3 – WH INSPECTION","","","","","199155517","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/4\"\nLENGTH: 6M\nWALL THICKNESS: 0.035\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","ZGMD_TBG_METALLIC","V1",0,10,100,63.41]
[1000627,"TBG:MTLC;INST,1/4\",6M,0.065\",6MO,A269/U>",null,null,"EA","INS","","","","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/4\"\nLENGTH: 6M\nWALL THICKNESS: 0.065\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","DESIGN PRESSURE AND TEMPERATURE- 1035 Barg @ 93 Deg C\nDocumentation required as per NOC standard SD-NOC-INS-114\n","STATEMENT OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 3 – WH INSPECTION","","","","","1004738","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/4\"\nLENGTH: 6M\nWALL THICKNESS: 0.065\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","ZGMD_TBG_METALLIC","V1",0,20,100,89.37]
[1000629,"TBG:MTLC;INST,1/2\",6M,0.065\",6MO,A269/U>",null,null,"EA","INS","","","","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/2\"\nLENGTH: 6M\nWALL THICKNESS: 0.065\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","","MATERIAL CERTIFICATE EN 10204 3.1\nNACE CONFORMITY STATEMENT\nQC PATH 3 – WH INSPECTION","","","","","199155312","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/2\"\nLENGTH: 6M\nWALL THICKNESS: 0.065\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","ZGMD_TBG_METALLIC","V1",0,250,500,191.05]
[1000630,"TBG:MTLC;INST,1/2\",6M,0.083\",6MO,A269/U>",null,null,"EA","INS","","","","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/2\"\nLENGTH: 6M\nWALL THICKNESS: 0.083\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","","MATERIAL CERTIFICATE EN 10204 3.1\nNACE CONFORMITY STATEMENT\nQC PATH 3 – WH INSPECTION","\"TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/2\"\"\nLENGTH: 6M\nWALL THICKNESS: 0.083\"\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254 \"\n\n","04","01","1000629","","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/2\"\nLENGTH: 6M\nWALL THICKNESS: 0.083\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","ZGMD_TBG_METALLIC","PD",0,0,0,190.26]
[1000631,"TBG:MTLC;INST,1/8\",6M,0.083\",6MO,A269/U>",null,null,"EA","INS","","","","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/8\"\nLENGTH: 6M\nWALL THICKNESS: 0.083\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","","","\"TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/2\"\"\nLENGTH: 6M\nWALL THICKNESS: 0.083\"\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254 \"\n\n","","","","","TUBING:METALLIC;\nTYPE: INSTRUMENTATION\nOUTSIDE DIAMETER: 1/8\"\nLENGTH: 6M\nWALL THICKNESS: 0.083\"\nMATERIAL: 6MO\nSPECIFICATION: ASTM A269/UNS S31254","ZGMD_TBG_METALLIC","PD",0,0,0,0.01]
[1000632,"(BLCK)BLD:PIPE;",null,null,"EA","PIP","","","","BLIND:PIPE;\nTYPE:\nSIZE:\nRATING:\nTHICKNESS:\nMATERIAL:\nSPECIFICATION:\nGRADE:","","","","06","","","","BLIND:PIPE;\nTYPE:\nSIZE:\nRATING:\nTHICKNESS:\nMATERIAL:\nSPECIFICATION:\nGRADE:","ZGMD_BLD_PIPE","PD",0,0,0,0.01]
[1000633,"PSU:CUSTOM BUILT UPS,SGL,3P+N 400V 50HZ>",null,null,"PC","ELE","4000308","AEG","","POWER SUPPLY UNIT:\nTYPE: CUSTOM BUILT UPS, SINGLE\nOUTPUT VOLTAGE: 3P+N 400V 50HZ\nELECTRICAL RATING: 12KVA\n","BACK-UP <(>&<)> POWER SUPPLIES: 3P+N 400V 50HZ,\nOUTPUT POWER: 3P+N 400V 50HZ,\nCOMPLETE UNIT ACCORDINGLY TO BUT WITHOUT BATTERY BANK\n\nDATA SHEET NO: ASBFM-07-50002-0001 AND\nSPECIFICATION: ALS-BF-ECE-ELE-0003","","CUSTOM BUILT UPS,\nSINGLE TYPE,\nBACK-UP <(>&<)> POWER SUPPLIES: 3P+N 400V 50HZ,\nOUTPUT POWER: 3P+N 400V 50HZ,\nBATTERY BACK-UP: 2HR,\nCOMPLETE UNIT ACCORDINGLY TO\nDATA SHEET NO. ASBFM-AU-10=901_DS AND\nSPECIFICATION: ASBFM-AU-1901_UPS_SPEC","","","","","POWER SUPPLY UNIT:\nTYPE: CUSTOM BUILT UPS, SINGLE\nOUTPUT VOLTAGE: 3P+N 400V 50HZ\nELECTRICAL RATING: 12KVA\n","ZGMD_PWR_SPLY_NM","PD",0,0,0,{"v":42877.54,"d":"42,877.54"}]
[1000636,"PKR:5.5\" 15.5PPF SLHT/XD,8\",13CR L80,OH>",null,null,"EA","DRL","4000004","BAKER HUGHES","H30197XXX","PACKER:\nTHREAD SIZE/WEIGHT/CONNECTION: 5.5\" 15.5PPF SLHT/XD\nOUTSIDE DIAMETER: 8\"\nGRADE: 13CR L80\nADDITIONAL INFORMATION: OPEN HOLE ISOLATION\nTYPE: MPAS-H\n","MPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 5.5\"\"\nWeight: 15.5ppf\nConnection: SLHT/XD both connection\nMetallurgy: L-80 13%Cr\nOutside diameter: 8\"\nPart#H30197XXX","","13 May 2017 PO Long Text as per below:\nMPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 5.5\"\"\nWeight: 15.5ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 13%Cr\nOutside diameter: 8\"\nPart#H30197XXX","","","","","PACKER:\nTHREAD SIZE/WEIGHT/CONNECTION: 5.5\" 15.5PPF SLHT/XD\nOUTSIDE DIAMETER: 8\"\nGRADE: 13CR L80\nADDITIONAL INFORMATION: OPEN HOLE ISOLATION\nTYPE: MPAS-H\n","ZGMD_PCKR_NM","PD",0,0,0,0.01]
[1000637,"PKR, OH, MPAS-H, 5.5\" SLHT, 1CR, 8\"OD",null,null,"EA","DRL","","","","13 May 2017 PO Long Text as per below:\nMPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 5.5\"\"\nWeight: 15.58ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 1%Cr\nOutside diameter: 8\"\nPart#H30188XXX\n","MPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 5.5\"\"\nWeight: 15.58ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 1%Cr\nOutside diameter: 8\"\nPart#H30188XXX\n\n","","13 May 2017 PO Long Text as per below:\nMPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 5.5\"\"\nWeight: 15.58ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 1%Cr\nOutside diameter: 8\"\nPart#H30188XXX\n","","","","","-","-","PD",0,0,0,0.01]
[1000638,"PKR, OH, MPAS-H, 7\" SLHT, 13CR, 8\"OD",null,null,"EA","DRL","","","","13 May 2017 PO Long Text as per below:\nMPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 7\"\nWeight: 23ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 13%Cr\nOutside diameter: 8\"\"\nPart#H30188XXX\n","MPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 7\"\nWeight: 23ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 13%Cr\nOutside diameter: 8\"\"\nPart#H30188XXX\n\n\n\n","","13 May 2017 PO Long Text as per below:\nMPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 7\"\nWeight: 23ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 13%Cr\nOutside diameter: 8\"\"\nPart#H30188XXX\n","","","","","-","-","PD",0,0,0,0.01]
[1000639,"PKR, OH, MPAS-H, 7\" SLHT, 1CR, 8\"OD",null,null,"EA","DRL","4000004","BAKER HUGHES","H301880016","13 May 2017 PO Long Text as per below:\nMPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 7\"\nWeight: 23ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 1%Cr\nOutside diameter: 8\"\n","MPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 7\"\nWeight: 23ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 1%Cr\nOutside diameter: 8\"\n\n\n","","13 May 2017 PO Long Text as per below:\n\"MPAS-H Open Hole Isolation Packer Mechanical Activated\nSize: 7\"\nWeight: 23ppf\nConnection:SLHT/XD both connection\nMetallurgy: L-80 1%Cr\nOutside diameter: 8\"\n\n","","","","","-","-","PD",0,0,0,0.01]
[1000640,"SSD,SLEEVE,HYD,4.5\",SL-APEX,BXP,13CR","SSD","SLIDING SLEEVE","EA","COM","4000004","BAKER HUGHES","H810302817","13 May 2017 PO Long Text as per below:\nSurface Controlled Non Elastomeric Sliding Sleeve\nCONTRACTOR’s Part Number H81030****\nSize (in ) :4-1/2\nMm Working Pressure (psi) :7,500\nMax OD (in) :6250\nThread Up :4-1/2\"\" 12 6 lb/ft SL-APEX Box\nThread Down :4-1/2\"\" 12 6 lb/ft SL-APEX Pin\nMetallurgy :L80 13 Cr, ISO 15156 (latest revision), All Components,\nexcept control line fittings\nSeal Type: Non-Elastomeric\nNipple Profile (in.): 3.750\nControl Connection: Available on request - 10k Fitting with anti-\nvibration feature. Suitable for lines 0 028\"\" to 0.065\"\"\nMechanical back up shifting mechanism: Yes CM profile sleeve\nMechanical back up shifting force (Ibs): 1000-2000\nMin Differentia Opening Pressure Rating (psi): 1,500\nTorsional Yield Strength thru Body (ft Ib) :5,300\nTensile Strength thru Body (Ibs): 288,000\nControl Line F was:\nThe valve shall be manufactured and tested with the\nstated control line fluid only, and certified to ISO 4406 ,17/15/12\n(latest revision).\nConforms to IS014998 (latest revision): Compliant\nControl line bypass:\n4 x single 1/4\"\" Encap (11mm x 11mm) lines OR 1 x\nTriple 3 x 1/4\"\" flatpack encap (36mm x 12mm) No requirement for\nadditional protective devices\nFlow area between OD of tool and ID of casing: 28.47 in²\nPart#H81030XXXX\n","Surface Controlled Non Elastomeric Sliding Sleeve\nCONTRACTOR’s Part Number H81030****\nSize (in ) :4-1/2\nMm Working Pressure (psi) :7,500\nMax OD (in) :6250\nThread Up :4-1/2\"\" 12 6 lb/ft SL-APEX Box\nThread Down :4-1/2\"\" 12 6 lb/ft SL-APEX Pin\nMetallurgy :L80 13 Cr, ISO 15156 (latest revision), All Components,\nexcept control line fittings\nSeal Type: Non-Elastomeric\nNipple Profile (in.): 3.750\nControl Connection: Available on request - 10k Fitting with anti-\nvibration feature. Suitable for lines 0 028\"\" to 0.065\"\"\nMechanical back up shifting mechanism: Yes CM profile sleeve\nMechanical back up shifting force (Ibs): 1000-2000\nMin Differentia Opening Pressure Rating (psi): 1,500\nTorsional Yield Strength thru Body (ft Ib) :5,300\nTensile Strength thru Body (Ibs): 288,000\nControl Line F was:\nThe valve shall be manufactured and tested with the\nstated control line fluid only, and certified to ISO 4406 ,17/15/12\n(latest revision).\nConforms to IS014998 (latest revision): Compliant\nControl line bypass:\n4 x single 1/4\"\" Encap (11mm x 11mm) lines OR 1 x\nTriple 3 x 1/4\"\" flatpack encap (36mm x 12mm) No requirement for\nadditional protective devices\nFlow area between OD of tool and ID of casing: 28.47 in²\nPart#H81030XXXX\n","","13 May 2017 PO Long Text as per below:\nSurface Controlled Non Elastomeric Sliding Sleeve\nCONTRACTOR’s Part Number H81030****\nSize (in ) :4-1/2\nMm Working Pressure (psi) :7,500\nMax OD (in) :6250\nThread Up :4-1/2\"\" 12 6 lb/ft SL-APEX Box\nThread Down :4-1/2\"\" 12 6 lb/ft SL-APEX Pin\nMetallurgy :L80 13 Cr, ISO 15156 (latest revision), All Components,\nexcept control line fittings\nSeal Type: Non-Elastomeric\nNipple Profile (in.): 3.750\nControl Connection: Available on request - 10k Fitting with anti-\nvibration feature. Suitable for lines 0 028\"\" to 0.065\"\"\nMechanical back up shifting mechanism: Yes CM profile sleeve\nMechanical back up shifting force (Ibs): 1000-2000\nMin Differentia Opening Pressure Rating (psi): 1,500\nTorsional Yield Strength thru Body (ft Ib) :5,300\nTensile Strength thru Body (Ibs): 288,000\nControl Line F was:\nThe valve shall be manufactured and tested with the\nstated control line fluid only, and certified to ISO 4406 ,17/15/12\n(latest revision).\nConforms to IS014998 (latest revision): Compliant\nControl line bypass:\n4 x single 1/4\"\" Encap (11mm x 11mm) lines OR 1 x\nTriple 3 x 1/4\"\" flatpack encap (36mm x 12mm) No requirement for\nadditional protective devices\nFlow area between OD of tool and ID of casing: 28.47 in²\nPart#H81030XXXX\n","","","","","-","-","PD",0,0,0,0.01]
[1000641,"VLV, ICD MN W/SLEEVE,4.5\" SLHT BXP 13CR","VLV","VALVE","EA","COM","","","","13 May 2017 PO Long Text as per below:\nINFLOW CONTROL VALVE -MN- WITH SLIDING SLEEVE\nSize: 4-1/2\"\nWeight: 12.6 PPF\nConnection: SLHT BXP, HB-3 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX","INFLOW CONTROL VALVE -MN- WITH SLIDING SLEEVE\nSize: 4-1/2\"\nWeight: 12.6 PPF\nConnection: SLHT BXP, HB-3 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX\n\n","","13 May 2017 PO Long Text as per below:\nINFLOW CONTROL VALVE -MN- WITH SLIDING SLEEVE\nSize: 4-1/2\"\nWeight: 12.6 PPF\nConnection: SLHT BXP, HB-3 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX","","","","","-","-","PD",0,0,0,0.01]
[1000642,"VLV, ICD MN W/SLEEVE,5.5\" SLHT BXP 13CR","VLV","VALVE","EA","COM","","","","13 May 2017 PO Long Text as per below:\nINFLOW CONTROL VALVE -MN- WITH SLIDING SLEEVE\nSize: 5-1/2\"\nWeight: 15.5 PPF\nConnection: SLHT BXP, HB-2 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX","INFLOW CONTROL VALVE -MN- WITH SLIDING SLEEVE\nSize: 5-1/2\"\nWeight: 15.5 PPF\nConnection: SLHT BXP, HB-2 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX\n\n\n","","13 May 2017 PO Long Text as per below:\nINFLOW CONTROL VALVE -MN- WITH SLIDING SLEEVE\nSize: 5-1/2\"\nWeight: 15.5 PPF\nConnection: SLHT BXP, HB-2 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX","","","","","-","-","PD",0,0,0,0.01]
[1000643,"VLV,BALL,3.5\",SL-APX,BXB,L80-13CR,HYD","VLV","VALVE","EA","COM","4000004","BAKER HUGHES","H826460008","13 May 2017 PO Long Text as per below:\nSurface Controlled Hydraulic Ball Valve\nCONTRACTOR’s Part Number :H826460008\nSize (in): 3-1/2\nMm Working Pressure (psi): 5,000\nMax OD (in): 5.342\nDrift (in) :2.870\nThread Up : 3-1/2\"\" ,9.2 Ib/ft SL-APEX Box\nThread Down: 3-1/2\"\",9.2 Ib/ft SL-APEX Box\nMetallurgy : L80 13 Cr, ISO 15156 (latest revision),All Components,\nexcept control line fittings\nSeal Type : Non-Elastomeric\nControl Connection:\nAvailable on request -10k Fitting with anti-vibration feature Suitable\nfor lines 0 028\"\" to 0 065\"\"\nMm Differential Opening Pressure Rating (psi): 1500 gas / 1000 liquid\nMechanical Back Up Lock Open Mechanism Lock open :standard\nConforms to ISO 28781 Type CC V1 01 (latest revisions): V1 01 Compliant\nConfirm zero detectable leak rate at point of delivery : Compliant\nControl line bypass:\n4 x single 1/4\"\" Encap (11mm x 11mm) lines OR 1 x\nTriple 3 x 1/4\"\" flatpack encap (36mm x 12mm). No requirement for\nadditional protective devices\nControl Line Fluids:\nThe valve shall be manufactured and tested with the stated control line\nfluid only, and certified to ISO 4406 , 17/15/12 (latest revision)\nFlow area between OD of tool and ID of casing : 4.48 In²\"\n\n\n\n","Surface Controlled Hydraulic Ball Valve\nCONTRACTOR’s Part Number :H826460008\nSize (in): 3-1/2\nMm Working Pressure (psi): 5,000\nMax OD (in): 5.342\nDrift (in) :2.870\nThread Up : 3-1/2\"\" ,9.2 Ib/ft SL-APEX Box\nThread Down: 3-1/2\"\",9.2 Ib/ft SL-APEX Box\nMetallurgy : L80 13 Cr, ISO 15156 (latest revision),All Components,\nexcept control line fittings\nSeal Type : Non-Elastomeric\nControl Connection:\nAvailable on request -10k Fitting with anti-vibration feature Suitable\nfor lines 0 028\"\" to 0 065\"\"\nMm Differential Opening Pressure Rating (psi): 1500 gas / 1000 liquid\nMechanical Back Up Lock Open Mechanism Lock open :standard\nConforms to ISO 28781 Type CC V1 01 (latest revisions): V1 01 Compliant\nConfirm zero detectable leak rate at point of delivery : Compliant\nControl line bypass:\n4 x single 1/4\"\" Encap (11mm x 11mm) lines OR 1 x\nTriple 3 x 1/4\"\" flatpack encap (36mm x 12mm). No requirement for\nadditional protective devices\nControl Line Fluids:\nThe valve shall be manufactured and tested with the stated control line\nfluid only, and certified to ISO 4406 , 17/15/12 (latest revision)\nFlow area between OD of tool and ID of casing : 4.48 In²\"\n\n\n\n","","13 May 2017 PO Long Text as per below:\nSurface Controlled Hydraulic Ball Valve\nCONTRACTOR’s Part Number :H826460008\nSize (in): 3-1/2\nMm Working Pressure (psi): 5,000\nMax OD (in): 5.342\nDrift (in) :2.870\nThread Up : 3-1/2\"\" ,9.2 Ib/ft SL-APEX Box\nThread Down: 3-1/2\"\",9.2 Ib/ft SL-APEX Box\nMetallurgy : L80 13 Cr, ISO 15156 (latest revision),All Components,\nexcept control line fittings\nSeal Type : Non-Elastomeric\nControl Connection:\nAvailable on request -10k Fitting with anti-vibration feature Suitable\nfor lines 0 028\"\" to 0 065\"\"\nMm Differential Opening Pressure Rating (psi): 1500 gas / 1000 liquid\nMechanical Back Up Lock Open Mechanism Lock open :standard\nConforms to ISO 28781 Type CC V1 01 (latest revisions): V1 01 Compliant\nConfirm zero detectable leak rate at point of delivery : Compliant\nControl line bypass:\n4 x single 1/4\"\" Encap (11mm x 11mm) lines OR 1 x\nTriple 3 x 1/4\"\" flatpack encap (36mm x 12mm). No requirement for\nadditional protective devices\nControl Line Fluids:\nThe valve shall be manufactured and tested with the stated control line\nfluid only, and certified to ISO 4406 , 17/15/12 (latest revision)\nFlow area between OD of tool and ID of casing : 4.48 In²\"\n\n\n\n","","","","","-","-","PD",0,0,0,0.01]
[1000644,"VLV,BALL,4.5\",SL-APX,BXP,L80-13CR,HYD","VLV","VALVE","EA","COM","","","","13 May 2017 PO Long Text as per below:\nSurface Controlled Hydraulic Ball Valve\nCONTRACTOR’s Part Number H82646****\nSize (in): 4-1/2\nMm Working Pressure (psi): 5,000\nMax OD (in): 8.36\nDrift (in) :3.885\nThread Up :4-1/2“ ,12.6 lb/ft SL-APEX Box\nThread Down: 4-1/2\"\",12.6 lb/ft SL-APEX Pin\nMetallurgy : L80 13 Cr, ISO 15156 (latest revision) All Components,\nexcept control line fittings\nSeal Type :Non-Elastomeric\nControl Connection:\nAvailable on request - 10k Fitting with anti-vibration feature Suitable\nfor lines 0.028\"\" to 0.065\"\"\nMm Differential Opening Pressure Rating (psi): 1500 gas 11000 liquid\nMechanical Back Up Lock Open Mechanism Lock open :standard\nConforms to ISO 28781 Type CC V1 01 (latest revisions): V1 01 Compliant\nConfirm zero detectable leak rate at point of delivery :Compliant\nControl line bypass\n4 x single 1/4\"\" Encap (11mm x 11mm) lines OR 1 x\nTriple 3 x 1/4\"\" flatpack encap (36mm x 12mm). No requirement for\nadditional protective devices\nControl Line Fluids\nThe valve shall be manufactured and tested with\nthe stated control line fluid any and certified to ISO 4406 17/15/12\n(latest revision)\nFlow area between OD of tool and ID of casing :5.08 In²\"\n","Surface Controlled Hydraulic Ball Valve\nCONTRACTOR’s Part Number H82646****\nSize (in): 4-1/2\nMm Working Pressure (psi): 5,000\nMax OD (in): 8.36\nDrift (in) :3.885\nThread Up :4-1/2“ ,12.6 lb/ft SL-APEX Box\nThread Down: 4-1/2\"\",12.6 lb/ft SL-APEX Pin\nMetallurgy : L80 13 Cr, ISO 15156 (latest revision) All Components,\nexcept control line fittings\nSeal Type :Non-Elastomeric\nControl Connection:\nAvailable on request - 10k Fitting with anti-vibration feature Suitable\nfor lines 0.028\"\" to 0.065\"\"\nMm Differential Opening Pressure Rating (psi): 1500 gas 11000 liquid\nMechanical Back Up Lock Open Mechanism Lock open :standard\nConforms to ISO 28781 Type CC V1 01 (latest revisions): V1 01 Compliant\nConfirm zero detectable leak rate at point of delivery :Compliant\nControl line bypass\n4 x single 1/4\"\" Encap (11mm x 11mm) lines OR 1 x\nTriple 3 x 1/4\"\" flatpack encap (36mm x 12mm). No requirement for\nadditional protective devices\nControl Line Fluids\nThe valve shall be manufactured and tested with\nthe stated control line fluid any and certified to ISO 4406 17/15/12\n(latest revision)\nFlow area between OD of tool and ID of casing :5.08 In²\"\n","","13 May 2017 PO Long Text as per below:\n13 May 2017 PO Long Text as per below:\nSurface Controlled Hydraulic Ball Valve\nCONTRACTOR’s Part Number H82646****\nSize (in): 4-1/2\nMm Working Pressure (psi): 5,000\nMax OD (in): 8.36\nDrift (in) :3.885\nThread Up :4-1/2“ ,12.6 lb/ft SL-APEX Box\nThread Down: 4-1/2\"\",12.6 lb/ft SL-APEX Pin\nMetallurgy : L80 13 Cr, ISO 15156 (latest revision) All Components,\nexcept control line fittings\nSeal Type :Non-Elastomeric\nControl Connection:\nAvailable on request - 10k Fitting with anti-vibration feature Suitable\nfor lines 0.028\"\" to 0.065\"\"\nMm Differential Opening Pressure Rating (psi): 1500 gas 11000 liquid\nMechanical Back Up Lock Open Mechanism Lock open :standard\nConforms to ISO 28781 Type CC V1 01 (latest revisions): V1 01 Compliant\nConfirm zero detectable leak rate at point of delivery :Compliant\nControl line bypass\n4 x single 1/4\"\" Encap (11mm x 11mm) lines OR 1 x\nTriple 3 x 1/4\"\" flatpack encap (36mm x 12mm). No requirement for\nadditional protective devices\nControl Line Fluids\nThe valve shall be manufactured and tested with\nthe stated control line fluid any and certified to ISO 4406 17/15/12\n(latest revision)\nFlow area between OD of tool and ID of casing :5.08 In²\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000645,"VLV,TR-SCSSV,T-10E,3-1/2\",SLAPEX,13CR","VLV","VALVE","EA","COM","","","","13 May 2017 PO Long Text as per below:\nSURFACE CONTROLLED SUBSURFACE SAFETY VALVES\nModel: Thunder 10E\nSize (in.): 3-1/2\nSet inside Casing Size: 7\"\" 23 ppf\nMin. internal Working Pressure (psi): 5,000\nEqualizing Mechanism: Self-Equalizing Thru-Flapper,Poppet Type\nMethod to establish control line communication when WRSCSSSV is to be\ninstalled: PUNCTURE COMMUNICATION TOOL\nProfile : 2.812 BA\nMin ID (in.): 2.812\nMax OD (In.): 6.235\nThread Up: 3-1/2\"\", 9.2 lb/ft SL-APEX Box\nThread Down:  3-1/2\"\", 9.2 lb/ft SL-APEX Pin\nMin. Tong Length Area at end connections to allow make up of connection\nwith torque turn machine and: 8\nMetallurgy: 13 CR 80 MYS 22 HRC MAX\nSeal Type Body Connections:Metal-to-Metal\nMinimum Fall Safe Setting Depth (TVD ft.). Based on Salt Water (8.6ppg\nor 0.45psi/ft) In Control Line: 3500\nSafety Valve Full Opening Pressure (psi):4000 + SITP\nSafety Valve start to Close Pressure(psi): 1827 + SITP\nTorsional Yield Strength thru Body(ft lb):4130\nTensile Strength thru Safety Valve Body(lbs): 303850\nMinimum Collapse Rating of the body(psi): 5000\nMinimum Control Line Chamber Rating(psi): 15000\nControl Line Fluid: Texaco Rondo H032\nCleanliness of Hydraulic chamber:NAS Class 6\nControl Line Connection:BAKER JAM NUT CONNECTION Nickel Alloy\nThe valve must be tested according to API 14A class 3S:YES\nTemperature Rating: 32-300F\nHydraulic activation method must be a rod piston Type: Yes\"\nPart#H82708****\n","SURFACE CONTROLLED SUBSURFACE SAFETY VALVES\nModel: Thunder 10E\nSize (in.): 3-1/2\nSet inside Casing Size: 7\"\" 23 ppf\nMin. internal Working Pressure (psi): 5,000\nEqualizing Mechanism: Self-Equalizing Thru-Flapper,Poppet Type\nMethod to establish control line communication when WRSCSSSV is to be\ninstalled: PUNCTURE COMMUNICATION TOOL\nProfile : 2.812 BA\nMin ID (in.): 2.812\nMax OD (In.): 6.235\nThread Up: 3-1/2\"\", 9.2 lb/ft SL-APEX Box\nThread Down:  3-1/2\"\", 9.2 lb/ft SL-APEX Pin\nMin. Tong Length Area at end connections to allow make up of connection\nwith torque turn machine and: 8\nMetallurgy: 13 CR 80 MYS 22 HRC MAX\nSeal Type Body Connections:Metal-to-Metal\nMinimum Fall Safe Setting Depth (TVD ft.). Based on Salt Water (8.6ppg\nor 0.45psi/ft) In Control Line: 3500\nSafety Valve Full Opening Pressure (psi):4000 + SITP\nSafety Valve start to Close Pressure(psi): 1827 + SITP\nTorsional Yield Strength thru Body(ft lb):4130\nTensile Strength thru Safety Valve Body(lbs): 303850\nMinimum Collapse Rating of the body(psi): 5000\nMinimum Control Line Chamber Rating(psi): 15000\nControl Line Fluid: Texaco Rondo H032\nCleanliness of Hydraulic chamber:NAS Class 6\nControl Line Connection:BAKER JAM NUT CONNECTION Nickel Alloy\nThe valve must be tested according to API 14A class 3S:YES\nTemperature Rating: 32-300F\nHydraulic activation method must be a rod piston Type: Yes\"\nPart#H82708****\n","","13 May 2017 PO Long Text as per below:\nSURFACE CONTROLLED SUBSURFACE SAFETY VALVES\nModel: Thunder 10E\nSize (in.): 3-1/2\nSet inside Casing Size: 7\"\" 23 ppf\nMin. internal Working Pressure (psi): 5,000\nEqualizing Mechanism: Self-Equalizing Thru-Flapper,Poppet Type\nMethod to establish control line communication when WRSCSSSV is to be\ninstalled: PUNCTURE COMMUNICATION TOOL\nProfile : 2.812 BA\nMin ID (in.): 2.812\nMax OD (In.): 6.235\nThread Up: 3-1/2\"\", 9.2 lb/ft SL-APEX Box\nThread Down:  3-1/2\"\", 9.2 lb/ft SL-APEX Pin\nMin. Tong Length Area at end connections to allow make up of connection\nwith torque turn machine and: 8\nMetallurgy: 13 CR 80 MYS 22 HRC MAX\nSeal Type Body Connections:Metal-to-Metal\nMinimum Fall Safe Setting Depth (TVD ft.). Based on Salt Water (8.6ppg\nor 0.45psi/ft) In Control Line: 3500\nSafety Valve Full Opening Pressure (psi):4000 + SITP\nSafety Valve start to Close Pressure(psi): 1827 + SITP\nTorsional Yield Strength thru Body(ft lb):4130\nTensile Strength thru Safety Valve Body(lbs): 303850\nMinimum Collapse Rating of the body(psi): 5000\nMinimum Control Line Chamber Rating(psi): 15000\nControl Line Fluid: Texaco Rondo H032\nCleanliness of Hydraulic chamber:NAS Class 6\nControl Line Connection:BAKER JAM NUT CONNECTION Nickel Alloy\nThe valve must be tested according to API 14A class 3S:YES\nTemperature Rating: 32-300F\nHydraulic activation method must be a rod piston Type: Yes\"\nPart#H82708****\n","","","","","-","-","PD",0,0,0,0.01]
[1000646,"VLV,TR-SCSSV,T-5E,5-1/2\",SLAPEX,13CR","VLV","VALVE","EA","COM","","","","13 May 2017 PO Long Text as per below:\n\"TUBING RETRIEVEABLE SURFACE CONTROLLED SUBSURFACE SAFETY VALVE\nModel: Thunder 5E\nSize (in.) : 5-1/2”\nSet inside Casing Size : 9-5/8\"\", 40 lb/ft\nMin. internal Working Pressure (psi) : 5,000\nEqualizing Mechanism : Self-Equalizing Thru-Flapper, Poppet Type\nMethod to establish control line communication when WRSCSSSV is to be\ninstalled: PUNCTURE COMMUNICATION TOOL\nProfile: 4.562 BA\nMin ID (In.) : 4.562\nMax OD (In.) : 8.535\nThread Up : 5-1/2\"\" ,15.5 lb/ft SL-APEX Box\nThread Down : 5-1/2\"\" ,15.5 lb/ft SL-APEX Pin\nMin. Tong Length Area at end connections to allow make up of connection\nwith torque turn machine and rig longs (in): 8\nMetallurgy : 13 CR 80 MYS 22 HRC MAX\nSeal Type Body Connections : Metal-to-Metal\nMinimum Fall Safe Setting Depth (IVO a). Based on Salt Water (8.6ppg or\n0.45 psi/ft): 3500\nSafety Valve Full Opening Pressure (psi) : 4200 + SITP\nSafely Value start to Close Pressure (psi) : 1827+ SITP\nTorsional Yield Strength thru Body (ft lb) : 10000\nTensile Strength thru Safety Vales Body(lbs) : 530000\nMinimum Collapse Rating of the body (psi) : 5000\nMinimum Control Line Chamber Rating(psi) : 15000\nControl Line Fluid : Texaco Rando HD32\nCleanliness of Hydraulic chamber: NAS Class 6\nControl Line Connection : BAKER JAM NUT CONNECTION Nickel Alloy\nThe valve must be tested according to API 14A class 3S: YES\nTemperature Rating needs to cover : 135F 32-300F\nHydraulic activation method must be a rod piston type: YES\"\nPart#H82708****\n","\"TUBING RETRIEVEABLE SURFACE CONTROLLED SUBSURFACE SAFETY VALVE\nModel: Thunder 5E\nSize (in.) : 5-1/2”\nSet inside Casing Size : 9-5/8\"\", 40 lb/ft\nMin. internal Working Pressure (psi) : 5,000\nEqualizing Mechanism : Self-Equalizing Thru-Flapper, Poppet Type\nMethod to establish control line communication when WRSCSSSV is to be\ninstalled: PUNCTURE COMMUNICATION TOOL\nProfile: 4.562 BA\nMin ID (In.) : 4.562\nMax OD (In.) : 8.535\nThread Up : 5-1/2\"\" ,15.5 lb/ft SL-APEX Box\nThread Down : 5-1/2\"\" ,15.5 lb/ft SL-APEX Pin\nMin. Tong Length Area at end connections to allow make up of connection\nwith torque turn machine and rig longs (in): 8\nMetallurgy : 13 CR 80 MYS 22 HRC MAX\nSeal Type Body Connections : Metal-to-Metal\nMinimum Fall Safe Setting Depth (IVO a). Based on Salt Water (8.6ppg or\n0.45 psi/ft): 3500\nSafety Valve Full Opening Pressure (psi) : 4200 + SITP\nSafely Value start to Close Pressure (psi) : 1827+ SITP\nTorsional Yield Strength thru Body (ft lb) : 10000\nTensile Strength thru Safety Vales Body(lbs) : 530000\nMinimum Collapse Rating of the body (psi) : 5000\nMinimum Control Line Chamber Rating(psi) : 15000\nControl Line Fluid : Texaco Rando HD32\nCleanliness of Hydraulic chamber: NAS Class 6\nControl Line Connection : BAKER JAM NUT CONNECTION Nickel Alloy\nThe valve must be tested according to API 14A class 3S: YES\nTemperature Rating needs to cover : 135F 32-300F\nHydraulic activation method must be a rod piston type: YES\"\nPart#H82708****\n","","13 May 2017 PO Long Text as per below:\n\"TUBING RETRIEVEABLE SURFACE CONTROLLED SUBSURFACE SAFETY VALVE\nModel: Thunder 5E\nSize (in.) : 5-1/2”\nSet inside Casing Size : 9-5/8\"\", 40 lb/ft\nMin. internal Working Pressure (psi) : 5,000\nEqualizing Mechanism : Self-Equalizing Thru-Flapper, Poppet Type\nMethod to establish control line communication when WRSCSSSV is to be\ninstalled: PUNCTURE COMMUNICATION TOOL\nProfile: 4.562 BA\nMin ID (In.) : 4.562\nMax OD (In.) : 8.535\nThread Up : 5-1/2\"\" ,15.5 lb/ft SL-APEX Box\nThread Down : 5-1/2\"\" ,15.5 lb/ft SL-APEX Pin\nMin. Tong Length Area at end connections to allow make up of connection\nwith torque turn machine and rig longs (in): 8\nMetallurgy : 13 CR 80 MYS 22 HRC MAX\nSeal Type Body Connections : Metal-to-Metal\nMinimum Fall Safe Setting Depth (IVO a). Based on Salt Water (8.6ppg or\n0.45 psi/ft): 3500\nSafety Valve Full Opening Pressure (psi) : 4200 + SITP\nSafely Value start to Close Pressure (psi) : 1827+ SITP\nTorsional Yield Strength thru Body (ft lb) : 10000\nTensile Strength thru Safety Vales Body(lbs) : 530000\nMinimum Collapse Rating of the body (psi) : 5000\nMinimum Control Line Chamber Rating(psi) : 15000\nControl Line Fluid : Texaco Rando HD32\nCleanliness of Hydraulic chamber: NAS Class 6\nControl Line Connection : BAKER JAM NUT CONNECTION Nickel Alloy\nThe valve must be tested according to API 14A class 3S: YES\nTemperature Rating needs to cover : 135F 32-300F\nHydraulic activation method must be a rod piston type: YES\"\nPart#H82708****\n","","","","","-","-","PD",0,0,0,0.01]
[1000647,"VLV,WR-SCSSV,TAOFWSE-5, 5-1/2\",13CR","VLV","VALVE","EA","COM","","","","13 May 2017 PO Long Text as per below:\nWIRELINE RETRIEVEABLE SURFACE CONTROLLED SUBSURFACE SAFETY VALVE\nModel: TAOFWSE-5\nSize (in.): 5-1/2\"\"\nMin. internal Working Pressure (psi) : 5000\nEqualizing Mechanism: Self-Equalizing Thru-Rapper, Poppet Type\nLock-Type : 4.562 BA\nMin ID (in.): 2.562\nMax OD (in.): 4.640\nMetallurgy : 13 CR 80 MYS 22 HRC MAX\nMinimum Fail Safe Setting Depth (TVD ft). Based on Salt Water (8.6ppg or\n0.45 psi/ft) in Control Line: 4400\nSafety Valve Full Opening\nPressure (psi) : 3000 + SITP\nSafety Valve start to Close Pressure(psi) : 1300 + SIT\nControl Line Fluid : Texaco Rando HD32\nCleanliness of Hydraulic chamber : NAS 6\nThe WRSCSSSV shall operate with the same surface control system and\ncontrol line as the TRSCSSV when installed: YES\nMinimum Control Line Chamber Rating(psi) : 9000\nThe valve must be tested according to API 14A class 3S. : YES\nPart#H82760****\n","\"WIRELINE RETRIEVEABLE SURFACE CONTROLLED SUBSURFACE SAFETY VALVE\nModel: TAOFWSE-5\nSize (in.): 5-1/2\"\"\nMin. internal Working Pressure (psi) : 5000\nEqualizing Mechanism: Self-Equalizing Thru-Rapper, Poppet Type\nLock-Type : 4.562 BA\nMin ID (in.): 2.562\nMax OD (in.): 4.640\nMetallurgy : 13 CR 80 MYS 22 HRC MAX\nMinimum Fail Safe Setting Depth (TVD ft). Based on Salt Water (8.6ppg or\n0.45 psi/ft) in Control Line: 4400\nSafety Valve Full Opening\nPressure (psi) : 3000 + SITP\nSafety Valve start to Close Pressure(psi) : 1300 + SIT\nControl Line Fluid : Texaco Rando HD32\nCleanliness of Hydraulic chamber : NAS 6\nThe WRSCSSSV shall operate with the same surface control system and\ncontrol line as the TRSCSSV when installed: YES\nMinimum Control Line Chamber Rating(psi) : 9000\nThe valve must be tested according to API 14A class 3S. : YES\nPart#H82760****\n","","13 May 2017 PO Long Text as per below:\nWIRELINE RETRIEVEABLE SURFACE CONTROLLED SUBSURFACE SAFETY VALVE\nModel: TAOFWSE-5\nSize (in.): 5-1/2\"\"\nMin. internal Working Pressure (psi) : 5000\nEqualizing Mechanism: Self-Equalizing Thru-Rapper, Poppet Type\nLock-Type : 4.562 BA\nMin ID (in.): 2.562\nMax OD (in.): 4.640\nMetallurgy : 13 CR 80 MYS 22 HRC MAX\nMinimum Fail Safe Setting Depth (TVD ft). Based on Salt Water (8.6ppg or\n0.45 psi/ft) in Control Line: 4400\nSafety Valve Full Opening\nPressure (psi) : 3000 + SITP\nSafety Valve start to Close Pressure(psi) : 1300 + SIT\nControl Line Fluid : Texaco Rando HD32\nCleanliness of Hydraulic chamber : NAS 6\nThe WRSCSSSV shall operate with the same surface control system and\ncontrol line as the TRSCSSV when installed: YES\nMinimum Control Line Chamber Rating(psi) : 9000\nThe valve must be tested according to API 14A class 3S. : YES\nPart#H82760****\n","","","","","-","-","PD",0,0,0,0.01]
[1000648,"VLV,WR-SCSSV,TXVHDE,3-1/2\",13CR","VLV","VALVE","EA","COM","","","","13 May 2017 PO Long Text as per below:\nWIRELINE RETRIEVABLE SURFACE CONTROLLED SUB SURFACE SAFETY VALVE\nModel: TXVHDE\nSize (in.): 3-1/2\nMin. internal Working Pressure (psi) : 5,000\nEqualizing Mechanism:  Self-Equalizing Thru-Rapper, Poppet Type\nLock-Type: 2.812 AOF\nMin ID (in.) : 1.250\nMax OD (in.) : 2.865\nMetallurgy : 13 CR 80 MYS 22 HRC MAX\nMinimum Fail Safe Setting Depth (TVDft). Based on Salt Water (8.6ppg or\n0.45psi/ft) in Control Line : 4000\nSafety Valve Full Opening Pressure (psi) : 3360 + SITP\nSafety Valve start to Close Pressure : 1520 + SITP\nControl Line Fluid Texaco : Rando HD32\nCleanliness of Hydraulic chamber : NAS 6\nThe WRSCSSV shall operate with the same surface control system and\ncontrol line as the TRSCSSV when installed : YES\nMinimum Control Line Chamber Rating (psi): 15000\nThe valve must be tested according to API 14A class 3S : YES\"\nPart#H82556****","WIRELINE RETRIEVABLE SURFACE CONTROLLED SUB SURFACE SAFETY VALVE\nModel: TXVHDE\nSize (in.): 3-1/2\nMin. internal Working Pressure (psi) : 5,000\nEqualizing Mechanism:  Self-Equalizing Thru-Rapper, Poppet Type\nLock-Type: 2.812 AOF\nMin ID (in.) : 1.250\nMax OD (in.) : 2.865\nMetallurgy : 13 CR 80 MYS 22 HRC MAX\nMinimum Fail Safe Setting Depth (TVDft). Based on Salt Water (8.6ppg or\n0.45psi/ft) in Control Line : 4000\nSafety Valve Full Opening Pressure (psi) : 3360 + SITP\nSafety Valve start to Close Pressure : 1520 + SITP\nControl Line Fluid Texaco : Rando HD32\nCleanliness of Hydraulic chamber : NAS 6\nThe WRSCSSV shall operate with the same surface control system and\ncontrol line as the TRSCSSV when installed : YES\nMinimum Control Line Chamber Rating (psi): 15000\nThe valve must be tested according to API 14A class 3S : YES\"\nPart#H82556****","","13 May 2017 PO Long Text as per below:\nWIRELINE RETRIEVABLE SURFACE CONTROLLED SUB SURFACE SAFETY VALVE\nModel: TXVHDE\nSize (in.): 3-1/2\nMin. internal Working Pressure (psi) : 5,000\nEqualizing Mechanism:  Self-Equalizing Thru-Rapper, Poppet Type\nLock-Type: 2.812 AOF\nMin ID (in.) : 1.250\nMax OD (in.) : 2.865\nMetallurgy : 13 CR 80 MYS 22 HRC MAX\nMinimum Fail Safe Setting Depth (TVDft). Based on Salt Water (8.6ppg or\n0.45psi/ft) in Control Line : 4000\nSafety Valve Full Opening Pressure (psi) : 3360 + SITP\nSafety Valve start to Close Pressure : 1520 + SITP\nControl Line Fluid Texaco : Rando HD32\nCleanliness of Hydraulic chamber : NAS 6\nThe WRSCSSV shall operate with the same surface control system and\ncontrol line as the TRSCSSV when installed : YES\nMinimum Control Line Chamber Rating (psi): 15000\nThe valve must be tested according to API 14A class 3S : YES\"\nPart#H82556****","","","","","-","-","PD",0,0,0,0.01]
[1000650,"VLV, ICD W/SLEEVE,4.5\" SLHT BXP 13CR","VLV","VALVE","EA","COM","","","","13 May 2017 PO Long Text as per below:\nINFLOW CONTROL VALVE -W- WITH SLIDING SLEEVE\nSize: 4-1/2\"\nWeight: 12.6 PPF\nConnection: SLHT BXP, HB-3 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX","INFLOW CONTROL VALVE -W- WITH SLIDING SLEEVE\nSize: 4-1/2\"\nWeight: 12.6 PPF\nConnection: SLHT BXP, HB-3 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX\n\n","","13 May 2017 PO Long Text as per below:\nINFLOW CONTROL VALVE -W- WITH SLIDING SLEEVE\nSize: 4-1/2\"\nWeight: 12.6 PPF\nConnection: SLHT BXP, HB-3 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX","","","","","-","-","PD",0,0,0,0.01]
[1000651,"VLV, ICD W/SLEEVE,5.5\" SLHT BXP 13CR","VLV","VALVE","EA","COM","","","","13 May 2017 PO Long Text as per below:\nINFLOW CONTROL VALVE -W- WITH SLIDING SLEEVE\nSize: 5-1/2\"\nWeight: 15.5 PPF\nConnection: SLHT BXP, HB-2 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX","INFLOW CONTROL VALVE -W- WITH SLIDING SLEEVE\nSize: 5-1/2\"\nWeight: 15.5 PPF\nConnection: SLHT BXP, HB-2 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX\n\n","","13 May 2017 PO Long Text as per below:\nINFLOW CONTROL VALVE -W- WITH SLIDING SLEEVE\nSize: 5-1/2\"\nWeight: 15.5 PPF\nConnection: SLHT BXP, HB-2 SHIFTING TOOL OPERATED\nMetallurgy: 13 CR\nPart#H48688XXX","","","","","-","-","PD",0,0,0,0.01]
[1000661,"BOX:GLV,101X224X476MM,ASDCA-10-S07052-0>",null,null,"EA","PPE","4000822","CATU","CG-35/2","BOX:\nTYPE: GLOVES\nSIZE: 101X224X476MM\nDRAWING/DOCUMENT REFERENCE-1: ASDCA-10-S07052-0002_SH.5,11","FOR RUBBER INSULATING GLOVES,\nWITH PROTECTION WINDOW,\nINC. BOTTLE OF TALCUM POWDER\n","","","","","","","BOX:\nTYPE: GLOVES\nSIZE: 101X224X476MM\nDRAWING/DOCUMENT REFERENCE-1: ASDCA-10-S07052-0002_SH.5,11","ZGMD_BX_NM","V1",0,2,3,130.17]
[1000662,"(BLCK)SHIELD:SAF/EQ;F PROT,100% UV PROT",null,null,"EA","PPE","4000822","CATU","MO-184","SHIELD:SAFETY EQUIPMENT;\nTYPE: FACE PROTECTION\nMATERIAL: 100% UV PROTECTION","ADJUSTABLE ON HELMET\n\n","","","06","","1000510","","SHIELD:SAFETY EQUIPMENT;\nTYPE: FACE PROTECTION\nMATERIAL: 100% UV PROTECTION","ZGMD_SHIELD_SAF_EQ","PD",0,0,0,99.06]
[1000670,"HELMET:SAF V-GARD 930 WHT VENTED",null,null,"EA","PPE","","","","HELMET:\nTYPE: SAFETY V-GARD 930 WHITE VENTED","RATCHET SYSTEM AND OVER SPECTACLES\n504G\nLOGO\n","","\"HELMET, SAFETY VGARD 390 WHITE VENTED\nRATCHET SYSTEM AND OVER SPECTACLES\n504G\nLOGO","","","","1000499","HELMET:\nTYPE: SAFETY V-GARD 930 WHITE VENTED","ZGMD_HELM_NM","V1",0,100,250,{"v":37,"d":"37.00"}]
[1000671,"HELMET:SAF V-GARD 930 RD VENTED",null,null,"EA","PPE","","","","HELMET:\nTYPE: SAFETY V-GARD 930 RED VENTED","RATCHET SYSTEM AND OVER SPECTACLES\n504G\nLOGO\n","","","","","","1000498","HELMET:\nTYPE: SAFETY V-GARD 930 RED VENTED","ZGMD_HELM_NM","V1",0,8,25,37.23]
[1000672,"CHIN STRAP, SUITABLE FOR  V-GARD 930",null,null,"EA","PPE","","","","CHIN STRAP FOR SAFETY HELMET V GARD 930\n","CHIN STRAP FOR SAFETY HELMET V GARD 930\n\n","","","04","01","1000459","","-","-","PD",0,0,0,0.92]
[1000673,"C/L:0.25\"OD X 0.049\" WT,BARE,316L,NAS 1>",null,null,"FT","COM","4000009","SCHLUMBERGER USA","101115023","CONTROL LINE:\nSIZE: 0.25\"OD X 0.049\" WT\nTYPE: BARE\nMATERIAL: 316L\nFLUSHING/FILLING STANDARD: NAS 1638 CLASS 5\nFILLING TYPE: TEXACO RANDO OIL HDZ 15\nPACKING: WOODEN DRUM  36\" X 32\"\n\n","Bare Control Line (WT 0,049; 316L)\nSize (in.): 0.25\"\"\nMax Line OD (in.) : 0.25\"\"\nMin. Working Pressure (psi): 8,744\nTest Pressure (psi): 12,000\nMetallurgy : 316L\nWall Thickness (in.): 0.049\"\" WT\nInternal Cleanliness: Texaco Rando Oil HDZ 15,NAS 1638 class 5\nStorage Wooden drum : 36\" x 32\"\"\nPrinted Incremental Length: Mandatory\nManufacture: Welded and cold plug drawn, bright annealed tubing. Each\nend of the control line tube sealed off with stainless steel compression\nfitting pressure rated to test integrity of the control line, ends\ncovered with rubber sealant.\n\n\n","","22 May 2017 PO Long Text as per below:\nBare Control Line (WT 0,049; 316L)\nSize (in.): 0.25\"\"\nMax Line OD (in.) : 0.25\"\"\nMin. Working Pressure (psi): 8,744\nTest Pressure (psi): 12,000\nMetallurgy : 316L\nWall Thickness (in.): 0.049\"\" WT\nInternal Cleanliness: Texaco Rando Oil HDZ 15,NAS 1638 class 5\nStorage Wooden drum : 36\"\" x 32\"\"\nPrinted Incremental Length: Mandatory\nManufacture: Welded and cold plug drawn, bright annealed tubing. Each\nend of the control line tube sealed off with stainless steel compression\nfitting pressure rated to test integrity of the control line, ends\ncovered with rubber sealant.\"\n\n\n","","","","","CONTROL LINE:\nSIZE: 0.25\"OD X 0.049\" WT\nTYPE: BARE\nMATERIAL: 316L\nFLUSHING/FILLING STANDARD: NAS 1638 CLASS 5\nFILLING TYPE: TEXACO RANDO OIL HDZ 15\nPACKING: WOODEN DRUM  36\" X 32\"\n\n","ZGMD_C_L_NM","PD",0,0,0,0.01]
[1000674,"C/L,CLAMP,3.5\",1X(11X36)MM+2X(11x11)MM",null,null,"EA","COM","4000009","SCHLUMBERGER USA","3500-146","22 May 2017 PO Long Text as per below:\nControl Line Clamps (3 1/2\"\")\nSize (in.): 3-1/2\"\"\nControl lines accommodation: 1 x 11mm x 36 mm Quad Pack, 2 x 11mm x 1mm\nsingle encapsulated Control lines, and one 1/4\"\" bare control line\nsimultaneously\nMetallurgy Cast Iron\nClosing feature: Toggle type\n","Control Line Clamps (3 1/2\"\")\nSize (in.): 3-1/2\"\"\nControl lines accommodation: 1 x 11mm x 36 mm Quad Pack, 2 x 11mm x 1mm\nsingle encapsulated Control lines, and one 1/4\"\" bare control line\nsimultaneously\nMetallurgy Cast Iron\nClosing feature: Toggle type\n","","22 May 2017 PO Long Text as per below:\nControl Line Clamps (3 1/2\")\nSize (in.): 3-1/2\"\"\nControl lines accommodation: 1 x 11mm x 36 mm Quad Pack, 2 x 11mm x 1mm\nsingle encapsulated Control lines, and one 1/4\"\" bare control line\nsimultaneously\nMetallurgy Cast Iron\nClosing feature: Toggle type\n","","","","","-","-","PD",0,0,0,0.01]
[1000675,"C/L,CLAMP,4.5\",1X(11X36)MM+2X(11x11)MM",null,null,"EA","COM","4000009","SCHLUMBERGER USA","AS-4500-1529","22 May 2017 PO Long Text as per below:\nControl Line Clamps (4-1/2\")\nSize (in.) : 4-1/2\"\"\nControl lines accommodation: 1 x 11mm x 36 mm Quad Pack, 2 x 11mm x 1mm\nsingle encapsulated Control lines,and one 1/4\"\" bare control line\nsimultaneously\nMetallurgy: Low Friction type\nClosing feature:  Toggle Type\n","Control Line Clamps (4-1/2\")\nSize (in.) : 4-1/2\"\"\nControl lines accommodation: 1 x 11mm x 36 mm Quad Pack, 2 x 11mm x 1mm\nsingle encapsulated Control lines,and one 1/4\"\" bare control line\nsimultaneously\nMetallurgy: Low Friction type\nClosing feature:  Toggle Type\n","","22 May 2017 PO Long Text as per below:\nControl Line Clamps (4-1/2\")\nSize (in.) : 4-1/2\"\"\nControl lines accommodation: 1 x 11mm x 36 mm Quad Pack, 2 x 11mm x 1mm\nsingle encapsulated Control lines,and one 1/4\"\" bare control line\nsimultaneously\nMetallurgy: Low Friction type\nClosing feature:  Toggle Type\n","","","","","-","-","PD",0,0,0,0.01]
[1000676,"C/L,CLAMP,7\",1X(11X36)MM+2X(11x11)MM",null,null,"EA","COM","4000009","SCHLUMBERGER USA","AS-7000-1068","22 May 2017 PO Long Text as per below:\nControl Line Clamps (7\")\nSize (in.): 7\"\"\nControl lines accommodation\n1 x 11mm x 36 mm Quad Pack, 2 x 11mm x 1mm single encapsulated Control\nlines, and one 1/4\"\" bare control line simultaneously\nMetallurgy Low Friction: type\nClosing feature :Toggle Type\n","Control Line Clamps (7\")\nSize (in.): 7\"\"\nControl lines accommodation\n1 x 11mm x 36 mm Quad Pack, 2 x 11mm x 1mm single encapsulated Control\nlines, and one 1/4\"\" bare control line simultaneously\nMetallurgy Low Friction: type\nClosing feature :Toggle Type\n","","22 May 2017 PO Long Text as per below:\nControl Line Clamps (7\")\nSize (in.): 7\"\"\nControl lines accommodation\n1 x 11mm x 36 mm Quad Pack, 2 x 11mm x 1mm single encapsulated Control\nlines, and one 1/4\"\" bare control line simultaneously\nMetallurgy Low Friction: type\nClosing feature :Toggle Type\n","","","","","-","-","PD",0,0,0,0.01]
[1000677,"C/L:0.25\"OD X 0.049\" WT,ENCP,QUAD,825 I>",null,null,"FT","COM","4000009","SCHLUMBERGER USA","RR101115049","CONTROL LINE:\nSIZE: 0.25\"OD X 0.049\" WT\nTYPE: ENCAPSULATED, QUAD\nMATERIAL: 825 INC\nENCAPSULATION SECTION SIZE: 35MM X 11MM\nENCAPSULATION MATERIAL: RILSAN 11 (TT200)\nFLUSHING/FILLING STANDARD: NAS 1638 CLASS 5\nFILLING TYPE: TEXACO RANDO OIL HDZ 15\nPACKING: WOODEN DRUM  36\" X 32\"\n","Encapsulated, Quad, Control Line:\nSize (in.): 1/4\"\" x 4\nMax Line OD (in.): 0.25\"\"\nMM. Working Pressure (psi): 10,000\nTest Pressure (psi): 13,688\nMetallurgy: 825 Inc\nWall Thickness (In.): 0.049\nInternal Cleanliness: Texaco Rando Oil HDZ 15, NAS 1638 class 5\nStorage: Wooden drum 36\"\" x 32\"\"\nPrinted Incremental Length: Confirmed\nManufacture: Welded and cold plug drawn,bright annealed tubing. Each end\nof the control line tube sealed off with stainless steel compression\nfitting pressure rated to test integrity of the control line, ends\ncovered with rubber sealant.\nEncapsulation: Rilsan 11 (TT200), 35mm x11mm\nColor code : Confirmed\nTemperature rating (degrees F): 200\n","","22 May 2017 PO Long Text as per below:\n\"Encapsulated, Quad, Control Line:\nSize (in.): 1/4\"\" x 4\nMax Line OD (in.): 0.25\"\"\nMM. Working Pressure (psi): 10,000\nTest Pressure (psi): 13,688\nMetallurgy: 825 Inc\nWall Thickness (In.): 0.049\nInternal Cleanliness: Texaco Rando Oil HDZ 15, NAS 1638 class 5\nStorage: Wooden drum 36\"\" x 32\"\"\nPrinted Incremental Length: Confirmed\nManufacture: Welded and cold plug drawn,bright annealed tubing. Each end\nof the control line tube sealed off with stainless steel compression\nfitting pressure rated to test integrity of the control line, ends\ncovered with rubber sealant.\nEncapsulation: Rilsan 11 (TT200), 35mm x11mm\nColor code : Confirmed\nTemperature rating (degrees F) : 200\n","","","","","CONTROL LINE:\nSIZE: 0.25\"OD X 0.049\" WT\nTYPE: ENCAPSULATED, QUAD\nMATERIAL: 825 INC\nENCAPSULATION SECTION SIZE: 35MM X 11MM\nENCAPSULATION MATERIAL: RILSAN 11 (TT200)\nFLUSHING/FILLING STANDARD: NAS 1638 CLASS 5\nFILLING TYPE: TEXACO RANDO OIL HDZ 15\nPACKING: WOODEN DRUM  36\" X 32\"\n","ZGMD_C_L_NM","PD",0,0,0,0.01]
[1000678,"CABLE,11X11MM ENCP,316L,WT 0.028\"",null,null,"FT","DRL","4000009","SCHLUMBERGER USA","P485879","22 May 2017 PO Long Text as per below:\nEncapsulated Downhole Gauge Cable (WT 0.028\"; 316L)\nType: 100% solid copper conductor,encased In 1/4\"\" OD 316L SS encaps 11\nX 11 with POLYPROPYLENE fill\nWall Thickness (in): 0,028\"\"\nLength: To be specified upon ORDER\nWorking Pressure (psi) :10,000\n","Encapsulated Downhole Gauge Cable (WT 0.028\"; 316L)\nType: 100% solid copper conductor,encased In 1/4\"\" OD 316L SS encaps 11\nX 11 with POLYPROPYLENE fill\nWall Thickness (in): 0,028\"\"\nLength: To be specified upon ORDER\nWorking Pressure (psi) :10,000\n","","22 May 2017 PO Long Text as per below:\nEncapsulated Downhole Gauge Cable (WT 0.028\"; 316L)\nType: 100% solid copper conductor,encased In 1/4\"\" OD 316L SS encaps 11\nX 11 with POLYPROPYLENE fill\nWall Thickness (in): 0,028\"\"\nLength: To be specified upon ORDER\nWorking Pressure (psi) :10,000\n","","","","","-","-","PD",0,0,0,0.01]
[1000679,"CABLE:ENCP DHG,11X11MM ENCAPS,WT 0.035\">",null,null,"FT","DRL","4000009","SCHLUMBERGER USA","P486035","CABLE:\nTYPE: ENCAPSULATED DOWNHOLE GAUGE\nSIZE: 11X11MM ENCAPS, WT 0.035\"\nMATERIAL: 100% SOLID COPPER CONDUCTOR\nLENGTH: 21,000 FT\n","ENCAPSULATED DOWNHOLE GAUGE CABLE\nTYPE: 100% SOLID COPPER CONDUCTOR , ENCASED IN 1/4\" OD 316L SS\nENCAPS 11 X 11 WITH POLYPROPYLENE FILL\nWALL THICKNESS - 0.035\"\"\nWORKING PRESSURE - 10,000 PSI\n21,000 FT OF DOWNHOLE GAUGE CABLE WRAPPED ON EACH STEEL DRUM\"\n","","22 May 2017 PO Long Text as per below:\nENCAPSULATED DOWNHOLE GAUGE CABLE\nTYPE - 100% SOLID COPPER CONDUCTOR , ENCASED IN 1/4\" OD 316L SS\nENCAPS 11 X 11 WITH POLYPROPYLENE FILL\nWALL THICKNESS - 0.035\"\"\nWORKING PRESSURE - 10,000 PSI\n21,000 FT OF DOWNHOLE GAUGE CABLE WRAPPED ON EACH STEEL DRUM\"\n","","","","","CABLE:\nTYPE: ENCAPSULATED DOWNHOLE GAUGE\nSIZE: 11X11MM ENCAPS, WT 0.035\"\nMATERIAL: 100% SOLID COPPER CONDUCTOR\nLENGTH: 21,000 FT\n","ZGMD_CBL_NM","PD",0,0,0,0.01]
[1000680,"CABLE:SURF CBL,2 MMX1.5MM,250 V",null,null,"FT","COM","4000009","SCHLUMBERGER USA","A10BZ-01015T-B-02","CABLE:\nTYPE: SURFACE CABLE\nSIZE: 2 MMX1.5MM\nVOLTAGE: 250 VOLT\n","SURFACE CABLE FOR SCHLUMBERGER XDPG-CA DIGITAL PERMANENT GAUGE\nSECTION: 2 MM x 1.5MM 250 VOLT SCREENED BFOB INSTRUMENT CABLE WITH BLACK\nSHEATH FIRE RESISTANT TO IEC6 331\nTEMPERATURE RATING: 90°C MAXIMUM\n","","22 May 2017 PO Long Text as per below:\nSURFACE CABLE FOR SCHLUMBERGER XDPG-CA DIGITAL PERMANENT GAUGE\nSection: 2 MMx1.5MM 250 VOLT SCREENED BFOB INSTRUMENT CABLE WITH BLACK\nSHEATH FIRE RESISTANT TO IEC6 331 TEMPERATURE RATING: 90°C MAXIMUM\"\n","","","","","CABLE:\nTYPE: SURFACE CABLE\nSIZE: 2 MMX1.5MM\nVOLTAGE: 250 VOLT\n","ZGMD_CBL_NM","PD",0,0,0,0.01]
[1000681,"UNIT:SURF ACQ",null,null,"EA","INS","4000009","SCHLUMBERGER USA","101022253","UNIT:\nTYPE: SURFACE ACQUISITION\nATEX: N/A","SURFACE ACQUISITION UNIT (WELLWATCHER ARCONN NG)\nDATA ACQUISITION 1 DATASET / SEC. OR BETTER\nPOWER FAILURE INDICATOR LED\nPOWER REQUIREMENTS 110-240 V AC 50/60 HZ\nBATTERY BACK UP 12 VDC, 1.2 AMP HOUR CAPACITY\nUNIT SUPPLIED WITH 4 FIC CARDS (P/N 101022827)\nCOMMUNICATION CARD ISOLATED RS232/ RS-485 (P/N 101120028)\nDIMENSION: 7.25\" X 19\" X 15.75\" WHICH FITS 19\" RACK MOUNT\nAPPROX SHIPPING WEIGHT: 30 LBM\nNO OF CHANNELS: 4 (DEFAULT) UP TO 16. ONE INTERFACE CARD PER CHANNEL\nNO. OF GAUGES: UP TO 8 PER CHANNEL\nGAUGES SUPPORTED: NPQG, DPGTA, XPQG\n\nREFER ATTACHED DOCUMENT","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","22 May 2017 PO Long Text as per below:\nSurface Acquisition (Arconn Wellwatcher NG)\nData acquisition 1 dataset / sec. or better\nPower failure indicator LED\nPower requirements 110-240 VAC 50 - 60 Hz; 4 FIC Cards\nBattery back up 12 Vdc, 1.2 Amp hour capacity\n","","","","","UNIT:\nTYPE: SURFACE ACQUISITION\nATEX: N/A","ZGMD_UNIT_NM","PD",1,0,0,{"v":38040.8,"d":"38,040.80"}]
[1000682,"GAUGE:MNDRL;3.5\",9.2#,3-1/2\" 9.2 LB/FT >",null,null,"EA","COM","4000009","SCHLUMBERGER USA","100953716_XX_EXT","GAUGE:MANDREL;\nSIZE: 3.5\"\nWEIGHT: 9.2#\nTHREAD UP: 3-1/2\" 9.2 LB/FT SL-APEX BOX\nTHREAD DOWN: 3-1/2\" 9.2 LB/FT SL-APEX PIN\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 2.902\"\nDRIFT: 2.867\"\nMATERIAL: 13% CR 80 KSI 18-22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","Permanent Gauge Mandrel - External Reading\nMax OD (in.), combined with 5 x Encapsulated control lines: 5.28\nMandrel: Long tapers, longitudinal slot for 5 chemical Injection/control\nlines (11mm x 11mm)\nMetallurgy : 13% Cr 80 ksi 18-22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb): 4,000\nTensile Strength thru Body (Ibs): 239,800\n","","22 May 2017 PO Long Text as per below:\n\"Permanent Gauge Mandrel - External Reading\nSize (in.):3-1/2\"\"\nMin. Working Pressure (psi): 5,000\nMax OD (in.), combined with 5 x Encapsulated control lines: 5.28\nMin ID (In.): 2.902\nDrift (in.): 2.867\nTemp rating (degrees F) : 300\nGauge Installation :External\nMandrel: Long tapers, longitudinal slot for 5 chemical Injection/control\nlines (11mm x 11mm)\nSurface Testing Feature: Yes\nThread Up : 3-1/2\"\" 9.2 lb/ft SL-APEX Box\nThread Down : 3-1/2\"\" 9.2 lb/ft SL-APEX Pin\nMetallurgy : 13% Cr 80 ksi 18-22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb): 4,000\nTensile Strength thru Body (Ibs): 239,800\n","","","","","GAUGE:MANDREL;\nSIZE: 3.5\"\nWEIGHT: 9.2#\nTHREAD UP: 3-1/2\" 9.2 LB/FT SL-APEX BOX\nTHREAD DOWN: 3-1/2\" 9.2 LB/FT SL-APEX PIN\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 2.902\"\nDRIFT: 2.867\"\nMATERIAL: 13% CR 80 KSI 18-22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","ZGMD_GGE_MANDREL","PD",0,0,0,0.01]
[1000683,"GAUGE:MNDRL;3-1/2\",3-1/2\" 9.2 LB/FT SL->",null,null,"EA","COM","4000009","SCHLUMBERGER USA","100953716_XX_INT OR 103201255","GAUGE:MANDREL;\nSIZE: 3-1/2\"\nTHREAD UP: 3-1/2\" 9.2 LB/FT SL-APEX BOX\nTHREAD DOWN: 3-1/2\" 9.2 LB/FT SL-APEX PIN\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 2.898\"\nDRIFT: 2.867\"\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\n","Permanent Gauge Mandrel - Internal Reading\nMax OD (in.), combined with 5 x Encapsulated control lines. : 5.28\nMin ID (in.): 2.898\nMandrel : Long tapers, longitudinal slot for 5 chemical\nInjection/control lines (11mm x 11mm)\nMetallurgy : 13% Cr 80 ksi 18-22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb): 4,000\nTensile Strength thru Body (Ibs): 237,600\n","","22 May 2017 PO Long Text as per below:\nPermanent Gauge Mandrel - Internal Reading\nSize (in.) : 3-1/2\"\"\nMin. Working Pressure (psi): 5,000\nMax OD (in.), combined with 5 x Encapsulated control lines. : 5.28\nMin ID (in.): 2.898\nDrift (in.) : 2.867\nTemp rating (degrees F) : 300\nGauge installation : External\nMandrel : Long tapers, longitudinal slot for 5 chemical\nInjection/control lines (11mm x 11mm)\nSurface Testing Feature : Yes\nThread Up : 3-1/2\"\" 9.2 lb/ft SL-APEX Box\nThread Down : 3-1/2\"\" 9.2 lb/ft SL-APEX Pin\nMetallurgy : 13% Cr 80 ksi 18-22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb): 4,000\nTensile Strength thru Body (Ibs): 237,600\n","","","","","GAUGE:MANDREL;\nSIZE: 3-1/2\"\nTHREAD UP: 3-1/2\" 9.2 LB/FT SL-APEX BOX\nTHREAD DOWN: 3-1/2\" 9.2 LB/FT SL-APEX PIN\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 2.898\"\nDRIFT: 2.867\"\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\n","ZGMD_GGE_MANDREL","PD",0,0,0,{"v":12576.9,"d":"12,576.90"}]
[1000684,"GAUGE:MNDRL;3.5\",9.2#,3-1/2\" 9.2 LB/FT >",null,null,"EA","COM","4000009","SCHLUMBERGER USA","RR100911758","GAUGE:MANDREL;\nSIZE: 3.5\"\nWEIGHT: 9.2#\nTHREAD UP: 3-1/2\" 9.2 LB/FT SL-APEX BOX\nTHREAD DOWN: 3-1/2\" 9.2 LB/FT SL-APEX PIN\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 2.902\"\nDRIFT: 2.867\"\nMATERIAL: 13% CR 80 KSI 18-22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","Permanent Dual Gauge Mandrel - Internal <(>&<)> External Reading\nMax OD (in.), combined with 5 xEncapsulated control lines: 5.384\nMandrel: Long tapers longitudinal slot for 5 chemical Injection/control\nlines (11mm x 11mm)\nTorsional Yield Strength thru Body (ft-lb): 4,000\nTensile Strength thru Body (Ibs):260,000\n","","22 May 2017 PO Long Text as per below:\nPermanent Dual Gauge Mandrel - Internal <(>&<)> External Reading\nSize (in.): 3-1/2\"\"\nMin. Working Pressure (psi): 5,000\nMax OD (in.), combined with 5 xEncapsulated control lines: 5.384\nMin ID (in.): 2.902\nDrift (in.): 2.867\nTemp rating (degrees F) : 300\nGauge Installation: External\nMandrel: Long tapers longitudinal slot for 5 chemical Injection/control\nlines (11mm x 11mm)\nSurface Testing Feature: Yes\nThread Up: 3-1/2\"\" 9.2 lb/ft SL-APEX Box\nThread Down:  3-1/2\"\" 9.2 lb/ft SL-APEX Pin\nMetallurgy : 13% Cr 80 ksi 18-22 HRC to\nNACE MR 0175\nTorsional Yield Strength thru Body (ft-lb): 4,000\nTensile Strength thru Body (Ibs):260,000\n","","","","","GAUGE:MANDREL;\nSIZE: 3.5\"\nWEIGHT: 9.2#\nTHREAD UP: 3-1/2\" 9.2 LB/FT SL-APEX BOX\nTHREAD DOWN: 3-1/2\" 9.2 LB/FT SL-APEX PIN\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 2.902\"\nDRIFT: 2.867\"\nMATERIAL: 13% CR 80 KSI 18-22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","ZGMD_GGE_MANDREL","PD",0,0,0,0.01]
[1000685,"GAUGE:MNDRL;4.5\",12.6#,4-1/2\" 12.6 LB/F>",null,null,"EA","COM","4000009","SCHLUMBERGER USA","RR100940583","GAUGE:MANDREL;\nSIZE: 4.5\"\nWEIGHT: 12.6#\nTHREAD UP: 4-1/2\" 12.6 LB/FT SL-APEX BOX\nTHREAD DOWN: 4-1/2\" 12.6 LB/FT SL-APEX PIN\nPRESSURE RATING: 8000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 3.864\"\nDRIFT: 3.833\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","Permanent Dual Gauge Mandrel - External Reading\nMax OD (In.), combined with 5 x Encapsulated control lines: 6.515\nMandrel: Long tapers, longitudinal slot for 5 chemical injection/control\nlines (11mm x 11mm)\nTorsional Yield Strength thru Body (ft-lb) : 5,225\nTensile Strength thru Body (Ibs) : 680,700\"\n","","22 May 2017 PO Long Text as per below:\nPermanent Dual Gauge Mandrel - External Reading\nSize (in.): 4-1/2\"\"\nMin. Working Pressure (psi): 8,000\nMax OD (In.), combined with 5 x Encapsulated control lines: 6.515\nMin ID (In.) : 3.864\nDrift (In.) : 3.833\nTemp rating (degrees F) : 300\nGauge installation : External\nMandrel: Long tapers, longitudinal slot for 5 chemical injection/control\nlines (11mm x 11mm)\nSurface Testing Feature : Yes\nThread Up:  4-1/2\"\" 12.6 lb/ft SL-APEX Box\nThread Down : 4-1/2\"\" 12.6 lb/ft SL-APEX Pin\nMetallurgy : 13% Cr 80 ksi 18 - 22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb) : 5,225\nTensile Strength thru Body (Ibs) : 680,700\"\n","","","","","GAUGE:MANDREL;\nSIZE: 4.5\"\nWEIGHT: 12.6#\nTHREAD UP: 4-1/2\" 12.6 LB/FT SL-APEX BOX\nTHREAD DOWN: 4-1/2\" 12.6 LB/FT SL-APEX PIN\nPRESSURE RATING: 8000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 3.864\"\nDRIFT: 3.833\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","ZGMD_GGE_MANDREL","PD",0,0,0,0.01]
[1000686,"GAUGE:MNDRL;4.5\",12.6#,4-1/2\" 12.6 LB/F>",null,null,"EA","COM","4000009","SCHLUMBERGER USA","RR100925405","GAUGE:MANDREL;\nSIZE: 4.5\"\nWEIGHT: 12.6#\nTHREAD UP: 4-1/2\" 12.6 LB/FT SL-APEX BOX\nTHREAD DOWN: 4-1/2\" 12.6 LB/FT SL-APEX PIN\nPRESSURE RATING: 6,700 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 3.855\"\nDRIFT: 3.833\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","Permanent Dual Gauge Mandrel - Internal <(>&<)> External Reading\nMax OD (In.), combined with 5 x Encapsulated control lines. : 5.938\nMandrel: Long tapers, longitudinal slot for 5 chemical injection/control\nlines (11mm x 11mm)\nTorsional Yield Strength thru Body (ft-lb) : 5,225\nTensile Strength thru Body (Ibs) : 337,900\"\n","","22 May 2017 PO Long Text as per below:\n\"Permanent Dual Gauge Mandrel - Internal <(>&<)> External Reading\nSize (in.): 4-1/2\"\"\nMin. Working Pressure (psi): 6,700\nMax OD (In.), combined with 5 x Encapsulated control lines. : 5.938\nMin ID (In.) : 3.855\nDrift (In.) : 3.833\nTemp rating (degrees F) : 300\nGauge installation: External\nMandrel: Long tapers, longitudinal slot for 5 chemical injection/control\nlines (11mm x 11mm)\nSurface Testing Feature Yes\nThread Up : 4-1/2\"\" 12.6 lb/ft SL-APEX Box\nThread Down:  4-1/2\"\" 12.6 lb/ft SL-APEX Pin\nMetallurgy : 13% Cr 80 ksi 18 - 22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb) : 5,225\nTensile Strength thru Body (Ibs) : 337,900\"\n","","","","","GAUGE:MANDREL;\nSIZE: 4.5\"\nWEIGHT: 12.6#\nTHREAD UP: 4-1/2\" 12.6 LB/FT SL-APEX BOX\nTHREAD DOWN: 4-1/2\" 12.6 LB/FT SL-APEX PIN\nPRESSURE RATING: 6,700 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 3.855\"\nDRIFT: 3.833\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","ZGMD_GGE_MANDREL","PD",0,0,0,0.01]
[1000687,"GAUGE:MNDRL;5.5\",15.5#,5-1/2\" 15.5 LB/F>",null,null,"EA","COM","4000009","SCHLUMBERGER USA","RR100923125","GAUGE:MANDREL;\nSIZE: 5.5\"\nWEIGHT: 15.5#\nTHREAD UP: 5-1/2\" 15.5 LB/FT SL-APEX BOX\nTHREAD DOWN: 5-1/2\" 15.5 LB/FT SL-APEX PIN\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 4.892\"\nDRIFT: 4.825\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","Permanent Gauge Mandrel - External Reading\nMax OD (In.), combined with 5 x Encapsulated control lines. : 7.396\nMandrel: Long tapers, longitudinal slot for 5 chemical injection/control\nlines (11mm x 11mm)\nTorsional Yield Strength thruBody (ft-lb) : 8,995\nTensile Strength thru Body (Ibs) : 687,259\"\n","","22 May 2017 PO Long Text as per below:\nPermanent Gauge Mandrel - External Reading\nSize (In.): 5.5\"\"\nMin. Working Pressure (psi) : 5,000\nMax OD (In.), combined with 5 x Encapsulated control lines. : 7.396\nMin ID (In.) : 4.892\nDrift (In.) : 4.825\nTemp rating (degrees F) : 300\nGauge installation : External\nMandrel: Long tapers, longitudinal slot for 5 chemical injection/control\nlines (11mm x 11mm)\nSurface Testing Feature : Yes\nThread Up : 5-1/2\"\" 15.5 lb/ft SL-APEX Box\nThread Down : 5-1/2\"\" 15.5 lb/ft SL-APEX Pin\nMetallurgy : 13% Cr 80 ksi 18 - 22 HRC to NACE MR 0175\nTorsional Yield Strength thruBody (ft-lb) : 8,995\nTensile Strength thru Body (Ibs) : 687,259\"\n","","","","","GAUGE:MANDREL;\nSIZE: 5.5\"\nWEIGHT: 15.5#\nTHREAD UP: 5-1/2\" 15.5 LB/FT SL-APEX BOX\nTHREAD DOWN: 5-1/2\" 15.5 LB/FT SL-APEX PIN\nPRESSURE RATING: 5000 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 4.892\"\nDRIFT: 4.825\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","ZGMD_GGE_MANDREL","PD",0,0,0,0.01]
[1000688,"GAUGE:MNDRL;5.5\",15.5#,5-1/2\" 15.5 LB/F>",null,null,"EA","COM","4000009","SCHLUMBERGER USA","RR101125950","GAUGE:MANDREL;\nSIZE: 5.5\"\nWEIGHT: 15.5#\nTHREAD UP: 5-1/2\" 15.5 LB/FT SL-APEX BOX\nTHREAD DOWN: 5-1/2\" 15.5 LB/FT SL-APEX PIN\nPRESSURE RATING: 5,700 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 4.856\"\nDRIFT: 4.825\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","Permanent Dual Gauge Mandrel - Internal <(>&<)> External Reading\nMax OD (In.), combined with 5 x Encapsulated control lines. : 6.775\nMandrel: Long tapers, longitudinal slot for 5 chemical injection/control\nlines (11mm x 11mm)\nTorsional Yield Strength thru Body (ft-lb): 8,648\nTensile Strength thru Body (Ibs) :441,750\n\n","","22 May 2017 PO Long Text as per below:\nPermanent Dual Gauge Mandrel - Internal <(>&<)> External Reading\nSize (In.) : 5-1/2\"\"\nMin. Working Pressure (psi) : 5,700\nMax OD (In.), combined with 5 x Encapsulated control lines. : 6.775\nMin ID (In.) : 4.856\nDrift (In.) : 4.825\nTemp rating (degrees F) : 300\nGauge installation : External\nMandrel: Long tapers, longitudinal slot for 5 chemical injection/control\nlines (11mm x 11mm)\nSurface Testing Feature : Yes\nThread Up : 5-1/2\"\" 15.5 lb/ft SL-APEX Box\nThread Down : 5-1/2\"\" 15.5 lb/ft SL-APEX Pin\nMetallurgy : 13% Cr 80 ksi 18 - 22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb): 8,648\nTensile Strength thru Body (Ibs) :441,750\n \"\n","","","","","GAUGE:MANDREL;\nSIZE: 5.5\"\nWEIGHT: 15.5#\nTHREAD UP: 5-1/2\" 15.5 LB/FT SL-APEX BOX\nTHREAD DOWN: 5-1/2\" 15.5 LB/FT SL-APEX PIN\nPRESSURE RATING: 5,700 PSI\nTEMPERATURE RATING: 300°F\nINSIDE DIAMETER: 4.856\"\nDRIFT: 4.825\"\nMATERIAL: 13% CR 80 KSI 18 - 22 HRC\nGAUGE INSTALLATION: EXTERNAL\nSURFACE TESTING FEATURE: YES\nSPECIFICATION: NACE MR 0175\n","ZGMD_GGE_MANDREL","PD",0,0,0,0.01]
[1000689,"SLIDING SLEEVE SURFACE,5.5\", NON ELASTOM",null,null,"EA","COM","4000009","SCHLUMBERGER USA","240-765-4562X-554-MSLAPEXM","22 May 2017 PO Long Text as per below:\nSurface Controlled Non Elastomeric Sliding Sleeve:\nSize (in.): 5-1/2\"\"\nMin. Working Pressure (psi): 5,000\nMax OD (in.): 7,990\nThread Up:  5-1/2\"\" 15.5 lb/ft SL Apex Box\nThread Down: 5-1/2\"\" 15.5 lb/ft SL Apex Pin\nMetallurgy: 13 Cr 80 ksi 18 - 22 HRC to NACE MR 0175\nSeal Type: Non-Elastomeric\nNipple Profile: 4.562\nControl Connection: Metal to metal control line connection that is\nexternally testable to 10,000 psi after make-up. The test port is a\n1/4\"\" 28 thread with a 1/16\"\" HIP TaperSeal Fitting\nInternal Connections: Proprietary metal-to-metal connections that\neliminates the need for o-rings\nMechanical back up shifting mechanism:  Featured. Shifting profile\n(fishneck) on the ID of the Inner sleeve can be engaged with an Industry\nstandard Type B Shifting Tool run on slickline or CT\nUnloading Pressure (psi): The DLV sleeve has been tested to meet the\nrequirement of shifting with a differential pressure of 2,000 psi.\nActual FAT requires 5,000 psi differential pressure.\nMechanical back up shifting force (Ibs): max 2,500 lbs\nTorsional Yield Strength thru Body (ftlb) : 8,000 ft.lb\nTensile Strength thru Body (lbs) : 503,000 lb\"\n","Surface Controlled Non Elastomeric Sliding Sleeve:\nSize (in.): 5-1/2\"\"\nMin. Working Pressure (psi): 5,000\nMax OD (in.): 7,990\nThread Up:  5-1/2\"\" 15.5 lb/ft SL Apex Box\nThread Down: 5-1/2\"\" 15.5 lb/ft SL Apex Pin\nMetallurgy: 13 Cr 80 ksi 18 - 22 HRC to NACE MR 0175\nSeal Type: Non-Elastomeric\nNipple Profile: 4.562\nControl Connection: Metal to metal control line connection that is\nexternally testable to 10,000 psi after make-up. The test port is a\n1/4\"\" 28 thread with a 1/16\"\" HIP TaperSeal Fitting\nInternal Connections: Proprietary metal-to-metal connections that\neliminates the need for o-rings\nMechanical back up shifting mechanism:  Featured. Shifting profile\n(fishneck) on the ID of the Inner sleeve can be engaged with an Industry\nstandard Type B Shifting Tool run on slickline or CT\nUnloading Pressure (psi): The DLV sleeve has been tested to meet the\nrequirement of shifting with a differential pressure of 2,000 psi.\nActual FAT requires 5,000 psi differential pressure.\nMechanical back up shifting force (Ibs): max 2,500 lbs\nTorsional Yield Strength thru Body (ftlb) : 8,000 ft.lb\nTensile Strength thru Body (lbs) : 503,000 lb\n","","22 May 2017 PO Long Text as per below:\nSurface Controlled Non Elastomeric Sliding Sleeve:\nSize (in.): 5-1/2\"\"\nMin. Working Pressure (psi): 5,000\nMax OD (in.): 7,990\nThread Up:  5-1/2\"\" 15.5 lb/ft SL Apex Box\nThread Down: 5-1/2\"\" 15.5 lb/ft SL Apex Pin\nMetallurgy: 13 Cr 80 ksi 18 - 22 HRC to NACE MR 0175\nSeal Type: Non-Elastomeric\nNipple Profile: 4.562\nControl Connection: Metal to metal control line connection that is\nexternally testable to 10,000 psi after make-up. The test port is a\n1/4\"\" 28 thread with a 1/16\"\" HIP TaperSeal Fitting\nInternal Connections: Proprietary metal-to-metal connections that\neliminates the need for o-rings\nMechanical back up shifting mechanism:  Featured. Shifting profile\n(fishneck) on the ID of the Inner sleeve can be engaged with an Industry\nstandard Type B Shifting Tool run on slickline or CT\nUnloading Pressure (psi): The DLV sleeve has been tested to meet the\nrequirement of shifting with a differential pressure of 2,000 psi.\nActual FAT requires 5,000 psi differential pressure.\nMechanical back up shifting force (Ibs): max 2,500 lbs\nTorsional Yield Strength thru Body (ftlb) : 8,000 ft.lb\nTensile Strength thru Body (lbs) : 503,000 lb\"\n","","","","","-","-","PD",0,0,0,0.01]
[1000690,"VLV,BAR, SPACER ASSEMBLY, 4.5\"","VLV","VALVE","EA","WSI","4000009","SCHLUMBERGER USA","100352171","22 May 2017 PO Long Text as per below:\nSPACER BAR ASSEMBLY, 4.500\"","Permanent Gauge Mandrel - Internal Reading\nSize (in.) : 3-1/2\"\"\nMin. Working Pressure (psi): 5,000\nMax OD (in.), combined with 5 x Encapsulated control lines. : 5.28\nMin ID (in.): 2.898\nDrift (in.) : 2.867\nTemp rating (degrees F) : 300\nGauge installation : External\nMandrel : Long tapers, longitudinal slot for 5 chemical\nInjection/control lines (11mm x 11mm)\nSurface Testing Feature : Yes\nThread Up : 3-1/2\"\" 9.2 lb/ft SL-APEX Box\nThread Down : 3-1/2\"\" 9.2 lb/ft SL-APEX Pin\nMetallurgy : 13% Cr 80 ksi 18-22 HRC to NACE MR 0175\nTorsional Yield Strength thru Body (ft-lb): 4,000\nTensile Strength thru Body (Ibs): 237,600\"\n","","22 May 2017 PO Long Text as per below:\nSPACER BAR ASSEMBLY, 4.500\"\n","","","","","-","-","ND",0,0,0,{"v":16651,"d":"16,651.00"}]
[1000691,"WLT LOCK OPEN:TRSSV;EXERCISE TL TRMAXX->",null,null,"EA","WSI","4000009","SCHLUMBERGER USA","100352169","WIRELINE TOOL LOCK OPEN:TRSSV;\nTYPE: EXERCISE TOOL TRMAXX-5E\nSIZE OD: 3.53\nLENGTH: 64.8\nWEIGHT: 200LBS\nCONNECTION: 1 9/16\nCONNECTION TYPE: UNS-2 PIN\nFISH NECK SIZE: 2.313\nMATERIAL: 4140\nMAXIMUM OD: 3.53\nFISHNECK SIZE: 2.313\nDRAWING/DOCUMENT REFERENCE-1: 100352169","For SLB TRMAXX 5E\n\nDatasheet attached.\n","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","22 May 2017 PO Long Text as per below:\nFLOW TUBE EXERCISE TOOL, 4.500\"\n","","","","","WIRELINE TOOL LOCK OPEN:TRSSV;\nTYPE: EXERCISE TOOL TRMAXX-5E\nSIZE OD: 3.53\nLENGTH: 64.8\nWEIGHT: 200LBS\nCONNECTION: 1 9/16\nCONNECTION TYPE: UNS-2 PIN\nFISH NECK SIZE: 2.313\nMATERIAL: 4140\nMAXIMUM OD: 3.53\nFISHNECK SIZE: 2.313\nDRAWING/DOCUMENT REFERENCE-1: 100352169","ZGMD_WLT_L_O_TL_TR","PD",1,0,0,{"v":22219.86,"d":"22,219.86"}]
[1000692,"WLR:SLB FLW TBE EXC RDK,4.5,103600624",null,null,"EA","WSI","4000009","SCHLUMBERGER USA","103600624","WIRELINE TOOL REDRESS KIT:\nTYPE: SLB FLOW TUBE EXC RDK\nSIZE OD: 4.5\nDRAWING/DOCUMENT REFERENCE-1: 103600624","(100352169_REDKIT)\n\n","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","22 May 2017 PO Long Text as per below:\nFLOW TUBE EXERCISE TOOL, 4.500\", REDRESS KIT\n","","","","","WIRELINE TOOL REDRESS KIT:\nTYPE: SLB FLOW TUBE EXC RDK\nSIZE OD: 4.5\nDRAWING/DOCUMENT REFERENCE-1: 103600624","ZGMD_WLT_REDR_KIT","PD",1,0,0,{"v":1072.14,"d":"1,072.14"}]
[1000693,"WLT LOCK OPEN:TRSSV;HYD DEFO TL TRMAXX5>",null,null,"EA","WSI","4000009","SCHLUMBERGER USA","100395993","WIRELINE TOOL LOCK OPEN:TRSSV;\nTYPE: HYD DEFO TOOL TRMAXX5E\nSIZE OD: 3.76\nLENGTH: 94.5\nWEIGHT: 200LBS\nCONNECTION: 1 9/16 SR\nCONNECTION TYPE: SUCKER ROD\nFISH NECK SIZE: 2.313\nMATERIAL: L-80 4140\nMAXIMUM OD: 3.76\nFISHNECK SIZE: 2.313\nDRAWING/DOCUMENT REFERENCE-1: 100395993","For SLB TRMAXX 5 E\n\nDatasheet attached.\n\n\n\n","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","22 May 2017 PO Long Text as per below:\n\"HYDRAULIC DEFORMATION LOCKOUT TOOL:\nSize:  4.500”\nOutside diameter: 3.812” OD, DS\"\n","","","","","WIRELINE TOOL LOCK OPEN:TRSSV;\nTYPE: HYD DEFO TOOL TRMAXX5E\nSIZE OD: 3.76\nLENGTH: 94.5\nWEIGHT: 200LBS\nCONNECTION: 1 9/16 SR\nCONNECTION TYPE: SUCKER ROD\nFISH NECK SIZE: 2.313\nMATERIAL: L-80 4140\nMAXIMUM OD: 3.76\nFISHNECK SIZE: 2.313\nDRAWING/DOCUMENT REFERENCE-1: 100395993","ZGMD_WLT_L_O_TL_TR","PD",1,0,0,{"v":45306.45,"d":"45,306.45"}]
[1000694,"WLT LOCK OPEN:TRSSV;LK OUT 4.5 TRMAXX5E>",null,null,"EA","WSI","4000009","SCHLUMBERGER USA","100932640","WIRELINE TOOL LOCK OPEN:TRSSV;\nTYPE: LOCK OUT 4.5 TRMAXX5E\nSIZE OD: 3.72\nLENGTH: 68.04\nWEIGHT: 200LBS\nCONNECTION: 1 9/16 SR\nCONNECTION TYPE: SUCKER ROD\nFISH NECK SIZE: 2.313\nMATERIAL: L80 4140\nMAXIMUM OD: 3.72\nFISHNECK SIZE: 2.313\nDRAWING/DOCUMENT REFERENCE-1: 100932640","4.5 lock open tool for SLB TRMAXX 5E\n\nDatasheet attached.\n\n","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","22 May 2017 PO Long Text as per below:\nSIMPLIFIED LOCK OUT TOOL, 4.500\"\nOutside diameter: 3.812” OD","","","","","WIRELINE TOOL LOCK OPEN:TRSSV;\nTYPE: LOCK OUT 4.5 TRMAXX5E\nSIZE OD: 3.72\nLENGTH: 68.04\nWEIGHT: 200LBS\nCONNECTION: 1 9/16 SR\nCONNECTION TYPE: SUCKER ROD\nFISH NECK SIZE: 2.313\nMATERIAL: L80 4140\nMAXIMUM OD: 3.72\nFISHNECK SIZE: 2.313\nDRAWING/DOCUMENT REFERENCE-1: 100932640","ZGMD_WLT_L_O_TL_TR","PD",1,0,0,{"v":19298.52,"d":"19,298.52"}]
[1000695,"WLR:RDRSS KIT DEFORMATION,4.5,(10039599>",null,null,"EA","WSI","4000009","SCHLUMBERGER USA","103600622","WIRELINE TOOL REDRESS KIT:\nTYPE: REDRESS KIT DEFORMATION\nSIZE OD: 4.5\nDRAWING/DOCUMENT REFERENCE-1: (100395993_REDKIT)","(100395993_REDKIT)\n","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","22 May 2017 PO Long Text as per below:\nREDRESS KIT DEFORMATION TOOL:\nSize: 4.500\", REDRESS KIT","","","","","WIRELINE TOOL REDRESS KIT:\nTYPE: REDRESS KIT DEFORMATION\nSIZE OD: 4.5\nDRAWING/DOCUMENT REFERENCE-1: (100395993_REDKIT)","ZGMD_WLT_REDR_KIT","PD",1,0,0,{"v":2556.77,"d":"2,556.77"}]
[1000696,"VLV,LOCK, DB-6, 3.812\"","VLV","VALVE","EA","WSI","4000009","SCHLUMBERGER USA","10254-000-05000","22 May 2017 PO Long Text as per below:\nDB-6 LOCK, 3.812”\n","DB-6 LOCK, 3.812”\n\n","","22 May 2017 PO Long Text as per below:\nDB-6 LOCK, 3.812”\n\n","","","","","-","-","ND",0,0,0,{"v":19285,"d":"19,285.00"}]
[1000697,"VLV,LOCK, DB-6, REDRESS KIT, 4.5\"","VLV","VALVE","EA","WSI","4000009","SCHLUMBERGER USA","16530-000-04000","22 May 2017 PO Long Text as per below:\nDB-6 LOCK REDRESS KIT, 4.500\"\nREDRESS KIT FOR 4-1/2 DB- 6 LOCK","DB-6 LOCK REDRESS KIT, 4.500\"\nREDRESS KIT FOR 4-1/2 DB- 6 LOCK\n","","22 May 2017 PO Long Text as per below:\nDB-6 LOCK REDRESS KIT, 4.500\"\nREDRESS KIT FOR 4-1/2 DB- 6 LOCK","","","","","-","-","ND",0,0,0,{"v":3645,"d":"3,645.00"}]
[1000698,"VLV,PRONG PULLING TOOL, 4.5\"","VLV","VALVE","EA","WSI","4000009","SCHLUMBERGER USA","15203-000-01000_PULLPRONG","22 May 2017 PO Long Text as per below:\nPULLING PRONG TOOL, 4.500\"\n","PULLING PRONG TOOL, 4.500\"\n\n","","22 May 2017 PO Long Text as per below:\nPULLING PRONG TOOL, 4.500\"\n\n","","","","","-","-","ND",0,0,0,{"v":15988,"d":"15,988.00"}]
[1000699,"VLV,PRONG RUNNING TOOL, 3.5\"","VLV","VALVE","EA","WSI","4000009","SCHLUMBERGER USA","15098-000-01000_RUNPRONG","22 May 2017 PO Long Text as per below:\nRUNNING PRONG TOOL\nSize: 3.500\"\n","RUNNING PRONG TOOL\nSize: 3.500\"\n\n","","22 May 2017 PO Long Text as per below:\nRUNNING PRONG TOOL\nSize: 3.500\"\n","","","","","-","-","ND",0,0,0,{"v":11988,"d":"11,988.00"}]
[1000700,"VLV,PULLING TOOL, PRS, 4.5\"","VLV","VALVE","EA","WSI","4000009","SCHLUMBERGER USA","15203-000-01000","22 May 2017 PO Long Text as per below:\nPRS PULLING TOOL, 4.500\"\n\n","PRS PULLING TOOL, 4.500\"\n\n","","22 May 2017 PO Long Text as per below:\nPRS PULLING TOOL, 4.500\"\n\n","","","","","-","-","ND",0,0,0,{"v":24255,"d":"24,255.00"}]
[1000701,"VLV,RUNNING TOOL, Z-6, 3.5\"","VLV","VALVE","EA","WSI","4000009","SCHLUMBERGER USA","15098-000-01000","22 May 2017 PO Long Text as per below:\nZ-6 RUNNING TOOL, 3.500\"\n\n","Z-6 RUNNING TOOL, 3.500\"\n\n","","22 May 2017 PO Long Text as per below:\nZ-6 RUNNING TOOL, 3.500\"\n\n","","","","","-","-","ND",0,0,0,{"v":19686,"d":"19,686.00"}]
[1000702,"WLR:RDRSS KIT LK OUT TL,4.5,(100932640_>",null,null,"EA","WSI","4000009","SCHLUMBERGER USA","103600623","WIRELINE TOOL REDRESS KIT:\nTYPE: REDRESS KIT LOCK OUT TOOL\nSIZE OD: 4.5\nDRAWING/DOCUMENT REFERENCE-1: (100932640_REDKIT)","(100932640_REDKIT)","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","22 May 2017 PO Long Text as per below:\nREDRESS KIT SLOT TOOL:\nSize: 4.500\",REDRESS KIT\n","","","","","WIRELINE TOOL REDRESS KIT:\nTYPE: REDRESS KIT LOCK OUT TOOL\nSIZE OD: 4.5\nDRAWING/DOCUMENT REFERENCE-1: (100932640_REDKIT)","ZGMD_WLT_REDR_KIT","PD",1,0,0,{"v":1152.39,"d":"1,152.39"}]
[1000703,"VLV,WIRELINE RETRIEVEABLE, 4.5\",5K","VLV","VALVE","EA","WSI","4000009","SCHLUMBERGER USA","23287-000-00001","22 May 2017 PO Long Text as per below:\nWIRELINE RETRIEVABLE SAFETY VALVE:\nWRDP-1A-DS\nInternal Diameter: 1.875\" ID\nOutside Diameter: 3.812\" OD\nPressure: 5K\n","WIRELINE RETRIEVABLE SAFETY VALVE:\nWRDP-1A-DS\nInternal Diameter: 1.875\" ID\nOutside Diameter: 3.812\" OD\nPressure: 5K\n","","22 May 2017 PO Long Text as per below:\nWIRELINE RETRIEVABLE SAFETY VALVE:\nWRDP-1A-DS\nInternal Diameter: 1.875\" ID\nOutside Diameter: 3.812\" OD\nPressure: 5K\n","","","","","-","-","ND",0,0,0,{"v":45223,"d":"45,223.00"}]
[1000704,"GSKT:F/VLVSEAT,HNBR ELAST-O-LION 985","VLV","VALVE","EA","MES","4000480","PETROLVALVES","45OR237900 NW","GASKET:\nTYPE: FOR VALVE SEAT\nMATERIAL: HNBR ELAST-O-LION 985","BOM KIT\nASFBA-ESDV-290005ASDBA-\nESDV-290001ASEBA-\nESDV-290004","","GASKET FOR VALVE SEATMATERIAL:HNBR ELAST-O-LION 985MANUFACTURER\nPN:45OR237900 NWDRAWING\n\n BOM KIT\nASFBA-ESDV-290005ASDBA-\nESDV-290001ASEBA-\nESDV-290004","","","","","GASKET:\nTYPE: FOR VALVE SEAT\nMATERIAL: HNBR ELAST-O-LION 985","ZGMD_GSKT_NM","PD",0,0,0,0.01]
[1000710,"RESP:SCBA,BA",null,null,"EA","SSE","4000067","DRAEGER SAFETY A/S","PSS 5000 DP SCS (OLD PN:PSS 5000 DS SCS)","RESPIRATOR:\nTYPE: SCBA\nUSE: BREATHING APPARATUS","DRAGER,SELF-CONTAINED BREATHING, APPARATUS (SCBA)\nMODEL PSS 5000 DP SCS PSS 5000,\nPNEUMATIC GAUGE,\nSINGLE CYLINDER STRAP (SCS) PN# 3357845 (DP)\nPLUS LUNG DEMAND VALVE (LDV), WITH POLYMER DIAPHRAGM\nFOR USE IN H2S ENVIRONMENTS PN# 3338967\nFULL FACE MASK: FPS 7000\nPN# R562009 LTR/300\nBAR LIGHT WEIGHT CARBON COMPOSITE CYLINDER WITH\nRIGHT ANGLE VALVE,\nFITTED WITH EXCESS FLOW VALVE (FFV)\n2ND MP COMBINED CONNECTOR HOSE FORWARD -\nWAIST-SECURED PN# 3358403\n(SEE ATTACHED MSDS)\nNOTES:\nCERTIFICATE OF CONFORMITY TO INCLUDE CONFIRMATION OF\nCLEAN AIR FILL TO BS EN 12021 OR EQUIVALENT.\nMSDS (SAFETY DATA SHEET) TO BE PROVIDED","","","03","","","199103706","RESPIRATOR:\nTYPE: SCBA\nUSE: BREATHING APPARATUS","ZGMD_RESP_NM","PD",0,0,0,683.97]
[1000724,"COMPOSITE,FCE BLOCK BODY 4-1/8 5K INC625",null,null,"EA","DRL","4000005","GE-VETCO / UK","H385432-1","COMPOSITE BLOCK PART, 2-1-0\nBODY: 4-1/8\"\nPRESSURE: 5000 PSI MSP\nMODEL: VG-300\n13-5/8\" GR137 5000 PSI NT-2 BTM X 4-1/16 5000 PSI STUDDED TOP\nW/ONE STUDDED OUTLET, BTM PREP FOR CBT SEAL\nSTANDARD:75K LOW ALLOY NACE, AISI 4130, I/T -20F PSL2\nMETALLURGY: W/INCONEL 625 FULL CLAD","","","06 June 2017 PO Long Text as per below:\nCOMPOSITE BLOCK PART, 2-1-0\nBODY: 4-1/8\"\nPRESSURE: 5000 PSI MSP\nMODEL: VG-300\n13-5/8\" GR137 5000 PSI NT-2 BTM X 4-1/16 5000 PSI STUDDED TOP\nW/ONE STUDDED OUTLET, BTM PREP FOR CBT SEAL\nSTANDARD:75K LOW ALLOY NACE, AISI 4130, I/T -20F PSL2\nMETALLURGY: W/INCONEL 625 FULL CLAD","","","","","-","-","PD",0,0,0,0.01]
[1000728,"CONN:WH PART,NT-2,13-5/8\"",null,null,"EA","XMT","4000281","GE VETCO GRAY","A71917-1","CONNECTOR:\nTYPE: WELLHEAD PART,NT-2\nSIZE: 13-5/8\"\n","MODEL: VGS5.110.1.34\nTHREADING: THREAD ON HOUSING\nCERTIFICATION : 75K LA NACE\n","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","CONNECTOR:\nTYPE: WELLHEAD PART,NT-2\nSIZE: 13-5/8\"\n","ZGMD_CNNT_NM","PD",0,0,0,{"v":5516,"d":"5,516.00"}]
[1000729,"VLV PRT,MAN BONNET,INC625 OVERLAY,HHTRIM","VLV","VALVE","EA","WEL","4000005","GE-VETCO / UK","H134149-2","VALVE PART,MANUAL BONNET:\nPRESSURE: 4.062 IN 5000 PSI  MSP\nTYPE VG-300\nMETALLURGY:\n60K AISI 4130 NACE MR-01-75\nCLAD  WITH MINIMUM THICKNESS = 0.125\"\nUT INSPECT BASE MATERIAL PER VGS8.1.2\nS1 PRIOR  TO PREP FOR CLADDING\nMACHINE PREP FOR CLAD PER MFG. PROCESS DWGS\nVISUAL INSPECTION OF WELD PREPARATION IS   REQUIRED\nINCONEL 625 OVERLAY PER VGS 7.0002.6.10 TO  FINISH 0.125 MIN OVERLAY\nAFTER FINAL M/C\nALTERNATIVE OVERLAY PROCEDURE VGS 7.0002.1.2  OR VGS 7.0002.1.7 (TO\nFACILITATE MANUFACTURE)","","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long Text as per below:\nVALVE PART,MANUAL BONNET:\nPRESSURE: 4.062 IN 5000 PSI  MSP\nTYPE VG-300\nMETALLURGY:\n60K AISI 4130 NACE MR-01-75\nCLAD  WITH MINIMUM THICKNESS = 0.125\"\nUT INSPECT BASE MATERIAL PER VGS8.1.2\nS1 PRIOR  TO PREP FOR CLADDING\nMACHINE PREP FOR CLAD PER MFG. PROCESS DWGS\nVISUAL INSPECTION OF WELD PREPARATION IS   REQUIRED\nINCONEL 625 OVERLAY PER VGS 7.0002.6.10 TO  FINISH 0.125 MIN OVERLAY\nAFTER FINAL M/C\nALTERNATIVE OVERLAY PROCEDURE VGS 7.0002.1.2  OR VGS 7.0002.1.7 (TO\nFACILITATE MANUFACTURE)","","","","","-","-","PD",0,0,0,{"v":9150,"d":"9,150.00"}]
[1000739,"VLV PRT,SPLIT GATE ,4-1/8\" 5K ALLOY 625","VLV","VALVE","EA","WEL","4000005","GE-VETCO / UK","H133624-1","VALVE PART, GATE,MANUAL:\nSIZE <(>&<)> PRESSURE : 4-1/8\", 5000 PSI MSP\nMODEL: VG-300S.\nMETALLURGY : SPLIT,ALLOY 625 NACE,CARBIDE COATED","","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nVALVE PART, GATE,MANUAL:\nSIZE <(>&<)> PRESSURE : 4-1/8\", 5000 PSI MSP\nMODEL: VG-300S.\nMETALLURGY : SPLIT,ALLOY 625 NACE,CARBIDE COATED","","","","","-","-","PD",0,0,0,{"v":7607,"d":"7,607.00"}]
[1000740,"VLV PRT,SEAT,4-1/8\" 5K, ALLOY 625","VLV","VALVE","EA","WEL","4000005","GE-VETCO / UK","H130951-13","VALVE PART,SEAT:\nSIZE <(>&<)> PRESSURE:  4-1/8\", 5000 PSI MSP\nTYPE: VG-300\nMETALLURGY: ALLOY 625 NACE WITH TUNGSTEN CARBIDE COATING","","","06 June 2017 PO Long text as per belowr below:\nVALVE PART,SEAT:\nSIZE <(>&<)> PRESSURE:  4-1/8\", 5000 PSI MSP\nTYPE: VG-300\nMETALLURGY: ALLOY 625 NACE WITH TUNGSTEN CARBIDE COATING","","","","","-","-","PD",0,0,0,{"v":2319,"d":"2,319.00"}]
[1000741,"VLV PRT,STEM MAN,4-1/16\" 5M, INC 718, HH","VLV","VALVE","EA","WEL","4000005","GE-VETCO / UK","H130853-36","VALVE PART,STEM,MANUAL:\nSIZE <(>&<)> PRESSURE: 4-1/16\",  5000 PSI MSP\nDIMENSIONS: A =  17.08 B =   6.07\nMODEL: VG-300\n1-1/8\"-6ACME-2G LH MOD CENT THD\nMETALLURGY: INCONEL 718 NACE","","","06 June 2017 PO Long text as per belowr below:\nVALVE PART,STEM,MANUAL:\nSIZE <(>&<)> PRESSURE: 4-1/16\",  5000 PSI MSP\nDIMENSIONS: A =  17.08 B =   6.07\nMODEL: VG-300\n1-1/8\"-6ACME-2G LH MOD CENT THD\nMETALLURGY: INCONEL 718 NACE","","","","","-","-","PD",0,0,0,{"v":2250,"d":"2,250.00"}]
[1000742,"RING-SEAL,BNT, 5.740 ID,ALLOY 718",null,null,"EA","DRL","4000005","GE-VETCO / UK","H130151-26","RING-SEAL,BNT:\nID: 5.740\"\nMETALLURGY: ALLOY 718 NACE MR-01-75\nCOATING: MOS2 COATED","","","06 June 2017 PO Long text as per belowr below:\nRING-SEAL,BNT:\nID: 5.740\"\nMETALLURGY: ALLOY 718 NACE MR-01-75\nCOATING: MOS2 COATED","","","","","-","-","PD",0,0,0,{"v":2438,"d":"2,438.00"}]
[1000743,"VLV PRT,DRIVE BUSHING,VG 300,ALLOY 625","VLV","VALVE","EA","WEL","4000005","GE-VETCO / UK","H130871-3","VALVE PART,DRIVE BUSHING:\nTYPE:VG-300\nMETALLURGY:\n1-1/8-6 ACME LH MOD CENT THD\nALLOY 625 NACE","","","06 June 2017 PO Long text as per belowr below:\nVALVE PART,DRIVE BUSHING:\nTYPE:VG-300\nMETALLURGY:\n1-1/8-6 ACME LH MOD CENT THD\nALLOY 625 NACE","","","","","-","-","PD",0,0,0,{"v":1550,"d":"1,550.00"}]
[1000744,"GLAND:PACKING;VG-300 VLV,1-1/8\" STM,LOW>","VLV","VALVE","EA","WEL","4000005","GE-VETCO / UK","H130961-1","GLAND:PACKING;\nTYPE: VG-300 VALVE\nSIZE: 1-1/8\" STEM\nMATERIAL: LOW ALLOY NACE WITH PROT. COAT","FULL TRACEABILITY IN TERMS OF MANUFACTURING BATCH, DATE, DUROMETER\nRATING FOR ELASTOMERS.\nEN 10204 CERTIFICATE TYPE 3.1 VALID ONLY FOR METALLIC PARTS","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nVALVE PART,PACKING GLAND\nTYPE VG-300,FOR 1-1/8\" STEM\nMETALLURGY: LOW ALLOY NACE WITH PROTECTIVE COATING","","","","","GLAND:PACKING;\nTYPE: VG-300 VALVE\nSIZE: 1-1/8\" STEM\nMATERIAL: LOW ALLOY NACE WITH PROT. COAT","ZGMD_GLND_PCK","PD",0,0,0,{"v":252,"d":"252.00"}]
[1000745,"O-RING:AS568A-218,1.234\" (NOM 1-1/4\"),N>",null,null,"EA","DRL","4000005","GE-VETCO / UK","195000-218","O-RING:\nTYPE: AS568A-218\nINSIDE DIAMETER: 1.234\" (NOM 1-1/4\")\nMATERIAL: NBR D70 VGS5.1010.1.1\nINDUSTRY STANDARD: API-6A, PSL 1-3\nADDITIONAL INFORMATION: 0.139\" (NOM 1/8\") CS","FULL TRACEABILITY IN TERMS OF MANUFACTURING BATCH, DATE, DUROMETER\nRATING FOR ELASTOMERS.","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nO-RING:\nMODEL: AS568A-218\nID: 1.234\" (NOM 1-1/4\")\nCS: 0.139\" (NOM 1/8\")\nMATERIAL PER VGS5.1010.1.1\nMETALLURGY: NITRILE (NBR), 70 DURO A\nSTANDARD: API 6A, ISO 10423, API17D, PSL1-3","","","","","O-RING:\nTYPE: AS568A-218\nINSIDE DIAMETER: 1.234\" (NOM 1-1/4\")\nMATERIAL: NBR D70 VGS5.1010.1.1\nINDUSTRY STANDARD: API-6A, PSL 1-3\nADDITIONAL INFORMATION: 0.139\" (NOM 1/8\") CS","ZGMD_O_RNG_NM","PD",0,0,0,{"v":6,"d":"6.00"}]
[1000746,"PLATE:NAME;VG-300 VLV,INSTR PLT,1-1/8\" >","VLV","VALVE","EA","XMT","4000005","GE-VETCO / UK","H130895-3","PLATE:NAME;\nTYPE: VG-300 VALVE\nDESIGNATION: INSTRUCTION PLATE\nSIZE: 1-1/8\" STEM\nMATERIAL: 18-8SS","","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nVALVE PART,INSTRUCTION PLATE FOR 1-1/8\" STEM\nMODEL: VG-300,18-8SS","","","","","PLATE:NAME;\nTYPE: VG-300 VALVE\nDESIGNATION: INSTRUCTION PLATE\nSIZE: 1-1/8\" STEM\nMATERIAL: 18-8SS","ZGMD_PLT_NAME","PD",0,0,0,{"v":52,"d":"52.00"}]
[1000747,"BONNET:CAP,VG-300,1-1/8\" STM,60K LOW AL>",null,null,"EA","DRL","4000005","GE-VETCO / UK","H130883-1","BONNET:\nTYPE: CAP, VG-300\nSIZE: 1-1/8\" STEM\nMATERIAL: 60K LOW ALLOY NACE","WITH PROTECTIVE COATING","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nVALVE PART,BONNET CAP:\nTYPE: VG-300,FOR 1-1/8\" STEM\nMETALLURGY: 60K LOW ALLOY NACE WITH PROTECTIVE COATING","","","","","BONNET:\nTYPE: CAP, VG-300\nSIZE: 1-1/8\" STEM\nMATERIAL: 60K LOW ALLOY NACE","ZGMD_BONNET_NM","PD",0,0,0,{"v":720,"d":"720.00"}]
[1000748,"STUD:ALLTHD;1.125\",8UNR-2A,7.25\" (THREA>",null,null,"EA","WEL","4000005","GE-VETCO / UK","H464628-102 (OLD PN:H300518-6)","STUD:ALL-THREAD;\nDIAMETER: 1.125\"\nTHREADS: 8UNR-2A\nLENGTH: 7.25\" (THREAD LENGTH NOT OAL)\nSPECIFICATION: ASTM A320\nGRADE: L7M","STUD, ALL THREAD, PER VGS2.4.47, 1.125-8UNR-2A,\n\n7.250 LG, STUD MATERIAL PER API 20E BSL-1 ASTM\n\nA320 GR L7M, ZINC NICKEL PLATING PER VGS6.2.10.7","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","100139795","STUD:ALL-THREAD;\nDIAMETER: 1.125\"\nTHREADS: 8UNR-2A\nLENGTH: 7.25\" (THREAD LENGTH NOT OAL)\nSPECIFICATION: ASTM A320\nGRADE: L7M","ZGMD_STUD_ALLTHD","PD",80,0,0,23.32]
[1000749,"NUT:HEX;HVY,1-1/8\",8UN-2B,A194,GR-2HM",null,null,"EA","XMT","4000005","GE-VETCO / UK","H464644-110","NUT:HEX;\nTYPE: HEAVY\nDIAMETER: 1-1/8\"\nTHREADS: 8UN-2B\nSPECIFICATION: ASTM A194\nGRADE: GR-2HM","NUT, HEAVY HEX, 1.125-8UNC-2B, MATERIAL PER API\n\n20E BSL-1 ASTM A194 GR 2HM, ZINC NICKEL PLATING\n\nPER VGS6.2.10.9\n","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","NUT:HEX;\nTYPE: HEAVY\nDIAMETER: 1-1/8\"\nTHREADS: 8UN-2B\nSPECIFICATION: ASTM A194\nGRADE: GR-2HM","ZGMD_NUT_HX","PD",0,0,0,7.68]
[1000750,"STEM:THR P,1-1/8\" STM,0.562\" X 2-7/8\" L>",null,null,"EA","WEL","4000005","GE-VETCO / UK","H130893-4","STEM:\nTYPE: THRUST PIN, 1-1/8\" STEM\nSIZE: 0.562\" X 2-7/8\" LENGTH\nMATERIAL: 4140 STEEL, RC 43-48","","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nVALVE PART,THRUST PIN:\nTYPE: VG-300 FOR 1-1/8\" STEM\nMETALLURGY: 4140 STEEL\nCONNECTION:RC 43-48\nLENGTH: 0.562\" X 2-7/8\"","","","","","STEM:\nTYPE: THRUST PIN, 1-1/8\" STEM\nSIZE: 0.562\" X 2-7/8\" LENGTH\nMATERIAL: 4140 STEEL, RC 43-48","ZGMD_STEM_NM","PD",0,0,0,{"v":98,"d":"98.00"}]
[1000751,"RING:WIPER;SL,1.125\" DIA RD",null,null,"EA","XMT","4000005","GE-VETCO / UK","200095-7","RING:WIPER;\nTYPE: SEAL\nSIZE: 1.125\" DIA ROD\n","FULL TRACEABILITY IN TERMS OF MANUFACTURING BATCH, DATE, DUROMETER\nRATING FOR ELASTOMERS.\nEN 10204 CERTIFICATE TYPE 3.1 VALID ONLY FOR METALLIC PARTS","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nSEAL,WIPER:\nSIZE: 1.125\" ROD DIA","","","","","RING:WIPER;\nTYPE: SEAL\nSIZE: 1.125\" DIA ROD\n","ZGMD_RNG_WIPER","PD",0,0,0,{"v":44,"d":"44.00"}]
[1000752,"O-RING:AS568A-339,3.25\" NOM,0.1875\" NOM>",null,null,"EA","DRL","4000281","GE VETCO GRAY","195000-339","O-RING:\nTYPE: AS568A-339\nINSIDE DIAMETER: 3.25\" NOM\nWIDTH: 0.1875\" NOM\nMATERIAL: NITRILE (NBR), 70 DURO A\nINDUSTRY STANDARD: API-6A,ISO-10423,API17D,PSL1-3\nADDITIONAL INFORMATION: VGS5.1010.1.1","","MATERIAL CERTIFICATE EN 10204 2.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nO-RING, AS568A-339:\nID: 3.225\" (NOM 3-1/4\")\nCS: 0.210\" (NOM 3/16\")\nMATERIAL PER VGS5.1010.1.1\nMETALLURGY: NITRILE (NBR), 70 DURO A\nSTANDARD: API 6A, ISO 10423, API17D, PSL1-3","","","","","O-RING:\nTYPE: AS568A-339\nINSIDE DIAMETER: 3.25\" NOM\nWIDTH: 0.1875\" NOM\nMATERIAL: NITRILE (NBR), 70 DURO A\nINDUSTRY STANDARD: API-6A,ISO-10423,API17D,PSL1-3\nADDITIONAL INFORMATION: VGS5.1010.1.1","ZGMD_O_RNG_NM","PD",0,0,0,{"v":8,"d":"8.00"}]
[1000753,"BUSH:BUSH VG-300 VLV,1-1/8\" STM,VRGN PE>","VLV","VALVE","EA","WEL","4000005","GE-VETCO / UK","H130896-2","BUSHING:\nTYPE: BUSHING VG-300 VALVE\nSIZE: 1-1/8\" STEM\nMATERIAL: VIRGIN PEEK VGS 5.2053.1.1","VG-300 VALVE PSL-2 (TESTED TO PSL-3G UPON ASSEMBLY)\nMATERIAL CERTIFICATE EN 10204 TYPE 3.1 VALID FOR METALLIC PARTS ONLY\nFOR ELASTOMERS, COMPLETE MANUFACTURING RECORDS INCLUDING MANUFACTURING\nDATE, DUROMETER RATING, ETC. SHALL BE SUPPLIED.","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nVALVE PART,STEM,BUSHING\nTYPE: VG-300,FOR 1-1/8\" STEM\nVIRGIN PEEK PER VGS 5.2053.1 VGS5.2053.1.1 (PSL 1-3) VGS5.2053.1.2 (PSL\n4)","","","","","BUSHING:\nTYPE: BUSHING VG-300 VALVE\nSIZE: 1-1/8\" STEM\nMATERIAL: VIRGIN PEEK VGS 5.2053.1.1","ZGMD_BUSH_NM","PD",0,0,0,{"v":95,"d":"95.00"}]
[1000754,"RETR:THR P RETR SLV,1-1/8\" STM,VG-300 V>",null,null,"EA","XMT","4000005","GE-VETCO / UK","H130892-2","RETAINER:\nTYPE: THRUST PIN RETAINER SLEEVE\nSIZE: 1-1/8\" STEM, VG-300 VALVE\nMATERIAL: CARBON STEEL","","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nVALVE PART,THRUST PIN RETAINER SLEEVE:\nTYPE: VG-300 FOR 1-1/8\" STEM\nMETALLURGY: CARBON STEEL","","","","","RETAINER:\nTYPE: THRUST PIN RETAINER SLEEVE\nSIZE: 1-1/8\" STEM, VG-300 VALVE\nMATERIAL: CARBON STEEL","ZGMD_RETR_NM","PD",0,0,0,{"v":68,"d":"68.00"}]
[1000755,"SCREW:SET;0.25\",20UNRC-3A,0.375\",CNE,HX>",null,null,"EA","XMT","4000005","GE-VETCO / UK","199868-42","SCREW:SET;\nDIAMETER: 0.25\"\nTHREADS: 20UNRC-3A\nLENGTH: 0.375\"\nPOINT: CONE\nHEAD: HEX SOCKET\nMATERIAL: AS PER ASTM F912\nSPECIFICATION: W/LOC-WELL INSERT OR EQUIVALEN\n","","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nSET SCREW, HEX SOCKET\nDIMENSION: .250-20UNRC -3A X 0.375LG,CONE PT\nSTANDARD: ASTM F912\nCOAT PER=PLAIN - NOT COATED, W/LOC-WELL INSERT OR EQUIV","","","","","SCREW:SET;\nDIAMETER: 0.25\"\nTHREADS: 20UNRC-3A\nLENGTH: 0.375\"\nPOINT: CONE\nHEAD: HEX SOCKET\nMATERIAL: AS PER ASTM F912\nSPECIFICATION: W/LOC-WELL INSERT OR EQUIVALEN\n","ZGMD_SCRW_SET","PD",0,0,0,{"v":7,"d":"7.00"}]
[1000756,"VLV PRT,GATE ACTING, 4-1/8\" 5K,INC 625","VLV","VALVE","EA","WEL","4000005","GE-VETCO / UK","H133469-8","VALVE PART, GATE, REV ACTING:\nSIZE <(>&<)> PRESSURE: 4-1/8\",  5000 PSI MSP\nMODEL VG-300S, SPLIT\nMETALLURGY: INCONEL 625 NACE, TUNGSTEN CARBIDE COATED","","","06 June 2017 PO Long text as per belowr below:\nVALVE PART, GATE, REV ACTING:\nSIZE <(>&<)> PRESSURE: 4-1/8\",  5000 PSI MSP\nMODEL VG-300S, SPLIT\nMETALLURGY: INCONEL 625 NACE, TUNGSTEN CARBIDE COATED","","","","","-","-","PD",0,0,0,{"v":8505,"d":"8,505.00"}]
[1000757,"PLATE:NAME;NME PLT,VLV ASSY,API 6A,3.0 >","VLV","VALVE","EA","XMT","4000005","GE-VETCO / UK","R130057-1","PLATE:NAME;\nTYPE: NAME PLATE\nDESIGNATION: VALVE ASSEMBLY, API 6A\nSIZE: 3.0 X 2.5 X 26 SWG\nMATERIAL: 18-8 SS, GE","","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nNAMEPLATE,VALVE ASSEMBLY:\nCERTIFICATION: API 6A\nDIMENSION: 3.00 X 2.50 X 26 SWG, 18-8 SS, GE","","","","","PLATE:NAME;\nTYPE: NAME PLATE\nDESIGNATION: VALVE ASSEMBLY, API 6A\nSIZE: 3.0 X 2.5 X 26 SWG\nMATERIAL: 18-8 SS, GE","ZGMD_PLT_NAME","PD",0,0,0,{"v":28.8,"d":"28.80"}]
[1000758,"SCREW:DRV SCRW,0.25\",2\",RND,18-8 SS,GE,>",null,null,"EA","XMT","4000005","GE-VETCO / UK","191055-17","SCREW:\nTYPE: DRIVE SCREW\nLENGTH: 0.25\"\nSIZE: 2\"\nHEAD: ROUND\nMATERIAL: 18-8 SS, GE\nSPECIFICATION: DRIVE-U\nGRADE: PLAIN - NOT COATED","","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nDRIVE SCREW, ROUND HEAD\nDRIVE-U SIZE 2 X 0.250 LG\nMATL PER=18-8,COAT PER=PLAIN - NOT COATED","","","","","SCREW:\nTYPE: DRIVE SCREW\nLENGTH: 0.25\"\nSIZE: 2\"\nHEAD: ROUND\nMATERIAL: 18-8 SS, GE\nSPECIFICATION: DRIVE-U\nGRADE: PLAIN - NOT COATED","ZGMD_SCRW_NM","PD",0,0,0,{"v":4,"d":"4.00"}]
[1000759,"BOLT:EYE;SHLD EYEBOLT,1.125\",8UNC-2A,2.>",null,null,"EA","XMT","4000005","GE-VETCO / UK","R300737-1","BOLT:EYE;\nTYPE: SHOULDER EYEBOLT\nDIAMETER: 1.125\"\nTHREADS: 8UNC-2A\nLENGTH: 2.5\" SHANK\nTHREAD LENGTH: 2.5\" EYE ID\nMATERIAL: FORGED CARBON STEEL\n","NOC COATING STANDARD UPON FULL XMAS TREE ASSEMBLY","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nEYEBOLT, SHOULDER:\nSHANK LENGTH: 1.125-8UNC-2A X 2.500\nID: 2.500 EYE\nMETALLURGY: MATERIAL PER FORGED CARBON STEEL, COATING PLAIN - NOT COATED","","","","","BOLT:EYE;\nTYPE: SHOULDER EYEBOLT\nDIAMETER: 1.125\"\nTHREADS: 8UNC-2A\nLENGTH: 2.5\" SHANK\nTHREAD LENGTH: 2.5\" EYE ID\nMATERIAL: FORGED CARBON STEEL\n","ZGMD_BLT_EYE","PD",0,0,0,{"v":358,"d":"358.00"}]
[1000760,"STUD:ALLTHD;1.25\",8UN-2A,5.63\",5.63\" IS>",null,null,"EA","XMT","4000005","GE-VETCO / UK","H300518-7","STUD:ALL-THREAD;\nDIAMETER: 1.25\"\nTHREADS: 8UN-2A\nLENGTH: 5.63\"\nSIZE: 5.63\" IS THREAD LENGTH NOT OAL\nMATERIAL: CHAMFER AT EACH END\nSPECIFICATION: ASTM A320\nGRADE: GR L7","COATING AS PER VGS6.2.10.9","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","STUD:ALL-THREAD;\nDIAMETER: 1.25\"\nTHREADS: 8UN-2A\nLENGTH: 5.63\"\nSIZE: 5.63\" IS THREAD LENGTH NOT OAL\nMATERIAL: CHAMFER AT EACH END\nSPECIFICATION: ASTM A320\nGRADE: GR L7","ZGMD_STUD_ALLTHD","PD",0,0,0,{"v":25,"d":"25.00"}]
[1000761,"NUT:HEX;HVY,1.25\",8UN-2B,A194,GR-2H",null,null,"EA","WEL","4000005","GE-VETCO / UK","H300083-173","NUT:HEX;\nTYPE: HEAVY\nDIAMETER: 1.25\"\nTHREADS: 8UN-2B\nSPECIFICATION: ASTM A194\nGRADE: GR-2H","COATING PER VGS6.2.10.9","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","100139790","NUT:HEX;\nTYPE: HEAVY\nDIAMETER: 1.25\"\nTHREADS: 8UN-2B\nSPECIFICATION: ASTM A194\nGRADE: GR-2H","ZGMD_NUT_HX","PD",80,0,0,6.75]
[1000762,"O-RING:AS-568A,20.120\",0.555\" CS,MOLDED>",null,null,"EA","XMT","4000005","GE-VETCO / UK","R300787-2","O-RING:\nTYPE: AS-568A\nINSIDE DIAMETER: 20.120\"\nWIDTH: 0.555\" CS\nMATERIAL: MOLDED NITRILE 70 DURO\n","FULL TRACEABILITY FOR ELASTOMERS IN TERMS OF MANUFACTURING BATCH, DATE,\nDUROMETER RATINGS, ETC. SHALL BE SUBMITTED.","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nO-RING:\nTYPE: AS-568A\nID: 20.120\"\nCS: 0.555\"\nMETALLURGY: MOLDED NITRILE, 70 DURO","","","","","O-RING:\nTYPE: AS-568A\nINSIDE DIAMETER: 20.120\"\nWIDTH: 0.555\" CS\nMATERIAL: MOLDED NITRILE 70 DURO\n","ZGMD_O_RNG_NM","PD",0,0,0,{"v":196,"d":"196.00"}]
[1000763,"CONN:NT-2-DT A-ROT PLT,13-5/8\" 5000 PSI>",null,null,"EA","XMT","4000005","GE-VETCO / UK","H72717-1","CONNECTOR:\nTYPE: NT-2-DT ANTI-ROTATION PLATE\nSIZE: 13-5/8\" 5000 PSI\nMATERIAL: MILD STEEL\nCONNECTION: NT-2-DT XMAS TREE BTM","LOW STRESS MARK H72717-1(REV)\nDIMENSIONS: A = 25.00 +/-.12 B = 19.67 +/-.03 C = 23.50 +/-.03","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nCONNECTOR-WELLHEAD PART,NT-2-DT,ANTI-ROTATION PLATE:\nDIAMETER: 13-5/8\" 5000\nMETALLURGY: MILD STEEL\n2. LOW STRESS MARK H72717-1 (REV)\nDIMENSIONS: A = 25.00 +/-.12 B = 19.67 +/-.03 C = 23.50 +/-.03","","","","","CONNECTOR:\nTYPE: NT-2-DT ANTI-ROTATION PLATE\nSIZE: 13-5/8\" 5000 PSI\nMATERIAL: MILD STEEL\nCONNECTION: NT-2-DT XMAS TREE BTM","ZGMD_CNNT_NM","PD",0,0,0,{"v":881,"d":"881.00"}]
[1000764,"SCREW:CAP;0.5\",13UNRC-3A,1\",SKT (1960 S>",null,null,"EA","XMT","4000005","GE-VETCO / UK","6503054500","SCREW:CAP;\nDIAMETER: 0.5\"\nTHREADS: 13UNRC-3A\nLENGTH: 1\"\nHEAD: SOCKET (1960 SERIES)\nSPECIFICATION: ASTM A574\n","COATING AS PER VGS6.3.1.2.2\n","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nCAP SCREW:\nSOCKET HEAD (1960 SERIES)\nDIMENSION: 0.500-13UNRC -3A X 1.000LG\nMETALLURGY MATL PER=ASTM A574\nCOAT PER=VGS6.3.1.2.2","","","","","SCREW:CAP;\nDIAMETER: 0.5\"\nTHREADS: 13UNRC-3A\nLENGTH: 1\"\nHEAD: SOCKET (1960 SERIES)\nSPECIFICATION: ASTM A574\n","ZGMD_SCRW_CAP","PD",0,0,0,{"v":6,"d":"6.00"}]
[1000765,"INJECTION FITTING,STYLE 300 ,5-3/16 LG",null,null,"EA","DRL","4000005","GE-VETCO / UK","H133930-60","VALVE PART,INJECTION FITTING,STYLE 300 CLAD\nSIZE: 5/8\"-18UNF-2A,W/1/8 LP CONN\nMETALLURGY: 75K HIP ALLOY 625 NACE MR-01-75\nW/112 O-RING,70 DURO,HNBR,5-3/16\" LG","","","06 June 2017 PO Long text as per belowr below:\nVALVE PART,INJECTION FITTING,STYLE 300 CLAD\nSIZE: 5/8\"-18UNF-2A,W/1/8 LP CONN\nMETALLURGY: 75K HIP ALLOY 625 NACE MR-01-75\nW/112 O-RING,70 DURO,HNBR,5-3/16\" LG","","","","","-","-","PD",0,0,0,{"v":1214,"d":"1,214.00"}]
[1000766,"TREE CAP HUB,4-1/16\" 5M, E42,INC 718",null,null,"EA","DRL","4000005","GE-VETCO / UK","R72269-2","TREE CAP PART, BLIND HUB:\nSIZE <(>&<)> PRESSURE: 4-1/16\" 5M\nCONNECTION: E42 GRAYLOC BTM X BLIND TOP,W/ 1/2 NPT TAP\nMETALLURGY: INCONEL 718","","","06 June 2017 PO Long text as per below:\nTREE CAP PART, BLIND HUB:\nSIZE <(>&<)> PRESSURE: 4-1/16\" 5M\nCONNECTION: E42 GRAYLOC BTM X BLIND TOP,W/ 1/2 NPT TAP\nMETALLURGY: INCONEL 718","","","","","-","-","PD",0,0,0,{"v":7933,"d":"7,933.00"}]
[1000767,"TREE CAP ADAPTER BODY 4-1/16 5M -HHTRIM",null,null,"EA","DRL","4000005","GE-VETCO / UK","R130766-2","TREE CAP PART, ADAPTER, BODY:\nSIZE: 4-1/16\"\n5M FLG W/42GRS BTM X E42 GRAYLOC HUB TOP","","","06 June 2017 PO Long text as per belowr below:\nTREE CAP PART, ADAPTER, BODY:\nSIZE: 4-1/16\"\n5M FLG W/42GRS BTM X E42 GRAYLOC HUB TOP","","","","","-","-","PD",0,0,0,{"v":10447,"d":"10,447.00"}]
[1000768,"CLAMP:GRAYLOC 1045 CS,E,8.500 LG,2PC 4B>",null,null,"EA","DRL","4000005","GE-VETCO / UK","R90068-1","CLAMP:\nTYPE: GRAYLOC 1045 CS,E\nSIZE/CAPACITY: 8.500 LG\nNUMBER OF BOLTS: 2PC 4BOLT\nMATERIAL: CS","C/W BOLTING, STUD/TWO NUTS,SPH FACE, 1.000-8UNC-2\nMETALLURGY: ZINC NICKEL COATED A320-L7 STUD AND A194-GR7 NUTS\n\nCOATING AS PER NOC STANDARDS\n\nEQUIVALENT GRAYLOC PART NUMBERS AS FOLLOWS:\n\nA90047-72WB - CLAMP 5/E, ASTM A193 B7, TSA COATING\nA300105-267 - STUDS/NUTS FOR 5/E CLAMP, ASTM A320 L7/A194 GR7, ZINC\nNICKEL COATING\n\nCLAMP AND BOLTS DELIVERED ASSEMBLED\n","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nGRAYLOC CLAMP,2PC 4BOLT, E\nLG: 8.500\nCS: 1045 ,C/W BOLTING, STUD/TWO NUTS,SPH FACE, 1.000-8UNC-2\nMETALLURGY: ZINC NICKEL COATED SA320-L7 STUD AND SA194-GR2H NUTS","","","","","CLAMP:\nTYPE: GRAYLOC 1045 CS,E\nSIZE/CAPACITY: 8.500 LG\nNUMBER OF BOLTS: 2PC 4BOLT\nMATERIAL: CS","ZGMD_CLMP_NM","PD",0,0,0,416.49]
[1000769,"PLUG:PIPE;0.5\",HX,1/2\" LP,5000PSI,INC 6>",null,null,"EA","XMT","4000005","GE-VETCO / UK","383933","PLUG:PIPE;\nSIZE: 0.5\"\nHEAD: HEX\nCONNECTION: 1/2\" LP\nRATING: 5000PSI\nMATERIAL: INC 625\nSPECIFICATION: NACE\n","1-1/4 LG,W/SOLID NOSE","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nPLUG,PIPE:\nTYPE: 0.500\" LP W/ 1 LG HEX HD\nMETALLURGY: INCONEL 725","","","","","PLUG:PIPE;\nSIZE: 0.5\"\nHEAD: HEX\nCONNECTION: 1/2\" LP\nRATING: 5000PSI\nMATERIAL: INC 625\nSPECIFICATION: NACE\n","ZGMD_PLG_PIPE","PD",0,0,0,{"v":493,"d":"493.00"}]
[1000770,"TEE BODY ,4-1/16\", 5M-HH TRIM",null,null,"EA","DRL","4000005","GE-VETCO / UK","R130889-2","TEE PART, BODY:\nSIZE: 4-1/16\"\n5M FLG W/42GRS X 2-1/16 5M\nTUDDED W/20GRS X 4-1/16 5M STUDDED W/42GRS","","","06 June 2017 PO Long text as per belowr below:\nTEE PART, BODY:\nSIZE: 4-1/16\"\n5M FLG W/42GRS X 2-1/16 5M\nTUDDED W/20GRS X 4-1/16 5M STUDDED W/42GRS","","","","","-","-","PD",0,0,0,{"v":18947,"d":"18,947.00"}]
[1000771,"INSERT:INSRT PRT,1-1/4-8UN-2A X 7.25 LG>",null,null,"EA","DRL","4000005","GE-VETCO / UK","R130889-23","INSERT:\nTYPE: INSERT PORT\nSIZE: 1-1/4-8UN-2A X 7.25 LG\nMATERIAL: INCONEL 625\n","SIZE: 1-1/4-8UN-2A X 7.25 LG, A/F 1/2 LP","","06 June 2017 PO Long text as per belowr below:\nINSERT, PORT:\nSIZE: 1-1/4-8UN-2A X 7.25 LG, A/F 1/2 LP\nMETALLURGY: INCONEL 625","","","","","INSERT:\nTYPE: INSERT PORT\nSIZE: 1-1/4-8UN-2A X 7.25 LG\nMATERIAL: INCONEL 625\n","ZGMD_INSRT_NM","PD",0,0,0,{"v":343,"d":"343.00"}]
[1000772,"STUD:ALLTHD;0.875\",9UNC-2A,4\",4\" THRD L>",null,null,"EA","XMT","4000005","GE-VETCO / UK","R301234-874","STUD:ALL-THREAD;\nDIAMETER: 0.875\"\nTHREADS: 9UNC-2A\nLENGTH: 4\"\nSIZE: 4\" THREAD LENGTH NOT OAL\nSPECIFICATION: ASTM A320\nGRADE: GR L7","COATING AS PER VGS6.2.10.9","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","STUD:ALL-THREAD;\nDIAMETER: 0.875\"\nTHREADS: 9UNC-2A\nLENGTH: 4\"\nSIZE: 4\" THREAD LENGTH NOT OAL\nSPECIFICATION: ASTM A320\nGRADE: GR L7","ZGMD_STUD_ALLTHD","PD",0,0,0,{"v":32,"d":"32.00"}]
[1000773,"NUT:HEX;HVY,7/8\",9UNC-2B,A194,GR-2H",null,null,"EA","XMT","4000005","GE-VETCO / UK","R301263-22","NUT:HEX;\nTYPE: HEAVY\nDIAMETER: 7/8\"\nTHREADS: 9UNC-2B\nSPECIFICATION: ASTM A194\nGRADE: GR-2H","COATING AS PER VGS6.2.10.9","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","NUT:HEX;\nTYPE: HEAVY\nDIAMETER: 7/8\"\nTHREADS: 9UNC-2B\nSPECIFICATION: ASTM A194\nGRADE: GR-2H","ZGMD_NUT_HX","PD",0,0,0,18.24]
[1000774,"VALVE  BODY,4-1/16 5K, INC625 CLAD",null,null,"EA","DRL","4000005","GE-VETCO / UK","H385856-1","VALVE PART, BODY, FLG X GRAYLOC:\nSIZE: 4-1/16\"\nPRESSURE: 5000 PSI MSP\nMODEL VG-300\nSTANDARD: 75K LA NACE, I/T -20F, PSL2\nMETALLURGY: W/INCONEL 625 FULL CLAD\nCONNECTION: W/42GRS END X 6 GR52 GRAYLOC END","","","06 June 2017 PO Long text as per belowr below:\nVALVE PART, BODY, FLG X GRAYLOC:\nSIZE: 4-1/16\"\nPRESSURE: 5000 PSI MSP\nMODEL VG-300\nSTANDARD: 75K LA NACE, I/T -20F, PSL2\nMETALLURGY: W/INCONEL 625 FULL CLAD\nCONNECTION: W/42GRS END X 6 GR52 GRAYLOC END","","","","","-","-","PD",0,0,0,{"v":17988,"d":"17,988.00"}]
[1000775,"S/BLT:1.125\",7.5\",8UNR-2A BOTH ENDS,TAP>",null,null,"EA","XMT","4000005","GE-VETCO / UK","H300411-265","STUDBOLT:\nDIAMETER: 1.125\"\nLENGTH: 7.5\"\nTHREADS: 8UNR-2A BOTH ENDS\nMATERIAL: TAP END PER VGS2.4.13\nSPECIFICATION: ASTM A320\nGRADE: GRL7M\nSURFACE TREATMENT: VGS6.2.10.9\nNUT: SINGLE NUT\nMATERIAL DATASHEET: ASTM A194, GR2HM\n","","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nSTUD W/ONE NUT, TAP END,PER VGS2.4.13\nSIZE: 1.125-8UNR-2A X 1.125-8UNR-2A, 7.500 LG\nSTANDARD:\nSTUD MATERIAL PER ASTM A320 GRL7M\nNUT MATERIAL PER ASTM A194 GR2HM, COATING PER VGS6.2.10.9","","","","","STUDBOLT:\nDIAMETER: 1.125\"\nLENGTH: 7.5\"\nTHREADS: 8UNR-2A BOTH ENDS\nMATERIAL: TAP END PER VGS2.4.13\nSPECIFICATION: ASTM A320\nGRADE: GRL7M\nSURFACE TREATMENT: VGS6.2.10.9\nNUT: SINGLE NUT\nMATERIAL DATASHEET: ASTM A194, GR2HM\n","ZGMD_STUDBOLT_NM","PD",0,0,0,{"v":34,"d":"34.00"}]
[1000776,"PLATE:NAME;VLV ASSY,API 6A,1.75\" X 4.5\">","VLV","VALVE","EA","XMT","4000005","GE-VETCO / UK","H130465-2","PLATE:NAME;\nTYPE: VALVE ASSEMBLY\nDESIGNATION: API 6A\nSIZE: 1.75\" X 4.5\"\nMATERIAL: 304SS","","CERTIFICATE OF CONFORMITY\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nNAMEPLATE,VALVE ASSEMBLY:\nTYPE: API 6A SSV OR USV 1.750 X 4.500,304SS","","","","","PLATE:NAME;\nTYPE: VALVE ASSEMBLY\nDESIGNATION: API 6A\nSIZE: 1.75\" X 4.5\"\nMATERIAL: 304SS","ZGMD_PLT_NAME","PD",0,0,0,{"v":137,"d":"137.00"}]
[1000777,"ACTUATOR BONNET,RV, 4-1/16\" ,5K-HH TRIM",null,null,"EA","DRL","4000005","GE-VETCO / UK","R300729-11","ACTUATOR, MODEL RV, HYDRAULIC, W/ BONNET ASSY :\nTYPE: FOR 4-1/16\", 5,000 PSI VG-300 VALVE,HH TRIM\nC/W PEPPERL AND FUCHS PROXIMITY SENSOR, ROUNDED SWITCH COVER BOX AND\nVIEW WINDOW\nOD MAXIMUM HOUSING : 8.5 INCHES MAX\nOPERATING PRESSURE: 9,500 PSI\nHYDRAULIC CONNECTION: 1/2\"NPT FEMALE","","","06 June 2017 PO Long text as per belowr below:\nACTUATOR, MODEL RV, HYDRAULIC, W/ BONNET ASSY :\nTYPE: FOR 4-1/16\", 5,000 PSI VG-300 VALVE,HH TRIM\nC/W PEPPERL AND FUCHS PROXIMITY SENSOR, ROUNDED SWITCH COVER BOX AND\nVIEW WINDOW\nOD MAXIMUM HOUSING : 8.5 INCHES MAX\nOPERATING PRESSURE: 9,500 PSI\nHYDRAULIC CONNECTION: 1/2\"NPT FEMALE","","","","","-","-","PD",0,0,0,0.01]
[1000778,"VALVE,2-1/16\" 5K ,API FLG, HH-1 TRIM",null,null,"EA","DRL","4000005","GE-VETCO / UK","H385861-1","VALVE, API FLG X GRAYLOC:\nSIZE <(>&<)> PRESSURE: 2-1/16\" 5000 PSI MSP\nTYPE: VG-300S, 2-1/16\" 5000 PSI FLG END\nMETALLURGY: HH-1 TRIM, W/20GRS END X B20 GRAYLOC END\nCERTIFICATION: API 6A U HH-NL PSL2 PR2","","","06 June 2017 PO Long text as per belowr below:\nVALVE, API FLG X GRAYLOC:\nSIZE <(>&<)> PRESSURE: 2-1/16\" 5000 PSI MSP\nTYPE: VG-300S, 2-1/16\" 5000 PSI FLG END\nMETALLURGY: HH-1 TRIM, W/20GRS END X B20 GRAYLOC END\nCERTIFICATION: API 6A U HH-NL PSL2 PR2","","","","","-","-","PD",0,0,0,{"v":27821.76,"d":"27,821.76"}]
[1000779,"HUB:BLD;GRAYLOC,BLD,B20,NACE INC 718",null,null,"EA","DRL","4000005","GE-VETCO / UK","A90052-8","HUB:BLIND;\nTYPE: GRAYLOC, BLIND\nPIPE SIZE: B20\nMATERIAL: NACE INCONEL 718\n","W/1/2\" LP TAP 120K\n","","06 June 2017 PO Long text as per belowr below:\nGRAYLOC HUB, BLIND\nTYPE: B20, W/1/2\" LP TAP 120K\nMETALLURGY: NACE INCONEL 718","","","","","HUB:BLIND;\nTYPE: GRAYLOC, BLIND\nPIPE SIZE: B20\nMATERIAL: NACE INCONEL 718\n","ZGMD_HB_BLD","PD",0,0,0,{"v":1146.85,"d":"1,146.85"}]
[1000780,"CLAMP:GRAYLOC,B,6.75\" LG,2PC 4BOLT,AISI>",null,null,"EA","DRL","4000005","GE-VETCO / UK","H90502-26","CLAMP:\nTYPE: GRAYLOC ,B\nSIZE/CAPACITY: 6.75\" LG\nNUMBER OF BOLTS: 2PC 4BOLT\nMATERIAL: AISI 1040","METALLURGY: AISI 1040,C/W BOLTING,STUD/TWO NUTS, 0.875-9UNC-2\n\nCOATING AS PER NOC STANDARDS\n\nEQUIVALENT GRAYLOC PART NUMBERS AS FOLLOWS:\n\nA90031-87WB - CLAMP B, ASTM A193 B7, TSA COATING\n145661 - STUDS/NUTS FOR B CLAMP, ASTM A320 L7/A194 GR7, ZINC NICKEL\nCOATING\n\nCLAMP AND BOLTS DELIVERED ASSEMBLED","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","","","","","","CLAMP:\nTYPE: GRAYLOC ,B\nSIZE/CAPACITY: 6.75\" LG\nNUMBER OF BOLTS: 2PC 4BOLT\nMATERIAL: AISI 1040","ZGMD_CLMP_NM","PD",0,0,0,284.34]
[1000781,"VG-SEAL RING, 20, ALLOY 718 NACE",null,null,"EA","DRL","4000005","GE-VETCO / UK","H139000-78","VG-SEAL RING, 20, HIGH STRENGTH:\nMETALLURGY: ALLOY 718 NACE, MOS2 W/GRAPHITE COATED","","","06 June 2017 PO Long text as per belowr below:\nVG-SEAL RING, 20, HIGH STRENGTH:\nMETALLURGY: ALLOY 718 NACE, MOS2 W/GRAPHITE COATED","","","","","-","-","PD",0,0,0,{"v":1124.53,"d":"1,124.53"}]
[1000782,"O-RING:AS568A-451,10.975\" (NOM. 11\"),0.>",null,null,"EA","XMT","4000005","GE-VETCO / UK","195000-451","O-RING:\nTYPE: AS568A-451\nINSIDE DIAMETER: 10.975\" (NOM. 11\")\nWIDTH: 0.275\" (NOM 0.25\")\nMATERIAL: NITRILE (NBR) VGS5.1010.1.1\nINDUSTRY STANDARD: FOR API 6A PSL-3\nADDITIONAL INFORMATION: 70 DURO A","FULL MANUFACTURING TRACEABILITY IN TERMS OF DATE, BATCH, DUROMETER, ETC\nSHALL BE PROVIDED","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nO-RING, AS568A-451\nID: 10.975\" (NOM 11)\nCS: 0.275\" (NOM 1/4)","","","","","O-RING:\nTYPE: AS568A-451\nINSIDE DIAMETER: 10.975\" (NOM. 11\")\nWIDTH: 0.275\" (NOM 0.25\")\nMATERIAL: NITRILE (NBR) VGS5.1010.1.1\nINDUSTRY STANDARD: FOR API 6A PSL-3\nADDITIONAL INFORMATION: 70 DURO A","ZGMD_O_RNG_NM","PD",0,0,0,{"v":41,"d":"41.00"}]
[1000783,"O-RING:AS568A-443,7.475\" (NOM. 7.5\"),0.>",null,null,"EA","XMT","4000005","GE-VETCO / UK","195000-443","O-RING:\nTYPE: AS568A-443\nINSIDE DIAMETER: 7.475\" (NOM. 7.5\")\nWIDTH: 0.275\" (NOM. 0.25\") CS\nMATERIAL: NITRILE (NBR) VGS5.1010.1.1\nINDUSTRY STANDARD: FOR API 6A, PSL-3\nADDITIONAL INFORMATION: 70 DURO A","FULL MANUFACTURING TRACEABILITY IN TERMS OF DATE, BATCH, DUROMETER, ETC.\nSHALL BE SUBMITTED","CERTIFICATE OF CONFORMITY\nMATERIAL CERTIFICATE EN 10204 3.1\nQC PATH 2 – DOC PRE-REVIEW+WH INSPECTION","06 June 2017 PO Long text as per belowr below:\nO-RING, AS568A-443:\nID: 7.475 (NOM 7-1/2\")\nCS: 0.275 (NOM 1/4\")","","","","","O-RING:\nTYPE: AS568A-443\nINSIDE DIAMETER: 7.475\" (NOM. 7.5\")\nWIDTH: 0.275\" (NOM. 0.25\") CS\nMATERIAL: NITRILE (NBR) VGS5.1010.1.1\nINDUSTRY STANDARD: FOR API 6A, PSL-3\nADDITIONAL INFORMATION: 70 DURO A","ZGMD_O_RNG_NM","PD",0,0,0,{"v":19,"d":"19.00"}]
[1000784,"ACTUATOR BONNET,CSWC, 4-1/16\" 5K-HH TRIM",null,null,"EA","DRL","4000005","GE-VETCO / UK","R300729-10","ACTUATOR, MODEL CSWC\nHYDRAULIC WIRE-CUTTING ACTUATOR, C/W BONNET ASSY W/ BACKSEAT, FOR 4-\n1/16\"5,000 PSI VG-300 VALVE\nW/ SIDE MOUNT LIMIT SWITCH ASSY AND QUICK DISCONNECT (WITH PEPPERLAND\nFUCHS PROXIMITY SENSOR)\nMAXIMUM HOUSING OD: 12 INCHES MAX\nOPERATING PRESSURE: 9,500 PSI\nDISPLACEMENT VOLUME: 63 CUBIC INCHES","","","06 June 2017 PO Long text as per belowr below:\nACTUATOR, MODEL CSWC\nHYDRAULIC WIRE-CUTTING ACTUATOR, C/W BONNET ASSY W/ BACKSEAT, FOR 4-\n1/16\"5,000 PSI VG-300 VALVE\nW/ SIDE MOUNT LIMIT SWITCH ASSY AND QUICK DISCONNECT (WITH PEPPERLAND\nFUCHS PROXIMITY SENSOR)\nMAXIMUM HOUSING OD: 12 INCHES MAX\nOPERATING PRESSURE: 9,500 PSI\nDISPLACEMENT VOLUME: 63 CUBIC INCHES","","","","","-","-","PD",0,0,0,0.01]
[1000786,"CTRL:CPU 417-5H,24VDC,ASDCY-10-I01004-4>","CTR","CENTRALISER","EA","CNT","4000138","SIEMENS A/S","6ES7417-5HT06-0AB0","CONTROLLER:\nTYPE: CPU 417-5H\nRATING: 24VDC\nDRAWING/DOCUMENT REFERENCE-1: ASDCY-10-I01004-4101_SH.41\nDRAWING/DOCUMENT REFERENCE-2: ASYYY-10-I01199-2700_SH.112","SIMATIC S7-400H, CPU 417-5H\nCENTRAL PROCESSING UNIT FOR S7-400H AND S7-400F/FH\n5 INTERFACES: 1X MPI/DP, 1X DP,\n1X PN AND 2 FOR SYNC MODULES\n32 MB MEMORY (16 MB DATA/16 MB CODE)\n\nSEE ATTACHED.","","08 June 2017 PO Long text as per below:\nCPU:SIMATIC\nMODEL:SIMATIC S7-400H, CPU 417-5H\nCENTRAL UNIT FOR S7-400H AND S7-400F/FH\n5 INTERFACES: 1X MPI/DP, 1X DP,1X PN AND 2 FOR SYNC MODULES 32 MB MEMORY\n16 MB DATA/16 MB CODE)","","","","","CONTROLLER:\nTYPE: CPU 417-5H\nRATING: 24VDC\nDRAWING/DOCUMENT REFERENCE-1: ASDCY-10-I01004-4101_SH.41\nDRAWING/DOCUMENT REFERENCE-2: ASYYY-10-I01199-2700_SH.112","ZGMD_CTRLR_NM","PD",2,0,0,{"v":15637.11,"d":"15,637.11"}]
[1000787,"MODULE:V6 SYNCHRONIZATION,220MA,ASDCY-1>",null,null,"EA","CNT","4000138","SIEMENS A/S","6ES7960-1AA06-0XA0","MODULE:\nTYPE: V6 SYNCHRONIZATION\nRATING: 220MA\nDRAWING/DOCUMENT REFERENCE-1: ASDCY-10-I01004-4101_SH.41\nDRAWING/DOCUMENT REFERENCE-2: ASYYY-10-I01199-2700_SH.242","SYNC. SUBMODULE FOR SIMATIC S7-400H(for HT06 CPU's)\n\nSEE ATTACHED.","","08 June 2017 PO Long text as per below:\nSYNC MODULE:\nMODEL: SYNC. SUBMODULE FOR SIMATIC S7-400H(for HT06 CPU's)\n","","","","","MODULE:\nTYPE: V6 SYNCHRONIZATION\nRATING: 220MA\nDRAWING/DOCUMENT REFERENCE-1: ASDCY-10-I01004-4101_SH.41\nDRAWING/DOCUMENT REFERENCE-2: ASYYY-10-I01199-2700_SH.242","ZGMD_MOD_NM","V1",0,5,8,520.88]
[1000788,"PROCR:CP 443-1 COMM,10-100MBIT/S,5VDC,A>",null,null,"EA","CNT","4000138","SIEMENS A/S","6GK7443-1EX30-0XE0","PROCESSOR:\nTYPE: CP 443-1 COMMUNICATION\nRATING: 10-100MBIT/S\nSUPPLY: 5VDC\nDRAWING/DOCUMENT REFERENCE-1: ASDCY-10-I01004-4101_SH.41\nDRAWING/DOCUMENT REFERENCE-2: ASYYY-10-I01199-2700_SH.125","MODEL: SIMATIC NET CP 443-1 2 X 10/100 MBITS/S (IE SWITCH RJ 45 PROTS)\nISO TCP; UDP\nPROFINET-IO CONTROLLER; S7- COMMUNICATION\nOPEN COMMUNICATION (SENT/RECEIVE) S7-ROUTING\nIP-CONFIGRATION VIA DHCP/BLOCK\nIP ACCESS CONTROL LIST\nTIME SYNCHRONISATION\nEXTENDED WEB-DIAGNOSIS; FAST STARTUP; PROFIENERGY SUPPORT\n\nSEE ATTACHED.","","08 June 2017 PO Long text as per below:\nCARD:\nMODEL: SIMATIC NET CP 443-1 2 X 10/100 MBITS/S (IE SWITCH RJ 45 PROTS)\nISO TCP; UDP\nPROFINET-IO CONTROLLER; S7- COMMUNICATION\nOPEN COMMUNICATION (SENT/RECEIVE) S7-ROUTING\nIP-CONFIGRATION VIA DHCP/BLOCK\nIP ACCESS CONTROL LIST\nTIME SYNCHRONISATION\nEXTENDED WEB-DIAGNOSIS; FAST STARTUP; PROFIENERGY SUPPORT.","","","","","PROCESSOR:\nTYPE: CP 443-1 COMMUNICATION\nRATING: 10-100MBIT/S\nSUPPLY: 5VDC\nDRAWING/DOCUMENT REFERENCE-1: ASDCY-10-I01004-4101_SH.41\nDRAWING/DOCUMENT REFERENCE-2: ASYYY-10-I01199-2700_SH.125","ZGMD_PROC_NM","PD",4,0,0,{"v":2754.83,"d":"2,754.83"}]
[1000792,"VLV,TRSCSSV,SP,5-1/2\",13CR","VLV","VALVE","EA","COM","4000007","HALLIBURTON USA SINGAPORE","102689489","TR-SCSSSV:TUBING RETRIEVABLE SURFACE CONTROLLED SUB-SURFACE SAFETY VALVE\nSIZE (IN.): 5.5 TO SET INSIDE 9-5/8\" 40 PPF\nMIN. INTERNAL WORKING PRESSURE: (PSI) 5,000\nMAX OD (IN.):7.69\"\nMIN ID (IN.):4.58\"\nTHREAD UP: 5-1/2' 15.5 LB/FT SL APEX BOX\nTHREAD DOWN: 5-1/2\" 15.5 LB/FT SL APEX PIN\nMETALLURGY: 13 CR /410 STAINLESS STEEL/ NICKEL ALLOY 925 NACE MR0175/\nISO 15156\nCLOSURE TYPE: FLAPPER\nSERVICE: H2S\nPRESSURE RATING (PSI): 5,000\nLOCK PROFILE RQ\n","","","13 June PO Long Text as per below:\nTR-SCSSSV:TUBING RETRIEVABLE SURFACE CONTROLLED SUB-SURFACE SAFETY VALVE\nSIZE (IN.): 5.5 TO SET INSIDE 9-5/8\" 40 PPF\nMIN. INTERNAL WORKING PRESSURE: (PSI) 5,000\nMAX OD (IN.):7.69\"\nMIN ID (IN.):4.58\"\nTHREAD UP: 5-1/2' 15.5 LB/FT SL APEX BOX\nTHREAD DOWN: 5-1/2\" 15.5 LB/FT SL APEX PIN\nMETALLURGY: 13 CR /410 STAINLESS STEEL/ NICKEL ALLOY 925 NACE MR0175/\nISO 15156\nCLOSURE TYPE: FLAPPER\nSERVICE: H2S\nPRESSURE RATING (PSI): 5,000\nLOCK PROFILE RQ\n","","","","","-","-","PD",0,0,0,{"v":53545,"d":"53,545.00"}]
[1000793,"SHKL:DEE,BLK CTD+GREASED PINS,126 MM,JA>",null,null,"EA","MAR","4001064","OIL Offspring International Ltd","","SHACKLE:\nTYPE: DEE\nMATERIAL: BLACK COATED + GREASED PINS\nDIAMETER: 126 MM\nINSIDE WIDTH: JAW GAP 170 MM\nINSIDE LENGTH: 450 MM","LTM END JOINING SHACKLE FOR DN90R4 CHAIN\nDRAWING REF 050712 REV.0C\nTESTS AND CONTROLS BY THIRD PARTY\nLTM TYPE ROUND PIN END JOINING SHACKLE TYPE D\nPIN DIAMETER 140 MM\nPALM DIAMETER 287 MM EST WEIGHT 260 KG\nBREAKING LOAD TEST 8170 KN\nPROOF LOAD TEST 6440 KN","CERTIFICATE OF CONFORMITY\nSURVEY/RELEASE NOTE- IN-SERVICE AGENCY\nQC PATH 3 – WH INSPECTION","","","","","","SHACKLE:\nTYPE: DEE\nMATERIAL: BLACK COATED + GREASED PINS\nDIAMETER: 126 MM\nINSIDE WIDTH: JAW GAP 170 MM\nINSIDE LENGTH: 450 MM","ZGMD_SHKL_NM","PD",2,0,0,{"v":10444.5,"d":"10,444.50"}]
[1000794,"HELMET:V GARD,ALL,SUMMER LNR","LNR","LINER","EA","PPE","","","","HELMET:\nTYPE: V GARD\nSIZE: ALL\nMATERIAL: SUMMER LINER\nCOLOUR:\nSTANDARD:","","","","","","","199139844","HELMET:\nTYPE: V GARD\nSIZE: ALL\nMATERIAL: SUMMER LINER\nCOLOUR:\nSTANDARD:","ZGMD_HELM_NM","V1",0,300,600,10.38]
[1000800,"ASSY,HPHOSE,NYLON,29\",0.375”IDx0.65”OD",null,null,"EA","SSE","4000028","SURVIVAL SYSTEMS INT. LTD.","8356-128B","HOSE:\nTYPE:\nSIZE:\nINLET CONNECTION:\nOUTLET CONNECTION:\nLENGTH:\nRATING:\nMATERIAL:\nCOLOUR:\nCONNECTION:","QC requirements:\n\nAdherence to SD-NOC-SAF-021","CERTIFICATE OF CONFORMITY\nPRESSURE TEST REPORTS\nQC PATH 3 – WH INSPECTION","\"HP HOSE ASSEMPLY\nHose Material: Nylon Tube, Urethane Cover, Aramid Fiber Reinforced.\nLength: 19 inches\nDiameter: 0.375” I.D x 0.65” O.D.\nMax. Working Pressure: 4,000 psi\nFittings:  Hose End, Female 37° SEA (JIC) Flare, Swivel, 3/8\"\" I.D. Hose\nx 3/8\"\" O.D. Tube x 9/16-18 UNF Pipe Thread\nFittings Material: Cad Plated Steel.\n\nBOM /KIT :\n\n\"LB 1: Serial number 292, QA.SA.D.007.ASADI-X-070608\nLB 2: Serial number 275, QA.SA.D.007.ASADI-X-070609\nLB 3: Serial number 293, QA.SA.D.007.ASADI-X-070610\"\n\n\n\n\n\n\n\n\"\n","","","","","HOSE:\nTYPE:\nSIZE:\nINLET CONNECTION:\nOUTLET CONNECTION:\nLENGTH:\nRATING:\nMATERIAL:\nCOLOUR:\nCONNECTION:","ZGMD_HOSE_NM","PD",2,0,0,388.62]
[1000801,"ADPT:ELB;37° FLR,0.375\" MPT X 0.5\" TBE,>",null,null,"EA","SSE","4000028","SURVIVAL SYSTEMS INT. LTD.","047-0113","ADAPTOR:ELBOW;\nDEGREE: 37° FLARE\nSIZE: 0.375\" MPT X 0.5\" TUBE\nMATERIAL: CAD PLATED STEEL","","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","\"Dimensions: 0.375” MPT x 0.5” Tube 37° Flare\nMaterial: Cad Plated Steel.\"\n\nBOM-KIT :\n\"LB 1: Serial number 292, QA.SA.D.007.ASADI-X-070608\nLB 2: Serial number 275, QA.SA.D.007.ASADI-X-070609\nLB 3: Serial number 293, QA.SA.D.007.ASADI-X-070610\"\n","","","","","ADAPTOR:ELBOW;\nDEGREE: 37° FLARE\nSIZE: 0.375\" MPT X 0.5\" TUBE\nMATERIAL: CAD PLATED STEEL","ZGMD_ADPT_ELB","PD",0,0,0,84.75]
[1000802,"VLV:CHECK;3/8 MPT X 3/8 MPT,HYD CLUSTER>","VLV","VALVE","EA","SSE","4000028","SURVIVAL SYSTEMS INT. LTD.","8442-000B","VALVE:CHECK;\nSIZE: 3/8 MPT X 3/8 MPT\nCONNECTION:\nTYPE: HYDRAULIC CLUSTER\nBODY MATERIAL: BRASS\nDRAWING/DOCUMENT REFERENCE-1: DWG-8442\n","","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","\"VALVE HYDRAULIC CHECK CLUSTER\n3/8MPT X 3/8 MPT\nMATERIAL: BRASS\nDRAWING REF: 8442\"\n\nBOM KIT :\n\"LB 1: Serial number 292, QA.SA.D.007.ASADI-X-070608\nLB 2: Serial number 275, QA.SA.D.007.ASADI-X-070609\nLB 3: Serial number 293, QA.SA.D.007.ASADI-X-070610\"\n","","","","","VALVE:CHECK;\nSIZE: 3/8 MPT X 3/8 MPT\nCONNECTION:\nTYPE: HYDRAULIC CLUSTER\nBODY MATERIAL: BRASS\nDRAWING/DOCUMENT REFERENCE-1: DWG-8442\n","ZGMD_VLV_CHK","PD",2,0,0,{"v":2367.08,"d":"2,367.08"}]
[1000803,"BUSH:0.375”NPTM X 0.25”NPTF",null,null,"EA","SSE","4000028","SURVIVAL SYSTEMS INT. LTD.","038-0169","BUSHING:\nSIZE: 0.375”NPTM X 0.25”NPTF\n","","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","\"Material: Cad Plated Steel\nSize: 0.375” NPT Male x 0.25” NPT Female\"\n\n\"LB 1: Serial number 292, QA.SA.D.007.ASADI-X-070608\nLB 2: Serial number 275, QA.SA.D.007.ASADI-X-070609\nLB 3: Serial number 293, QA.SA.D.007.ASADI-X-070610\"\n","","","","","BUSHING:\nSIZE: 0.375”NPTM X 0.25”NPTF\n","ZGMD_BUSH_NM","PD",0,0,0,4.21]
[1000804,"ADPT:ELB;90°,0.25\" OD TBE X 0.25\" NPT,(>",null,null,"EA","SSE","4000028","SURVIVAL SYSTEMS INT. LTD.","047-0035","ADAPTOR:ELBOW;\nDEGREE: 90°\nSIZE: 0.25\" OD TUBE X 0.25\" NPT\nCONNECTION: (7/16-20 UNF) X (M X M)\nMATERIAL: CAD PLATED STEEL","MALE - SAE 37° FLARE x IPS","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","\"Details:  Elbow 90°, Male - SAE 37°  FLARE x IPS\nSize: 0.25” O.D. Tube (7/16-20 UNF) x 0.25” NPT (Male x Male)\nMaterial: Cad Plated Steel.\n          \"\nBOM KIT\n\n\n\"LB 1: Serial number 292, QA.SA.D.007.ASADI-X-070608\nLB 2: Serial number 275, QA.SA.D.007.ASADI-X-070609\nLB 3: Serial number 293, QA.SA.D.007.ASADI-X-070610\"\n","","","","","ADAPTOR:ELBOW;\nDEGREE: 90°\nSIZE: 0.25\" OD TUBE X 0.25\" NPT\nCONNECTION: (7/16-20 UNF) X (M X M)\nMATERIAL: CAD PLATED STEEL","ZGMD_ADPT_ELB","PD",0,0,0,20.71]
[1000805,"T:SPP;",null,null,"EA","SSE","4000028","SURVIVAL SYSTEMS INT. LTD.","047-0090","TEE:SPP;","","CERTIFICATE OF CONFORMITY\nQC PATH 3 – WH INSPECTION","\"Details: Male - SAE 37°  x NPT\nSize: 0.5” Tube (3/4-16) Male x 0.375” NPT Female\n Material: Cad Plated Steel.\n\"\nBOM KIT\n\n\"LB 1: Serial number 292, QA.SA.D.007.ASADI-X-070608\nLB 2: Serial number 275, QA.SA.D.007.ASADI-X-070609\nLB 3: Serial number 293, QA.SA.D.007.ASADI-X-070610\"\n","","","","","TEE:SPP;","ZGMD_T_SPP","PD",0,0,0,29.87]
[1000806,"(BLCK)FAB:U BOLT-HDG (INSULATED) F/2\",P",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: U BOLT-HDG (INSULATED) FOR 2\"\nDescription FAB Materials 2: PIPE","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: U BOLT-HDG (INSULATED) FOR 2\"\nDescription FAB Materials 2: PIPE","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000807,"(BLCK)FAB:10'' P BY MT QLMXQLF 7000M,IPS",null,null,"M","FAB","","","","FABRICATION:\nDescription FAB Materials 1: 10'' PIPE BY MT QLMXQLF 7000M\nDescription FAB Materials 2: IPS","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: 10'' PIPE BY MT QLMXQLF 7000M\nDescription FAB Materials 2: IPS","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000808,"(BLCK)FAB:6'' ELB 90 QLF 7000M",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: 6'' ELBOW 90 QLF 7000M\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: 6'' ELBOW 90 QLF 7000M\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000809,"(BLCK)FAB:6'' P BY MT QLMXQLF 7000M I,PS",null,null,"M","FAB","","","","FABRICATION:\nDescription FAB Materials 1: 6'' PIPE BY MT QLMXQLF 7000M I\nDescription FAB Materials 2: PS","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: 6'' PIPE BY MT QLMXQLF 7000M I\nDescription FAB Materials 2: PS","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000810,"(BLCK)FAB:20'' P BY MT PEXPE 7000M IP,S",null,null,"M","FAB","","","","FABRICATION:\nDescription FAB Materials 1: 20'' PIPE BY MT PEXPE 7000M IP\nDescription FAB Materials 2: S","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: 20'' PIPE BY MT PEXPE 7000M IP\nDescription FAB Materials 2: S","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000811,"(BLCK)FAB:ASEDY-56-505121-0001-1",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0001-1\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0001-1\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000812,"(BLCK)FAB:ASEDY-56-505121-0002-2",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0002-2\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0002-2\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000813,"(BLCK)FAB:PAINTED BLD 14\"150#FF  A10,5 G",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 14\"150#FF ASTM A10\nDescription FAB Materials 2: 5 GLV","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 14\"150#FF ASTM A10\nDescription FAB Materials 2: 5 GLV","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000814,"(BLCK)FAB:ASEDY-56-505121-0003-1",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0003-1\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0003-1\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000815,"(BLCK)FAB:ASEDY-56-505121-0003-2",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0003-2\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0003-2\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000816,"(BLCK)FAB:ASEDY-56-505121-0003-3",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0003-3\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0003-3\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000817,"(BLCK)FAB:ASEDY-56-505121-0003-4",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0003-4\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0003-4\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000818,"(BLCK)FAB:ASEDY-56-505221-0001-1",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0001-1\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0001-1\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000819,"(BLCK)FAB:ASEDY-56-505221-0001-2",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0001-2\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0001-2\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000820,"(BLCK)FAB:ASEDY-56-505221-0002-1",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0002-1\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0002-1\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000821,"(BLCK)FAB:ASEDY-56-505221-0003-1",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0003-1\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0003-1\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000822,"(BLCK)FAB:ASEDY-56-505221-0003-2",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0003-2\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0003-2\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000823,"(BLCK)FAB:ASEDY-56-505221-0003-3",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0003-3\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0003-3\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000824,"(BLCK)FAB:ASEDY-56-505221-0003-4",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0003-4\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505221-0003-4\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000825,"(BLCK)FAB:ASEDY-56-500760-0001-1",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-500760-0001-1\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-500760-0001-1\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000826,"(BLCK)FAB:ASEDY-56-505121-0002-1",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0002-1\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0002-1\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000827,"(BLCK)FAB:ASEDY-56-505121-0002-3",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0002-3\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASEDY-56-505121-0002-3\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000828,"(BLCK)FAB:ASAEY-56-405128-0001-1",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ASAEY-56-405128-0001-1\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ASAEY-56-405128-0001-1\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000829,"(BLCK)FAB:EABI01-ASEAA-56-401003-0003-1",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: EABI01-ASEAA-56-401003-0003-1\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: EABI01-ASEAA-56-401003-0003-1\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000830,"(BLCK)FAB:PAINTED BLD 1\",1500# RTJ,LTCS,",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\",1500# RTJ ,LTCS\nDescription FAB Materials 2: .\nDescription FAB Materials 3:\nDescription FAB Materials 4:\nDRAWING/DOCUMENT REFERENCE-1:\nDRAWING/DOCUMENT REFERENCE-2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","06","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\",1500# RTJ ,LTCS\nDescription FAB Materials 2: .\nDescription FAB Materials 3:\nDescription FAB Materials 4:\nDRAWING/DOCUMENT REFERENCE-1:\nDRAWING/DOCUMENT REFERENCE-2:","ZGMD_FAB_NM","PD",0,0,0,37.33]
[1000831,"(BLCK)FAB:PAINTED BLD 1\",150# RF,LTCS",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\",150# RF ,LTCS\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","06","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\",150# RF ,LTCS\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,3.17]
[1000832,"FAB:PAINTED BLD 1\",300# RF,LTCS",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\",300# RF ,LTCS\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","03","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\",300# RF ,LTCS\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.27]
[1000833,"FAB:PAINTED BLD 1\",300# RF,SS",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\",300# RF , SS\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","03","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\",300# RF , SS\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,1.87]
[1000834,"FAB:PAINTED BLD 1\",600# RTJ,LTCS",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\", 600# RTJ ,LTCS\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","03","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 1\", 600# RTJ ,LTCS\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,1.97]
[1000835,"FAB:PAINTED BLD 2\",300# RF,LTCS",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\",300# RF ,LTCS\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","03","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\",300# RF ,LTCS\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,727.62]
[1000836,"FAB:PAINTED BLD 2\",300# RF,SS",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\",300# RF , SS\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","03","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\",300# RF , SS\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.68]
[1000837,"FAB:PAINTED BLD 2\",600# RTJ,LTCS",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\", 600# RTJ ,LTCS\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","03","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\", 600# RTJ ,LTCS\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,53.62]
[1000838,"FAB:PAINTED BLD 2\",600# RTJ,SS",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\", 600# RTJ , SS\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","03","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\", 600# RTJ , SS\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.68]
[1000839,"FAB:ORIF PLT,ASABI- FE-29041,9",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ORIFICE PLATE, ASABI- FE-29041\nDescription FAB Materials 2: 9","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","03","","","","FABRICATION:\nDescription FAB Materials 1: ORIFICE PLATE, ASABI- FE-29041\nDescription FAB Materials 2: 9","ZGMD_FAB_NM","PD",0,0,0,1.36]
[1000840,"(BLCK)FAB:ORIF PLT W/BOLTS,ASABB-,FE-575",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: ORIFICE PLATE W/BOLTS,  ASABB-\nDescription FAB Materials 2: FE-575006","","SURVEY/RELEASE NOTE APPROVED VER AGENCY","","06","","","","FABRICATION:\nDescription FAB Materials 1: ORIFICE PLATE W/BOLTS,  ASABB-\nDescription FAB Materials 2: FE-575006","ZGMD_FAB_NM","PD",0,0,0,0.01]
[1000841,"FAB:PAINTED BLD 2\",1500# RTJ,LTCS",null,null,"EA","FAB","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\",1500# RTJ, LTCS\nDescription FAB Materials 2:","","SURVEY/RELEASE NOTE APPROVED VER AGENCY\nQC PATH 1- FAT+DOC PRE-REVIEW+WH INSP","","03","","","","FABRICATION:\nDescription FAB Materials 1: PAINTED BLD 2\",1500# RTJ, LTCS\nDescription FAB Materials 2:","ZGMD_FAB_NM","PD",0,0,0,0.01]

{"sheet":"Liste","index":1,"n_rows":6,"n_cols":2,"rows_kept":6}
["Chercher","Remplacer par"]
["COND","CONDUCTOR"]
["SSD","SLIDING SLEEVE"]
["CTR","CENTRALISER"]
["LNR","LINER"]
["VLV","VALVE"]