{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Plan Métrés","DSu","Tableau perte et coef"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Plan Métrés","index":0,"n_rows":25,"n_cols":7,"rows_kept":25,"cut":false,"hidden":false,"merged":[[2,6,2,7],[1,2,1,5]],"flags":["formulas_cached_only"]}
[]
[null,null,"Métrés"]
[null,null,"Chantier:",null,"Projet:"]
[null,null,"Dossier:",null,"Nom:"]
[null,null,"Lot:","Gros œuvre","Date:","2010-09-05"]
[]
[null,null,"Libellés","Désignation","Unité","Quantité"]
[null,null,"01.01","TERRASSEMENT",null,null,0]
[null,null,"01.01.01","Terrassement emprise hérisson, débord de 1,00m, terre évacuées à la DP","m3",72.136,1]
[null,null,"01.01.02","Traitement termites sur l'emprise de la construction, débord de 1,00m","m²",430.02,1]
[null,null,"01.01.03","Terrassement en puits f140, niveau fond de fouille à -2,22 soit 178,71 NGF, terres évacuées à la DP","m3",65.958,1]
[null,null,"01.01.04","Fouilles en rigoles au droit des longrines et sous longrines pour fourreaux","m3",17.829,1]
[null,null,"01.01.05","Fouilles en rigoles pour canalisations EU/EV en PVC","m3",1.791,1]
[null,null,"01.01.06","Remblais au pourtour du bâtiment, terres provenant des fouilles","m3",19,1]
[{"$nulls":6},0]
[null,null,"01.02","FONDATIONS",null,null,0]
[null,null,"01.02.01","Gros béton à 250 Kg/m3 cis attentes","m3",53.592,1]
[null,null,"01.02.02","Massifs supports de charpente et LG bureaux",null,null,0]
[null,null,"01.02.02.a","Coffrage pour massifs, parement ordinaire","m²",46.08,1]
[null,null,"01.02.02.b","Béton à 350 Kg/m3 pour massifs","m3",9.216,1]
[null,null,"01.02.02.c","Aciers HA (non compris barre d'ancrage)","Kg",460.8,1]
[]
[{"$nulls":6},10]
[]
[{"$nulls":5},""]

{"sheet":"DSu","index":1,"n_rows":44,"n_cols":15,"rows_kept":44,"cut":false,"hidden":false,"merged":[[6,3,6,9],[7,3,7,9],[6,10,7,14],[8,12,9,12],[8,13,9,13],[8,5,9,5],[8,6,9,6],[8,8,9,8],[8,10,9,10],[8,11,9,11],[8,7,9,7],[8,9,9,9],[8,4,9,4],[3,3,3,8],[4,3,4,8],[4,11,4,12],[3,11,3,12],[1,2,2,14],[43,7,43,8],[8,14,9,14],[39,7,39,8],[40,7,40,8],[41,7,41,8],[42,7,42,8],[40,13,40,14],[41,13,41,14],[42,13,42,14],[43,13,43,14]],"flags":["formulas_cached_only"]}
[]
[null,null,"SOUS DETAIL DE PRIX UNITAIRE D'OUVRAGE"]
[]
[null,null,"Chtier:",{"$nulls":7},"Date:","2010-09-05"]
[null,null,"Etude:",{"$nulls":7},"Nom:"]
[]
[null,null,"Code","Désignation",{"$nulls":6},"DEBOURSES"]
["H",null,null,""]
["J",null,"Unité","Nombre","Total","U","Q","Perte","PU","Coef divers","MO","MX","ML","ST","PRST"]
["U",null,"",""]
["ml",null,"MO",null,null,"H","",null,"",null,""]
["m²",{"$nulls":5},"",null,"",null,""]
["m3",{"$nulls":5},"",null,"",null,""]
["l",{"$nulls":5},"",null,"",null,""]
["Kg",{"$nulls":5},"",null,"",null,""]
[{"$nulls":6},"",null,"",null,""]
[{"$nulls":6},"",null,"",null,""]
[{"$nulls":6},"",null,"",null,""]
[{"$nulls":6},"",null,"",null,""]
[{"$nulls":6},"",null,"",null,""]
[null,null,"MX",null,null,null,"",{"$nulls":4},""]
[{"$nulls":6},"",{"$nulls":4},""]
[{"$nulls":6},"",{"$nulls":4},""]
[{"$nulls":6},"",{"$nulls":4},""]
[{"$nulls":6},"",{"$nulls":4},""]
[{"$nulls":6},"",{"$nulls":4},""]
[{"$nulls":6},"",{"$nulls":4},""]
[{"$nulls":6},"",{"$nulls":4},""]
[{"$nulls":6},"",{"$nulls":4},""]
[null,null,"ML",null,null,null,"",{"$nulls":5},""]
[{"$nulls":6},"",{"$nulls":5},""]
[{"$nulls":6},"",{"$nulls":5},""]
[{"$nulls":6},"",{"$nulls":5},""]
[{"$nulls":6},"",{"$nulls":5},""]
[null,null,"ST",null,null,null,"",{"$nulls":6},""]
[{"$nulls":6},"",{"$nulls":6},""]
[{"$nulls":6},"",{"$nulls":6},""]
[null,null,"PRST",null,null,null,"",{"$nulls":7},""]
[{"$nulls":6},"",{"$nulls":7},""]
[{"$nulls":7},"PU",null,0,0,0,0,0,0]
[{"$nulls":7},"Déboursé sec",null,"Q","","x PU",0,""]
[{"$nulls":7},"Sous Traitant",null,"Q","","x Coût",0,""]
[{"$nulls":7},"Prestataire",null,"Q","","x Coût",0,""]
[{"$nulls":7},"Budget d'heure",null,"Q","","x TU",0,""]

{"sheet":"Tableau perte et coef","index":2,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[[1,1,1,4]],"flags":["formulas_cached_only"]}
[]
[null,"Perte et coefficient"]
[]
[null,"code","Désignation","perte","coefficient"]
[null,1,"VRD"]
[null,101,"foisonnement terre",null,1.3]
[null,102,"Perte du compactage (pour 1 passe)",0.05]
[null,103,"Perte sur granulats",0.05]
[null,104,"Perte sur PVC ( Découpe + chute)",0.15]
[null,105,"Perte sur bidim (recouvrement + perte)",0.21]
[]
[null,2,"Coffrage"]
[null,201,"Bois (découpes + chutes)",0.1]
[null,202,"Majoration courbe",null,1.6]