{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Input & Output tables"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Input & Output tables","index":0,"n_rows":54,"n_cols":11,"rows_kept":54,"cut":false,"hidden":false,"merged":[[0,0,0,4],[2,0,2,4],[12,0,12,4],[21,0,21,2],[22,0,22,2],[23,0,23,2],[17,0,17,2],[18,0,18,2],[10,0,10,2],[1,0,1,4],[19,0,19,4],[15,0,15,4],[11,0,11,4],[4,0,4,2],[5,0,5,2],[6,0,6,2],[14,0,14,2],[16,0,16,4],[9,0,9,2],[33,1,33,9],[44,1,44,9],[20,0,20,4],[13,0,13,2],[28,0,28,2],[27,0,27,4],[24,0,24,2],[25,0,25,2]],"flags":["formulas_cached_only"]}
["Car properties"]
[]
["Chassis"]
["Suspended mass",null,null,700,"Kg"]
["Wheight distribution (front)",null,null,40,"%"]
["Suspended mass - Front axle",null,null,280,"Kg",2746.8,"N"]
["Suspended mass - Rear axle",null,null,420,"Kg",4120.2,"N"]
["Non suspended mass - Front (1 wheel)",null,null,40,"Kg",392.40000000000003,"N"]
["Non suspended mass - Rear (1 wheel)",null,null,40,"Kg",392.40000000000003,"N"]
["Front ride height",null,null,35,"mm"]
["Rear ride height",null,null,35,"mm"]
[]
["Tyre stiffness"]
["Front tyre - Kt Fr",null,null,200,"N/mm",200000,"N/m"]
["Rear tyre - Kt Rr",null,null,230,"N/mm",230000,"N/m"]
[]
["Spring stiffness"]
["Front spring - Ks Fr",null,null,105,"N/mm",105000,"N/m","Suppose the force is derectly applyed on the springs with no motion ratio."]
["Rear spring - Ks Rr",null,null,125,"N/mm",125000,"N/m","Calculations are made on front and rear axle (2 wheels/axle)."]
[]
["Aero"]
["Front aera - S",null,null,2,"m²"]
["Coefficient of drag - Cd",null,null,0.5,"N/A"]
["Coefficient of Downforce - Cz",null,null,0.65,"N/A"]
["Coefficient of Sideforce - Cy",null,null,0.1,"N/A"]
["Aero balance (front)",null,null,45,"%"]
[]
["Constant"]
["Air density",null,null,1.2255,"kg/m^3"]
[]
[]
[]
[]
[null,"Coeff appui avant"]
[null,5,10,15,20,25,30,35,40,45,"Garde au sol arrière"]
[5,1.635,1.642,1.637,1.636,1.665,1.684,1.699]
[10,1.518,1.531,1.537,1.547,1.576,1.612,1.617,1.609]
[15,1.416,1.432,1.445,1.482,1.509,1.53,1.532,1.52,1.526]
[20,null,1.366,1.384,1.404,1.437,1.441,1.448,1.446,1.437]
[25,null,null,1.312,1.34,1.364,1.374,1.371,1.36,1.362]
[30,null,null,null,1.271,1.291,1.298,1.292,1.284,1.281]
[35,{"$nulls":4},1.218,1.215,1.206,1.212,1.202]
["Garde au sol avant"]
[]
[null,"Coeff appui arrière"]
[null,5,10,15,20,25,30,35,40,45,"Garde au sol arrière"]
[5,2.136,2.114,2.085,2.074,2.109,2.15,2.155]
[10,2.082,2.065,2.05,2.063,2.095,2.139,2.138,2.099]
[15,2.035,2.039,2.035,2.068,2.102,2.126,2.106,2.069,2.053]
[20,null,2.016,2.021,2.045,2.088,2.098,2.08,2.056,2.02]
[25,null,null,2.001,2.038,2.072,2.07,2.048,2.016,1.994]
[30,null,null,null,2.016,2.037,2.038,2.008,1.979,1.953]
[35,{"$nulls":4},2.003,1.986,1.953,1.94,1.906]
["Garde au sol avant"]